{"text_format":"1","workbook":"xlsx","n_sheets":7,"sheets":["Introduction","Materials overview","Glass ECC V1.1","Data","Master Data","Calculation Guardian","Calculation Pilkington"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":59,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Introduction","index":0,"n_rows":4,"n_cols":2,"rows_kept":4,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"GlassECC v1.1 – EPD Based Glass Embodied Carbon Assessment Tool \nIntroduction & Methodology\n\n1. Description\nGlassECC is an EPD-based calculation tool for estimating the embodied carbon of insulating glass units (IGUs) using product-specific Environmental Product Declarations (EPDs). It is intended for early-stage design, comparative assessment, and transparent evaluation of façade glazing systems, enabling informed decision-making based on verifiable data.\n\n2. Methodology\nThe tool operates exclusively on Environmental Product Declarations (EPDs) data in accordance with EN 15804 and ISO 14025. All embodied carbon values are derived directly from the manufacturer’s declared EPD without the use of generic datasets, industry averages, or secondary databases.\n\n3. Calculation Approach\nThe embodied carbon of an IGU is calculated by:\n•\tDefining the IGU composition based on user inputs\n•\tBreaking down the unit into constituent components (glass panes, spacer, sealants, assembly)\n•\tAssigning each component to a specific EPD dataset\n•\tConverting declared units to kgCO₂e/m² where required\nResults are presented as total embodied carbon per 1-meter square area (kgCO₂e/m²).\n\n4. Data Sources\nAll input data is sourced from published and verified Environmental Product Declarations.\nFor each component, the tool provides:\n•\tManufacturer name\n•\tProduct name\n•\tProduct type\n•\tEPD reference number\n•\tValidity period\n"]
[null,"\n5. Limitations\nResults are dependent on the availability and quality of EPD data\nNot all manufacturers, products, or system are represented\n\n6. Reference\nThis tool is based on and extends the methodology presented in:\nIstratii, M. – “A Methodology for Accurate Embodied Carbon Assessment of Insulating Glass Units using EPD Data”\nProceedings of the Challenging Glass Conference 10\nAccess paper:https://proceedings.challengingglass.com/index.php/cgc/article/view/740\n\n7. Author & Affiliation\nAuthor: Mihail Istratii\nAffiliation: GLF Façade Specialists\nTool: GlassECC v1.1\nDate: June 2026\n\n8. Instructions for Use\n•\tUse only the light blue cells to generate the data from the drop down menus provided\n•\tSelect the composition of IGU, double glazed or triple glazed\n•\tDefine the IGU configuration using dropdown menus\n•\tVerify component composition and data references\n•\tReview calculated embodied carbon results (kgCO₂e/m²)\n•\tInterpret results in the context of system boundaries and assumptions"]

{"sheet":"Materials overview","index":1,"n_rows":103,"n_cols":5,"rows_kept":103,"cut":false,"hidden":false,"merged":[[96,1,102,1],[95,3,99,3],[95,4,99,4],[66,1,75,1],[3,1,3,4],[33,1,43,1],[36,3,38,3],[33,3,35,3],[33,4,43,4],[30,1,32,1],[5,1,29,1],[44,1,65,1],[76,1,82,1],[83,1,84,1],[2,1,2,4],[85,1,86,1],[90,1,95,1],[1,1,1,4],[87,1,89,1]]}
[]
[null,"GlassECC v1.1 – EPD Based Glass Embodied Carbon Assessment Tool \n\nMaterials overview\n\nThis sheet provides an overview of glass products and manufacturers included in GlassECC v1.1.\n\n•\tIt serves as a reference for:\n•\tIdentifying which manufacturers are represented\n•\tUnderstanding the types of products considered\n•\tReviewing associated EPD references and validity periods\n\nNote: This is a reference index. Product selection for calculations is performed within the main calculator."]
[]
[null,"List of products incorporated in Glass ECC V1.1"]
[null,"Manufacturer","Product","EPD reference","Validity period"]
[null,"AGC","Planibel Clearlite Low Carbon Monolithic","20240940455-FC","2029-12-31"]
[null,null,"Planibel Clearlite Low Carbon Monolithic offline coated (including ranges: Clearsight, Energy, ipasol, iplus, Luxclear, Stopray)","20240940459-FC","2029-12-31"]
[null,null,"Planibel Clearlite Low Carbon Monolithic toughened HST ","20240940456-FC","2029-12-31"]
[null,null,"Planibel Clearlite Low Carbon Monolithic toughened HST offline coated (including ranges: Clearsight, Energy, ipasol, iplus, Luxclear, Stopray)","20240940459-FC","2029-12-31"]
[null,null,"Planibel Clearlite Low Carbon Laminated ","20240940457-FC","2029-12-31"]
[null,null,"Planibel Clearlite Low Carbon Laminated offline coated (including ranges: Clearsight, Energy, ipasol, iplus, Luxclear, Stopray)","20240940457-FC","2029-12-31"]
[null,null,"Planibel Clearlite Low Carbon Laminated toughened ","20240940457-FC","2029-12-31"]
[null,null,"Planibel Clearlite Low Carbon Laminated toughened offline coated (including ranges: Clearsight, Energy, ipasol, iplus, Luxclear, Stopray)","20240940457-FC","2029-12-31"]
[null,null,"Planibel Clearlite Monolithic (including types: Dark Grey, Green, Grey, Linea Azzurra)","20240940452-FC","2029-12-31"]
[null,null,"Planibel Clearlite Monolithic offline coated (including ranges: Clearsight, Energy, ipasol, iplus, Luxclear, Stopray)","20240940460-FC","2029-12-31"]
[null,null,"Planibel Clearlite Monolithic toughened HST (including types: Dark Grey, Green, Grey, Linea Azzurra)","20240940468-FC","2029-12-31"]
[null,null,"Planibel Clearlite Monolithic toughened HST offline coated","20240940460-FC","2029-12-31"]
[null,null,"Planibel Clearlite Laminated (including types: Dark Grey, Green, Grey, Linea Azzurra)","20240940458-FC","2029-12-31"]
[null,null,"Planibel Clearlite Laminated offline coated (including ranges: Clearsight, Energy, ipasol, iplus, Luxclear, Stopray)","20240940458-FC","2029-12-31"]
[null,null,"Planibel Clearlite Laminated toughened (including types: Dark Grey, Green, Grey, Linea Azzurra)","20240940458-FC","2029-12-31"]
[null,null,"Planibel Clearlite Laminated toughened offline coated  (including ranges: Clearsight, Energy, ipasol, iplus, Luxclear, Stopray)","20240940458-FC","2029-12-31"]
[null,null,"Planibel Clearvision Monolithic(including types: Dark Grey, Green, Grey, Linea Azzurra)","20240940452-FC","2029-12-31"]
[null,null,"Planibel Clearvision Monolithic offline coated (including ranges: Clearsight, Energy, ipasol, iplus, Luxclear, Stopray)","20240940460-FC","2029-12-31"]
[null,null,"Planibel Clearvision Monolithic toughened HST (including types: Dark Grey, Green, Grey, Linea Azzurra)","20240940468-FC","2029-12-31"]
[null,null,"Planibel Clearvision Monolithic toughened HST offline coated (including ranges: Clearsight, Energy, ipasol, iplus, Luxclear, Stopray)","20240940460-FC","2029-12-31"]
[null,null,"Planibel Clearvision Laminated (including types: Dark Grey, Green, Grey, Linea Azzurra)","20240940458-FC","2029-12-31"]
[null,null,"Planibel Clearvision Laminated offline coated (including ranges: Clearsight, Energy, ipasol, iplus, Luxclear, Stopray)","20240940458-FC","2029-12-31"]
[null,null,"Planibel Clearvision Laminated toughened (including types: Dark Grey, Green, Grey, Linea Azzurra)","20240940458-FC","2029-12-31"]
[null,null,"Planibel Clearvision Laminated toughened offline coated (including ranges: Clearsight, Energy, ipasol, iplus, Luxclear, Stopray)","20240940458-FC","2029-12-31"]
[]
[null,"Euroglass","Eurofloat Monolithic","EPD-GLS-20250386-IBC1-DE","2030-07-22"]
[null,null,"Eurolamex Laminated","EPD-GLS-20230183-IBB3-EN","2029-02-04"]
[]
[null,"Guardian","NEXA 6 Monolithic Extraclear","4791438322.105.1","2029-08-29"]
[null,null,"NEXA 6 Monolithic Extraclear coated (including ranges: Sunguard, Anti-reflective, Pure sight, ThermaGuard, Dielectric mirror)"]
[null,null,"NEXA 6 Laminated (including: Extraclear, Ultraclear, Acoustic, Coloured, Structural XT, Transwhite, UV, Bird1st)"]
[null,null,"NEXA 9 Monolithic ","4791438322.106.1"]
[null,null,"NEXA 9 Monolithic coated (including ranges: Sunguard, Anti-reflective, Pure sight, ThermaGuard, Dielectric mirror)"]
[null,null,"NEXA 9 Laminated (including: Extraclear, Ultraclear, Acoustic, Coloured, Structural XT, Transwhite, UV, Bird1st)"]
[null,null,"Monolithic Extraclear ","4791438322.102.1"]
[null,null,"Monolithic Extraclear coated (including ranges: Sunguard, Climaguard, Anti-reflective, Pure sight, ThermaGuard, Dielectric mirror)","4791438322.101.1"]
[null,null,"Monolithic Ultraclear ","4791438322.103.1"]
[null,null,"Laminated  (including: Extraclear, Ultraclear, Acoustic, Coloured, Structural XT, Transwhite, UV, Bird1st)","4791438322.104.1"]
[]
[null,"Pilkington","Mirai – Monolithic  ","S-P-11498 V2","2029-01-23"]
[null,null,"Mirai – Monolithic offline coated (including ranges: Suncool, Optitherm, K Glass)","IES-0024742","2031-01-16"]
[null,null,"Mirai – Monolithic toughened  ","IES-0024744","2031-01-16"]
[null,null,"Mirai – Monolithic toughened offline coated (including ranges: Suncool, Optitherm, K Glass)","IES-0024743","2031-01-16"]
[null,null,"Mirai – Laminated (including ranges: Optilam, Optiphon)","IES-0024746","2031-01-16"]
[null,null,"Mirai – Laminated offline coated, Optilam (including ranges: Suncool, Optitherm, K Glass S)","IES-0024745","2031-01-16"]
[null,null,"Optifloat – Monolithic  ","S-P-08816","2028-04-30"]
[null,null,"Optifloat – Monolithic offline coated (including ranges: Suncool, Optitherm, K Glass S, Mirropane)","S-P-08819","2028-04-30"]
[null,null,"Optifloat – Monolithic online coated (including ranges: Activ, K Glass, NSG TEC, Optiview, Optishower)","S-P-08821","2028-04-30"]
[null,null,"Optifloat – Monolithic toughened ","S-P-08822","2028-04-30"]
[null,null,"Optifloat – Monolithic toughened offline coated (including ranges: Suncool, Optitherm, K Glass S, Mirropane)","S-P-08824","2028-04-30"]
[null,null,"Optifloat – Monolithic toughened online coated (including ranges: Activ, K Glass, NSG TEC, Optiview, Optishower)","S-P-08823","2028-04-30"]
[null,null,"Optilam – Laminated annealed (including ranges: Optilam, Optilam OW, Optiphon, Optiphon OW)","S-P-08826","2028-04-30"]
[null,null,"Optilam – Laminated annealed offline coated (including ranges: Suncool Optilam, Optitherm, Optilam K Glass S, Mirropane Optilam)","S-P-08827","2028-04-30"]
[null,null,"Optilam – Laminated annealed online coated (including ranges: Activ, K Glass, NSG TEC, Optiview, Optishower)","S-P-08828","2028-04-30"]
[null,null,"Optilam – Laminated toughened  ","IES-0017093","2029-12-10"]
[null,null,"Optiwhite – Monolithic (Low Iron)  ","S-P-08818","2028-04-30"]
[null,null,"Optiwhite – Monolithic offline coated (Low Iron) (including ranges: Optifloat, Optiwhite)","S-P-08821","2028-04-30"]
[null,null,"Optiwhite – Monolithic toughened (Low Iron) (including ranges: Optifloat, Optiwhite)","S-P-08823","2028-04-30"]
[null,null,"Optiwhite – Monolithic toughened offline coated (Low Iron) (including ranges: Suncool, Optitherm)","S-P-08826","2028-04-30"]
[null,null,"Patterned glass","S-P-08818","2028-04-30"]
[]
[null,"Saint Gobain","ORAÉ - Low carbon clear","S-P-09498/09499/08970/09500/09501/09502/09503 ","2028-12-20"]
[null,null,"ORAÉ - Low carbon magnetron-coated","S-P-09991/09425/09945/09992","2028-12-20"]
[null,null,"ORAÉ STADIP - Low carbon laminated float","EPD-IES-0024289","2030-06-11"]
[null,null,"PLANICLEAR - Clear float glass","S-P-00882","2026-09-29"]
[null,null,"DIAMANT - Extra clear low-iron glass","S-P-00883 ","2026-09-29"]
[null,null,"PLANICLEAR and DIAMANT - Magnetron-coated glass","S-P-00926","2026-12-14"]
[null,null,"STADIP - Laminated glass","S-P-00930","2026-12-14"]
[null,null,"SECURIT - Tempered glass","S-P-00927","2026-12-14"]
[null,null,"PARSOL -  Body tinted glass","S-P-00884","2026-09-29"]
[]
[null,"Fire rated glass","AGC Pyrobel T","EPD-AGC-20240539-IBH1-EN","2030-06-24"]
[null,null,"POLFLAM","Date of issue  28/11/2024","2029-11-28"]
[null,null,"Saint Gobain Vetrotech Contraflam 30 (5/5)","S-P-09642","2028-06-22"]
[null,null,"Saint Gobain Vetrotech Contraflam lite 30 CFL30 (5/5)","EPD-IES-0024348","2030-06-12"]
[null,null,"Saint Gobain Vetrotech Contraflam structure 30 STADIP CFS 30 (6/5/55.2)","EPD-IES-0024372","2030-06-15"]
[null,null,"Saint Gobain Vetrotech Contraflam structure 60 STADIP CFS 60  (6/5/5/55.2)","EPD-IES-0024375","2030-06-15"]
[]
[null,"Structural glass","Laminated toughened glass with Ionoplast film Kuraray Sentry glass"," EPD-KUR-20230073-CBA2-EN + 20240940468-FC","2029-03-11"]
[]
[null,"Painted/frit glass","Stronglasas","S-P-10601","2028-09-08"]
[]
[null,"Primary sealant","Fenzi - Butylver","EPD-IES-13054:001","2029-07-25"]
[null,null,"Butyle - Generic","EPD-FEI-20250068-IBP1-EN","2030-06-03"]
[]
[null,"Secondary sealant","Silicone - Dow corning 3362 - 3363","EPD-DBC-20220179-IBF1-EN","2027-08-30"]
[null,null,"Silicone - SIKA IG-25 HM","EPD-DBC-20220179-IBF1-EN","2027-08-30"]
[null,null,"Silicone generic","EPD-DBC-20220180-IBF1-EN","2027-08-30"]
[null,null,"Polysulphide - Fenzi Thiover","EPD-IES-13059:001","2029-07-25"]
[null,null,"Polysulphide - Generic","EPD-FEI-20250067-IBP1-EN","2030-06-03"]
[null,null,null,"S-P-08910","2028-03-23"]
[null,"Spacer bar","ALUPRO Aluminium H65 A155"]
[null,null,"ALUPRO Chromatech Ultra F"]
[null,null,"ALUPRO Multitech G"]
[null,null,"ALUPRO Thermix TX Pro"]
[null,null,"Swisspacer Advance","EPD-IES-0011836:001","2029-12-15"]
[null,null,"Swisspacer Ultimate","EPD-IES-0011837:001","2029-12-15"]
[null,null,"Technoform warm edge SP14","S-P-10425","2028-12-11"]

{"sheet":"Glass ECC V1.1","index":2,"n_rows":19,"n_cols":23,"rows_kept":19,"cut":false,"hidden":false,"merged":[[7,1,8,1],[7,3,8,3],[7,22,8,22],[18,1,18,4],[16,3,16,5],[17,1,17,5],[7,6,7,20],[7,5,8,5],[7,4,8,4],[2,2,2,21],[7,21,8,21],[3,2,3,3],[5,2,5,3],[4,2,4,3],[7,2,8,2],[6,2,6,3]]}
[]
[]
[null,"\n","EPD - Based Glass Embodied Carbon Assessment Tool"]
[null,"IGU Reference","Type 1"]
[null,"Composition","8/16/44.4"]
[null,"Size (H x W) m","1.0 x 1.0"]
[null,"Type","Double Glazed"]
[null,"Item","ECF symbol","Manufacturer","Product","Type","GWP LCA stages (kg CO2eq/m2)",null,null,null,null,null,null,null,null,null,null,null,null,null,null,"EPD reference","EPD valid to"]
[null,null,null,null,null,null,"A1-A3","A4","A5","B1","B2","B3","B4","B5","B6","B7","C1","C2","C3","C4","D"]
[null,"Glass outer pane","ECFOP","None","None","None",{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(G$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(H$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(I$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(J$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(K$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(L$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(M$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(N$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(O$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(P$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(Q$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(R$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(S$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(T$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(U$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(V$8,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D10=Table4[Manufacturer])*(E10=Table4[Product])*(F10=Table4[Type]),0),MATCH(W$8,Table4[#Headers],0)),\"\")","v":"00:00:00"}]
[null,"Spacer bar","ECFSB","None","None","None",{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(G$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(H$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(I$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(J$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(K$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(L$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(M$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(N$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(O$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(P$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(Q$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(R$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(S$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(T$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(U$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(V$8,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D11=Table4[Manufacturer])*(E11=Table4[Product])*(F11=Table4[Type]),0),MATCH(W$8,Table4[#Headers],0)),\"\")","v":"00:00:00"}]
[null,"Glass mid pane","ECFMID","Painted frit glass","Stronglasas","Monolithic toughened 6 mm",{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(G$9,Table4[#Headers],0)),\"\")","v":17.82},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(H$9,Table4[#Headers],0)),\"\")","v":7.7249999999999999E-2},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(I$9,Table4[#Headers],0)),\"\")","v":0.14850000000000002},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(J$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(K$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(L$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(M$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(N$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(O$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(P$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(Q$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(R$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(S$9,Table4[#Headers],0)),\"\")","v":1.26E-2},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(T$9,Table4[#Headers],0)),\"\")","v":1.3599999999999999E-2},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(U$9,Table4[#Headers],0)),\"\")","v":-4.8000000000000007},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(V$8,Table4[#Headers],0)),\"\")","v":"S-P-10601"},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D12=Table4[Manufacturer])*(E12=Table4[Product])*(F12=Table4[Type]),0),MATCH(W$8,Table4[#Headers],0)),\"\")","v":"2028-09-08"}]
[null,"Spacer bar","ECFSB","None","None","None",{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(G$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(H$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(I$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(J$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(K$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(L$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(M$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(N$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(O$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(P$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(Q$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(R$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(S$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(T$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(U$9,Table4[#Headers],0)),\"\")*4","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(V$8,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D13=Table4[Manufacturer])*(E13=Table4[Product])*(F13=Table4[Type]),0),MATCH(W$8,Table4[#Headers],0)),\"\")","v":"00:00:00"}]
[null,"Glass inner pane","ECFIP","None","None","None",{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(G$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(H$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(I$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(J$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(K$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(L$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(M$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(N$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(O$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(P$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(Q$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(R$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(S$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(T$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(U$9,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(V$8,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D14=Table4[Manufacturer])*(E14=Table4[Product])*(F14=Table4[Type]),0),MATCH(W$8,Table4[#Headers],0)),\"\")","v":"00:00:00"}]
[null,"Primary sealant","ECFPS","None","None","None",{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(G$9,Table4[#Headers],0)),\"\")*0.1","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(H$9,Table4[#Headers],0)),\"\")*0.1","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(I$9,Table4[#Headers],0)),\"\")*0.1","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(J$9,Table4[#Headers],0)),\"\")*0.1","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(K$9,Table4[#Headers],0)),\"\")*0.1","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(L$9,Table4[#Headers],0)),\"\")*0.1","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(M$9,Table4[#Headers],0)),\"\")*0.1","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(N$9,Table4[#Headers],0)),\"\")*0.1","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(O$9,Table4[#Headers],0)),\"\")*0.1","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(P$9,Table4[#Headers],0)),\"\")*0.1","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(Q$9,Table4[#Headers],0)),\"\")*0.1","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(R$9,Table4[#Headers],0)),\"\")*0.1","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(S$9,Table4[#Headers],0)),\"\")*0.1","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(T$9,Table4[#Headers],0)),\"\")*0.1","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(U$9,Table4[#Headers],0)),\"\")*0.1","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(V$8,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D15=Table4[Manufacturer])*(E15=Table4[Product])*(F15=Table4[Type]),0),MATCH(W$8,Table4[#Headers],0)),\"\")","v":"00:00:00"}]
[null,"Secondary sealant","ECFSS","None","None","None",{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(G$9,Table4[#Headers],0)),\"\")*0.6","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(H$9,Table4[#Headers],0)),\"\")*0.6","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(I$9,Table4[#Headers],0)),\"\")*0.6","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(J$9,Table4[#Headers],0)),\"\")*0.6","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(K$9,Table4[#Headers],0)),\"\")*0.6","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(L$9,Table4[#Headers],0)),\"\")*0.6","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(M$9,Table4[#Headers],0)),\"\")*0.6","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(N$9,Table4[#Headers],0)),\"\")*0.6","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(O$9,Table4[#Headers],0)),\"\")*0.6","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(P$9,Table4[#Headers],0)),\"\")*0.6","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(Q$9,Table4[#Headers],0)),\"\")*0.6","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(R$9,Table4[#Headers],0)),\"\")*0.6","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(S$9,Table4[#Headers],0)),\"\")*0.6","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(T$9,Table4[#Headers],0)),\"\")*0.6","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(U$9,Table4[#Headers],0)),\"\")*0.6","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(V$8,Table4[#Headers],0)),\"\")","v":0},{"$f":"IFERROR(INDEX(Table4[],MATCH(1,(D16=Table4[Manufacturer])*(E16=Table4[Product])*(F16=Table4[Type]),0),MATCH(W$8,Table4[#Headers],0)),\"\")","v":"00:00:00"}]
[null,"IGU assembly process","ECFPROC",null,null,null,{"$f":"_xlfn.IFS(C7=\"Double glazed\",10,C7=\"Triple glazed\",15,TRUE,0)","v":10}]
[null,"Toatal IGU Embodied Carbon per m2  (ECIGU - kgCO2/m2)",null,null,null,null,{"$f":"SUBTOTAL(109,G10:G17)","v":10},0,0,0,0,0,0,0,0,0,0,0,0,0,0]
[null,"This tool has been developed in conjunction with research presented at the Challenging Glass Cconference 10\nAuthor: Mihail Istratii  \nAffiliation: GLF Façade Specialists",null,null,null," Access paper"]

{"sheet":"Data","index":3,"n_rows":44,"n_cols":10,"rows_kept":44,"cut":false,"hidden":true,"merged":[]}
[]
["AGC","Euroglass","Guardian Glass","Pilkington/NSG","Saint-Gobain","Guardian","Fire rated glass","Spacer bar","Primary sealant","Secondary sealant"]
["Stratobel","Eurofloat","NEXA 6 monolithic","Mirai","ORAE (Low carbon)",null,"POLFLAM","ALU PRO Aluminium spacer H65","Fenzi - Butylver","Silicone - Dow corning 3362 - 3363"]
["Planibel","Eurolamex","NEXA 6 monolithic coated","Optifloat","PLANICLEAR",null,"AGC Pyrobel-T","ALU PRO Chromatech ultra F","Butyle - Generic","Silicone - SIKA IG-25 HM"]
["Planiclear",null,"NEXA 6 laminated",null,"DIAMANT",null,"Pilkington Pyrostop","ALU PRO Chromatech multitech G",null,"Polysulphide - Fenzi Thiover"]
[null,null,"NEXA 9 monolithic",null,"STADIP",null,"Vetrotech","ALU PRO Thermic TX Pro",null,"Polysulphide - Generic"]
[null,null,"NEXA 9 monolithic coated",null,"PARSOL"]
[null,null,"NEXA 9 laminated"]
[null,null,"Extraclear float"]
[null,null,"Ultraclear float"]
[null,null,"Extraclear coated float"]
[null,null,"Extraclear laminated"]
[]
[]
[]
[]
["Manufacturer","Product"]
["AGC","Stratobel"]
[null,"Planibel"]
[null,"Planiclear"]
["Euroglass","Eurofloat"]
[null,"Eurolamex"]
["Guardian Glass","NEXA 6 monolithic"]
[null,"NEXA 6 monolithic coated"]
[null,"NEXA 6 laminated"]
[null,"NEXA 9 monolithic"]
[null,"NEXA 9 monolithic coated"]
[null,"NEXA 9 laminated"]
[null,"Extraclear float"]
[null,"Ultraclear float"]
[null,"Extraclear coated float"]
[null,"Extraclear laminated"]
["Pilkington NSG","Mirai"]
[null,"Optifloat"]
["Saint Gobain","ORAE Low carbon"]
[null,"PLANICLEAR SG"]
[null,"DIAMANT"]
[null,"STADIP"]
[null,"PARSOL"]
["Guardian"]
["Fire rated glass","POLFLAM"]
[null,"AGC Pyrobel T"]
[null,"Pilkington Pyrostop"]
[null,"Vetrotech"]

{"sheet":"Master Data","index":4,"n_rows":631,"n_cols":24,"rows_kept":631,"cut":false,"hidden":true,"merged":[]}
["Item","Column1","Manufacturer","Product","Type","A1-A3","A4","A5","B1","B2","B3","B4","B5","B6","B7","C1","C2","C3","C4","D","EPD Reference","EPD Valid to"]
[]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic 3 mm",4.0999999999999996,0.27,0,0,0.11600000000000001,0,0,0,0,0,0,2.52E-2,0,0.123,0,"20240940455-FC","2029-12-31",null,3]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic 4 mm",5.5,{"$f":"($G$3/3)*X4","v":0.36000000000000004},0,0,{"$f":"($J$3/3)*X4","v":0.15466666666666667},0,0,0,0,0,0,{"$f":"($Q$3/3)*X4","v":3.3599999999999998E-2},0,{"$f":"($S$3/3)*X4","v":0.16400000000000001},0,"20240940455-FC","2029-12-31",null,4]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic 5 mm",6.9,{"$f":"($G$3/3)*X5","v":0.45000000000000007},0,0,{"$f":"($J$3/3)*X5","v":0.19333333333333336},0,0,0,0,0,0,{"$f":"($Q$3/3)*X5","v":4.1999999999999996E-2},0,{"$f":"($S$3/3)*X5","v":0.20500000000000002},0,"20240940455-FC","2029-12-31",null,5]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic 6 mm",8.3000000000000007,0.54,0,0,0.23200000000000001,0,0,0,0,0,0,5.04E-2,0,0.246,0,"20240940455-FC","2029-12-31",null,6]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic 8 mm",11,0.72000000000000008,0,0,0.30933333333333335,0,0,0,0,0,0,6.7199999999999996E-2,0,0.32800000000000001,0,"20240940455-FC","2029-12-31",null,8]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic offline coated 3 mm",4.5999999999999996,0.247,0,0,0.11600000000000001,0,0,0,0,0,0,2.52E-2,0,0.123,0,"20240940459-FC","2029-12-31",null,3]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic offline coated 4 mm",6.1,{"$f":"($G$8/3)*X9","v":0.32933333333333331},0,0,0.15466666666666667,0,0,0,0,0,0,3.3599999999999998E-2,0,0.16400000000000001,0,"20240940459-FC","2029-12-31",null,4]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic offline coated 5 mm",7.6,{"$f":"($G$8/3)*X10","v":0.41166666666666663},0,0,0.19333333333333336,0,0,0,0,0,0,4.1999999999999996E-2,0,0.20500000000000002,0,"20240940459-FC","2029-12-31",null,5]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic offline coated 6 mm",9.1,0.49399999999999999,0,0,0.23200000000000001,0,0,0,0,0,0,5.04E-2,0,0.246,0,"20240940459-FC","2029-12-31",null,6]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic offline coated 8 mm",12,0.65866666666666662,0,0,0.30933333333333335,0,0,0,0,0,0,6.7199999999999996E-2,0,0.32800000000000001,0,"20240940459-FC","2029-12-31",null,8]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic toughened HST 3 mm",5.0999999999999996,0.64700000000000002,0,0,0.11600000000000001,0,0,0,0,0,0,2.52E-2,0,0.123,0,"20240940456-FC","2029-12-31",null,3]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic toughened HST 4 mm",6.7,{"$f":"($G$13/3)*X14","v":0.86266666666666669},0,0,0.15466666666666667,0,0,0,0,0,0,3.3599999999999998E-2,0,0.16400000000000001,0,"20240940456-FC","2029-12-31",null,4]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic toughened HST 5 mm",8.3000000000000007,{"$f":"($G$13/3)*X15","v":1.0783333333333334},0,0,0.19333333333333336,0,0,0,0,0,0,4.1999999999999996E-2,0,0.20500000000000002,0,"20240940456-FC","2029-12-31",null,5]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic toughened HST 6 mm",9.9,1.294,0,0,0.23200000000000001,0,0,0,0,0,0,5.04E-2,0,0.246,0,"20240940456-FC","2029-12-31",null,6]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic toughened HST 8 mm",13.1,1.7253333333333334,0,0,0.30933333333333335,0,0,0,0,0,0,6.7199999999999996E-2,0,0.32800000000000001,0,"20240940456-FC","2029-12-31",null,8]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic toughened HST offline coated 3 mm",5.3,0.65700000000000003,0,0,0.11600000000000001,0,0,0,0,0,0,2.52E-2,0,0.123,0,"20240940459-FC","2029-12-31",null,3]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic toughened HST offline coated 4 mm",7,{"$f":"($G$18/3)*X19","v":0.876},0,0,0.15466666666666667,0,0,0,0,0,0,3.3599999999999998E-2,0,0.16400000000000001,0,"20240940459-FC","2029-12-31",null,4]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic toughened HST offline coated 5 mm",8.6999999999999993,{"$f":"($G$18/3)*X20","v":1.095},0,0,0.19333333333333336,0,0,0,0,0,0,4.1999999999999996E-2,0,0.20500000000000002,0,"20240940459-FC","2029-12-31",null,5]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic toughened HST offline coated 6 mm",10.4,1.3140000000000001,0,0,0.23200000000000001,0,0,0,0,0,0,5.04E-2,0,0.246,0,"20240940459-FC","2029-12-31",null,6]
[null,null,"AGC","Planibel Clearlite Low Carbon","Monolithic toughened HST offline coated 8 mm",13.8,1.752,0,0,0.30933333333333335,0,0,0,0,0,0,6.7199999999999996E-2,0,0.32800000000000001,0,"20240940459-FC","2029-12-31",null,8]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated 6.4 (33.1)",10.6,0.56399999999999995,0,0,0.11600000000000001,0,0,0,0,0,0,5.1700000000000003E-2,0,0.251,0,"20240940457-FC","2029-12-31",null,6.4]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated 6.8 (33.2)",12.7,{"$f":"($G$23/$X$23)*X24","v":0.59924999999999984},0,0,{"$f":"($J$23/$X$23)*X24","v":0.12324999999999998},0,0,0,0,0,0,{"$f":"($Q$23/$X$23)*X24","v":5.4931250000000001E-2},0,{"$f":"($S$23/$X$23)*X24","v":0.26668749999999997},0,"20240940457-FC","2029-12-31",null,6.8]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated 8.4 (44.1)",13.4,0.74024999999999985,0,0,0.15225,0,0,0,0,0,0,6.7856250000000007E-2,0,0.32943749999999999,0,"20240940457-FC","2029-12-31",null,8.4]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated 8.8 (44.2)",15.5,0.77549999999999986,0,0,0.1595,0,0,0,0,0,0,7.1087500000000012E-2,0,0.34512500000000002,0,"20240940457-FC","2029-12-31",null,8.8000000000000007]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated 10.4 (55.1)",16.2,0.91649999999999987,0,0,0.1885,0,0,0,0,0,0,8.4012500000000004E-2,0,0.40787499999999999,0,"20240940457-FC","2029-12-31",null,10.4]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated 10.8 (55.2)",18.3,0.95174999999999987,0,0,0.19575000000000001,0,0,0,0,0,0,8.7243750000000009E-2,0,0.42356250000000001,0,"20240940457-FC","2029-12-31",null,10.8]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated 11.5 (55.4)",22.5,1.0134374999999998,0,0,0.2084375,0,0,0,0,0,0,9.28984375E-2,0,0.45101562499999998,0,"20240940457-FC","2029-12-31",null,11.5]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated 12.4 (66.1)",19.100000000000001,1.0927499999999999,0,0,0.22474999999999998,0,0,0,0,0,0,0.10016875,0,0.48631249999999998,0,"20240940457-FC","2029-12-31",null,12.4]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated 12.8 (66.2)",21.2,1.1279999999999999,0,0,0.23199999999999998,0,0,0,0,0,0,0.10340000000000001,0,0.502,0,"20240940457-FC","2029-12-31",null,12.8]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated 13.5 (66.4)",25.4,1.1896874999999998,0,0,0.24468749999999997,0,0,0,0,0,0,0.1090546875,0,0.52945312499999997,0,"20240940457-FC","2029-12-31",null,13.5]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated 16.4 (88.1)",24.7,1.4452499999999995,0,0,0.29724999999999996,0,0,0,0,0,0,0.13248124999999999,0,0.64318749999999991,0,"20240940457-FC","2029-12-31",null,16.399999999999999]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated 16.8 (88.2)",26.8,1.4804999999999997,0,0,0.30449999999999999,0,0,0,0,0,0,0.13571250000000001,0,0.65887499999999999,0,"20240940457-FC","2029-12-31",null,16.8]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated 17.5 (88.4)",31,1.5421874999999996,0,0,0.31718749999999996,0,0,0,0,0,0,0.14136718749999999,0,0.68632812499999996,0,"20240940457-FC","2029-12-31",null,17.5]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated offline coated 6.4 (33.1)",11.5,0.56399999999999995,0,0,0.11600000000000001,0,0,0,0,0,0,5.1700000000000003E-2,0,0.251,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated offline coated 6.8 (33.2)",13.8,0.59924999999999984,0,0,0.12324999999999998,0,0,0,0,0,0,5.4931250000000001E-2,0,0.26668749999999997,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated offline coated  8.4 (44.1)",14.6,0.74024999999999985,0,0,0.15225,0,0,0,0,0,0,6.7856250000000007E-2,0,0.32943749999999999,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated offline coated 8.8 (44.2)",16.8,0.77549999999999986,0,0,0.1595,0,0,0,0,0,0,7.1087500000000012E-2,0,0.34512500000000002,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated offline coated 10.4 (55.1)",17.600000000000001,0.91649999999999987,0,0,0.1885,0,0,0,0,0,0,8.4012500000000004E-2,0,0.40787499999999999,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated offline coated 10.8 (55.2)",19.8,0.95174999999999987,0,0,0.19575000000000001,0,0,0,0,0,0,8.7243750000000009E-2,0,0.42356250000000001,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated offline coated 11.5 (55.4)",24.3,1.0134374999999998,0,0,0.2084375,0,0,0,0,0,0,9.28984375E-2,0,0.45101562499999998,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated offline coated 12.4 (66.1)",20.6,1.0927499999999999,0,0,0.22474999999999998,0,0,0,0,0,0,0.10016875,0,0.48631249999999998,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated offline coated 12.8 (66.2)",22.9,1.1279999999999999,0,0,0.23199999999999998,0,0,0,0,0,0,0.10340000000000001,0,0.502,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated offline coated 13.5 (66.4)",27.3,1.1896874999999998,0,0,0.24468749999999997,0,0,0,0,0,0,0.1090546875,0,0.52945312499999997,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated offline coated 16.4 (88.1)",26.7,1.4452499999999995,0,0,0.29724999999999996,0,0,0,0,0,0,0.13248124999999999,0,0.64318749999999991,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated offline coated 16.8 (88.2)",28.9,1.4804999999999997,0,0,0.30449999999999999,0,0,0,0,0,0,0.13571250000000001,0,0.65887499999999999,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated offline coated 17.5 (88.4)",33.4,1.5421874999999996,0,0,0.31718749999999996,0,0,0,0,0,0,0.14136718749999999,0,0.68632812499999996,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated toughened 9.5 (44.4)",21.9,1.72,0,0,0.11600000000000001,0,0,0,0,0,0,7.2499999999999995E-2,0,0.376,0,"20240940457-FC","2029-12-31",null,9.5]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated toughened 11.5 (55.4)",25.2,{"$f":"($G$49/$X$49)*X50","v":2.0821052631578945},0,0,{"$f":"($J$49/$X$49)*X50","v":0.14042105263157895},0,0,0,0,0,0,{"$f":"($Q$49/$X$49)*X50","v":8.7763157894736835E-2},0,{"$f":"($S$49/$X$49)*X50","v":0.45515789473684209},0,"20240940457-FC","2029-12-31",null,11.5]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated toughened 13.5 (66.4)",28.5,{"$f":"($G$49/$X$49)*X51","v":2.4442105263157892},0,0,{"$f":"($J$49/$X$49)*X51","v":0.1648421052631579},0,0,0,0,0,0,{"$f":"($Q$49/$X$49)*X51","v":0.10302631578947367},0,{"$f":"($S$49/$X$49)*X51","v":0.53431578947368419},0,"20240940457-FC","2029-12-31",null,13.5]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated toughened 17.5 (88.4)",35,{"$f":"($G$49/$X$49)*X52","v":3.1684210526315786},0,0,{"$f":"($J$49/$X$49)*X52","v":0.21368421052631578},0,0,0,0,0,0,{"$f":"($Q$49/$X$49)*X52","v":0.13355263157894737},0,{"$f":"($S$49/$X$49)*X52","v":0.69263157894736849},0,"20240940457-FC","2029-12-31",null,17.5]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated toughened offline coated 9.5 (44.4)",23.4,1.72,0,0,0.11600000000000001,0,0,0,0,0,0,7.2499999999999995E-2,0,0.376,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated toughened offline coated 11.5 (55.4)",26.9,2.0821052631578945,0,0,0.14042105263157895,0,0,0,0,0,0,8.7763157894736835E-2,0,0.45515789473684209,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated toughened offline coated 13.5 (66.4)",30.4,2.4442105263157892,0,0,0.1648421052631579,0,0,0,0,0,0,0.10302631578947367,0,0.53431578947368419,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite Low Carbon","Laminated toughened offline coated 17.5 (88.4)",37.4,3.1684210526315786,0,0,0.21368421052631578,0,0,0,0,0,0,0.13355263157894737,0,0.69263157894736849,0,"20240940457-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite","Monolithic 3 mm",8,0.27,0,0,0.11600000000000001,0,0,0,0,0,0,2.52E-2,0,0.123,0,"20240940452-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic 4 mm",10.6,0.36000000000000004,0,0,0.15466666666666667,0,0,0,0,0,0,3.3599999999999998E-2,0,0.16400000000000001,0,"20240940452-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic 5 mm",13.3,0.45000000000000007,0,0,0.19333333333333336,0,0,0,0,0,0,4.1999999999999996E-2,0,0.20500000000000002,0,"20240940452-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic 6 mm",16,0.54,0,0,0.23200000000000001,0,0,0,0,0,0,5.04E-2,0,0.246,0,"20240940452-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic 8 mm",21.3,0.72000000000000008,0,0,0.30933333333333335,0,0,0,0,0,0,6.7199999999999996E-2,0,0.32800000000000001,0,"20240940452-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic 10 mm",26.6,0.81,0,0,0.36,0,0,0,0,0,0,7.8E-2,0,0.39200000000000002,0,"20240940452-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic 12 mm",31.9,0.9,0,0,0.41099999999999998,0,0,0,0,0,0,8.8999999999999996E-2,0,4.6600000000000003E-2,0,"20240940452-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic offline coated 3 mm",9.9,0.247,0,0,0.11600000000000001,0,0,0,0,0,0,2.52E-2,0,0.123,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic offline coated 4 mm",12.7,0.32933333333333331,0,0,0.15466666666666667,0,0,0,0,0,0,3.3599999999999998E-2,0,0.16400000000000001,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic offline coated 5 mm",15.5,0.41166666666666663,0,0,0.19333333333333336,0,0,0,0,0,0,4.1999999999999996E-2,0,0.20500000000000002,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic offline coated 6 mm",18.3,0.49399999999999999,0,0,0.23200000000000001,0,0,0,0,0,0,5.04E-2,0,0.246,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic offline coated 8 mm",23.9,0.65866666666666662,0,0,0.30933333333333335,0,0,0,0,0,0,6.7199999999999996E-2,0,0.32800000000000001,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic offline coated 10 mm",29.4,0.74099999999999999,0,0,0.36,0,0,0,0,0,0,7.8E-2,0,0.39200000000000002,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic offline coated 12 mm",35,0.82299999999999995,0,0,0.41099999999999998,0,0,0,0,0,0,8.8999999999999996E-2,0,4.6600000000000003E-2,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic toughened HST 3 mm",11.4,0.64700000000000002,0,0,0.11600000000000001,0,0,0,0,0,0,2.52E-2,0,0.123,0,"20240940468-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic toughened HST 4 mm",15.1,0.86266666666666669,0,0,0.15466666666666667,0,0,0,0,0,0,3.3599999999999998E-2,0,0.16400000000000001,0,"20240940468-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic toughened HST 5 mm",18.8,1.0783333333333334,0,0,0.19333333333333336,0,0,0,0,0,0,4.1999999999999996E-2,0,0.20500000000000002,0,"20240940468-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic toughened HST 6 mm",22.5,1.294,0,0,0.23200000000000001,0,0,0,0,0,0,5.04E-2,0,0.246,0,"20240940468-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic toughened HST 8 mm",29.9,1.7253333333333334,0,0,0.30933333333333335,0,0,0,0,0,0,6.7199999999999996E-2,0,0.32800000000000001,0,"20240940468-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic toughened HST 10 mm",37.299999999999997,1.9350000000000001,0,0,0.30933333333333335,0,0,0,0,0,0,5.04E-2,0,0.246,0,"20240940468-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic toughened HST 12 mm",44.7,2.109,0,0,0.36,0,0,0,0,0,0,6.7199999999999996E-2,0,0.32800000000000001,0,"20240940468-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic toughened HST offline coated 3 mm",13.1,0.65700000000000003,0,0,0.11600000000000001,0,0,0,0,0,0,2.52E-2,0,0.123,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic toughened HST offline coated 4 mm",16.899999999999999,0.876,0,0,0.15466666666666667,0,0,0,0,0,0,3.3599999999999998E-2,0,0.16400000000000001,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic toughened HST offline coated 5 mm",20.8,1.095,0,0,0.19333333333333336,0,0,0,0,0,0,4.1999999999999996E-2,0,0.20500000000000002,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic toughened HST offline coated 6 mm",24.6,1.3140000000000001,0,0,0.23200000000000001,0,0,0,0,0,0,5.04E-2,0,0.246,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic toughened HST offline coated 8 mm",32.299999999999997,1.752,0,0,0.30933333333333335,0,0,0,0,0,0,6.7199999999999996E-2,0,0.32800000000000001,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic toughened HST offline coated 10 mm",40,1.9350000000000001,0,0,0.30933333333333335,0,0,0,0,0,0,5.04E-2,0,0.246,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearlite ","Monolithic toughened HST offline coated 12 mm",47.7,2.109,0,0,0.36,0,0,0,0,0,0,6.7199999999999996E-2,0,0.32800000000000001,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated 6.4 (33.1)",18.8,0.56399999999999995,0,0,0.11600000000000001,0,0,0,0,0,0,5.1700000000000003E-2,0,0.251,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated 6.8 (33.2)",20.9,0.59924999999999984,0,0,0.12324999999999998,0,0,0,0,0,0,5.4931250000000001E-2,0,0.26668749999999997,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated 8.4 (44.1)",24.4,0.74024999999999985,0,0,0.15225,0,0,0,0,0,0,6.7856250000000007E-2,0,0.32943749999999999,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated 8.8 (44.2)",26.5,0.77549999999999986,0,0,0.1595,0,0,0,0,0,0,7.1087500000000012E-2,0,0.34512500000000002,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated 10.4 (55.1)",29.9,0.91649999999999987,0,0,0.1885,0,0,0,0,0,0,8.4012500000000004E-2,0,0.40787499999999999,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated 10.8 (55.2)",32,0.95174999999999987,0,0,0.19575000000000001,0,0,0,0,0,0,8.7243750000000009E-2,0,0.42356250000000001,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated 11.5 (55.4)",36.299999999999997,1.0134374999999998,0,0,0.2084375,0,0,0,0,0,0,9.28984375E-2,0,0.45101562499999998,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated 12.4 (66.1)",35.5,1.0927499999999999,0,0,0.22474999999999998,0,0,0,0,0,0,0.10016875,0,0.48631249999999998,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated 12.8 (66.2)",37.6,1.1279999999999999,0,0,0.23199999999999998,0,0,0,0,0,0,0.10340000000000001,0,0.502,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated 13.5 (66.4)",41.8,1.1896874999999998,0,0,0.24468749999999997,0,0,0,0,0,0,0.1090546875,0,0.52945312499999997,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated 16.4 (88.1)",46.6,1.4452499999999995,0,0,0.29724999999999996,0,0,0,0,0,0,0.13248124999999999,0,0.64318749999999991,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated 16.8 (88.2)",48.7,1.4804999999999997,0,0,0.30449999999999999,0,0,0,0,0,0,0.13571250000000001,0,0.65887499999999999,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated 17.5 (88.4)",52.9,1.5421874999999996,0,0,0.31718749999999996,0,0,0,0,0,0,0.14136718749999999,0,0.68632812499999996,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated offline coated 6.4 (33.1)",21.2,0.56399999999999995,0,0,0.11600000000000001,0,0,0,0,0,0,5.1700000000000003E-2,0,0.251,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated offline coated 6.8 (33.2)",23.4,0.59924999999999984,0,0,0.12324999999999998,0,0,0,0,0,0,5.4931250000000001E-2,0,0.26668749999999997,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated offline coated  8.4 (44.1)",27,0.74024999999999985,0,0,0.15225,0,0,0,0,0,0,6.7856250000000007E-2,0,0.32943749999999999,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated offline coated 8.8 (44.2)",29.3,0.77549999999999986,0,0,0.1595,0,0,0,0,0,0,7.1087500000000012E-2,0,0.34512500000000002,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated offline coated 10.4 (55.1)",32.9,0.91649999999999987,0,0,0.1885,0,0,0,0,0,0,8.4012500000000004E-2,0,0.40787499999999999,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated offline coated 10.8 (55.2)",35.1,0.95174999999999987,0,0,0.19575000000000001,0,0,0,0,0,0,8.7243750000000009E-2,0,0.42356250000000001,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated offline coated 11.5 (55.4)",39.5,1.0134374999999998,0,0,0.2084375,0,0,0,0,0,0,9.28984375E-2,0,0.45101562499999998,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated offline coated 12.4 (66.1)",38.700000000000003,1.0927499999999999,0,0,0.22474999999999998,0,0,0,0,0,0,0.10016875,0,0.48631249999999998,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated offline coated 12.8 (66.2)",40.9,1.1279999999999999,0,0,0.23199999999999998,0,0,0,0,0,0,0.10340000000000001,0,0.502,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated offline coated 13.5 (66.4)",45.4,1.1896874999999998,0,0,0.24468749999999997,0,0,0,0,0,0,0.1090546875,0,0.52945312499999997,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated offline coated 16.4 (88.1)",50.4,1.4452499999999995,0,0,0.29724999999999996,0,0,0,0,0,0,0.13248124999999999,0,0.64318749999999991,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated offline coated 16.8 (88.2)",52.6,1.4804999999999997,0,0,0.30449999999999999,0,0,0,0,0,0,0.13571250000000001,0,0.65887499999999999,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated offline coated 17.5 (88.4)",57,1.5421874999999996,0,0,0.31718749999999996,0,0,0,0,0,0,0.14136718749999999,0,0.68632812499999996,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated toughened 9.5 (44.4)",39.6,1.72,0,0,0.11600000000000001,0,0,0,0,0,0,7.2499999999999995E-2,0,0.376,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated toughened 11.5 (55.4)",47.3,2.0821052631578945,0,0,0.14042105263157895,0,0,0,0,0,0,8.7763157894736835E-2,0,0.45515789473684209,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated toughened 13.5 (66.4)",54.9,2.4442105263157892,0,0,0.1648421052631579,0,0,0,0,0,0,0.10302631578947367,0,0.53431578947368419,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated toughened 17.5 (88.4)",70.3,3.1684210526315786,0,0,0.21368421052631578,0,0,0,0,0,0,0.13355263157894737,0,0.69263157894736849,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated toughened offline coated 9.5 (44.4)",42.6,1.72,0,0,0.11600000000000001,0,0,0,0,0,0,7.2499999999999995E-2,0,0.376,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated toughened offline coated 11.5 (55.4)",50.6,2.0821052631578945,0,0,0.14042105263157895,0,0,0,0,0,0,8.7763157894736835E-2,0,0.45515789473684209,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated toughened offline coated 13.5 (66.4)",58.5,2.4442105263157892,0,0,0.1648421052631579,0,0,0,0,0,0,0.10302631578947367,0,0.53431578947368419,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearlite ","Laminated toughened offline coated 17.5 (88.4)",74.400000000000006,3.1684210526315786,0,0,0.21368421052631578,0,0,0,0,0,0,0.13355263157894737,0,0.69263157894736849,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic 3 mm",8,0.27,0,0,0.11600000000000001,0,0,0,0,0,0,2.52E-2,0,0.123,0,"20240940452-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic 4 mm",10.6,0.36000000000000004,0,0,0.15466666666666667,0,0,0,0,0,0,3.3599999999999998E-2,0,0.16400000000000001,0,"20240940452-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic 5 mm",13.3,0.45000000000000007,0,0,0.19333333333333336,0,0,0,0,0,0,4.1999999999999996E-2,0,0.20500000000000002,0,"20240940452-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic 6 mm",16,0.54,0,0,0.23200000000000001,0,0,0,0,0,0,5.04E-2,0,0.246,0,"20240940452-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic 8 mm",21.3,0.72000000000000008,0,0,0.30933333333333335,0,0,0,0,0,0,6.7199999999999996E-2,0,0.32800000000000001,0,"20240940452-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic 10 mm",26.6,0.81,0,0,0.36,0,0,0,0,0,0,7.8E-2,0,0.39200000000000002,0,"20240940452-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic 12 mm",31.9,0.9,0,0,0.41099999999999998,0,0,0,0,0,0,8.8999999999999996E-2,0,4.6600000000000003E-2,0,"20240940452-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic offline coated 3 mm",9.9,0.247,0,0,0.11600000000000001,0,0,0,0,0,0,2.52E-2,0,0.123,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic offline coated 4 mm",12.7,0.32933333333333331,0,0,0.15466666666666667,0,0,0,0,0,0,3.3599999999999998E-2,0,0.16400000000000001,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic offline coated 5 mm",15.5,0.41166666666666663,0,0,0.19333333333333336,0,0,0,0,0,0,4.1999999999999996E-2,0,0.20500000000000002,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic offline coated 6 mm",18.3,0.49399999999999999,0,0,0.23200000000000001,0,0,0,0,0,0,5.04E-2,0,0.246,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic offline coated 8 mm",23.9,0.65866666666666662,0,0,0.30933333333333335,0,0,0,0,0,0,6.7199999999999996E-2,0,0.32800000000000001,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic offline coated 10 mm",29.4,0.74099999999999999,0,0,0.36,0,0,0,0,0,0,7.8E-2,0,0.39200000000000002,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic offline coated 12 mm",35,0.82299999999999995,0,0,0.41099999999999998,0,0,0,0,0,0,8.8999999999999996E-2,0,4.6600000000000003E-2,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic toughened HST 3 mm",11.4,0.64700000000000002,0,0,0.11600000000000001,0,0,0,0,0,0,2.52E-2,0,0.123,0,"20240940468-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic toughened HST 4 mm",15.1,0.86266666666666669,0,0,0.15466666666666667,0,0,0,0,0,0,3.3599999999999998E-2,0,0.16400000000000001,0,"20240940468-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic toughened HST 5 mm",18.8,1.0783333333333334,0,0,0.19333333333333336,0,0,0,0,0,0,4.1999999999999996E-2,0,0.20500000000000002,0,"20240940468-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic toughened HST 6 mm",22.5,1.294,0,0,0.23200000000000001,0,0,0,0,0,0,5.04E-2,0,0.246,0,"20240940468-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic toughened HST 8 mm",29.9,1.7253333333333334,0,0,0.30933333333333335,0,0,0,0,0,0,6.7199999999999996E-2,0,0.32800000000000001,0,"20240940468-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic toughened HST 10 mm",37.299999999999997,1.9350000000000001,0,0,0.30933333333333335,0,0,0,0,0,0,5.04E-2,0,0.246,0,"20240940468-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic toughened HST 12 mm",44.7,2.109,0,0,0.36,0,0,0,0,0,0,6.7199999999999996E-2,0,0.32800000000000001,0,"20240940468-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic toughened HST offline coated 3 mm",13.1,0.65700000000000003,0,0,0.11600000000000001,0,0,0,0,0,0,2.52E-2,0,0.123,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic toughened HST offline coated 4 mm",16.899999999999999,0.876,0,0,0.15466666666666667,0,0,0,0,0,0,3.3599999999999998E-2,0,0.16400000000000001,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic toughened HST offline coated 5 mm",20.8,1.095,0,0,0.19333333333333336,0,0,0,0,0,0,4.1999999999999996E-2,0,0.20500000000000002,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic toughened HST offline coated 6 mm",24.6,1.3140000000000001,0,0,0.23200000000000001,0,0,0,0,0,0,5.04E-2,0,0.246,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic toughened HST offline coated 8 mm",32.299999999999997,1.752,0,0,0.30933333333333335,0,0,0,0,0,0,6.7199999999999996E-2,0,0.32800000000000001,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic toughened HST offline coated 10 mm",40,1.9350000000000001,0,0,0.30933333333333335,0,0,0,0,0,0,5.04E-2,0,0.246,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Planibel Clearvision","Monolithic toughened HST offline coated 12 mm",47.7,2.109,0,0,0.36,0,0,0,0,0,0,6.7199999999999996E-2,0,0.32800000000000001,0,"20240940460-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvision","Laminated 6.4 (33.1)",18.8,0.56399999999999995,0,0,0.11600000000000001,0,0,0,0,0,0,5.1700000000000003E-2,0,0.251,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated 6.8 (33.2)",20.9,0.59924999999999984,0,0,0.12324999999999998,0,0,0,0,0,0,5.4931250000000001E-2,0,0.26668749999999997,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated 8.4 (44.1)",24.4,0.74024999999999985,0,0,0.15225,0,0,0,0,0,0,6.7856250000000007E-2,0,0.32943749999999999,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated 8.8 (44.2)",26.5,0.77549999999999986,0,0,0.1595,0,0,0,0,0,0,7.1087500000000012E-2,0,0.34512500000000002,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated 10.4 (55.1)",29.9,0.91649999999999987,0,0,0.1885,0,0,0,0,0,0,8.4012500000000004E-2,0,0.40787499999999999,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated 10.8 (55.2)",32,0.95174999999999987,0,0,0.19575000000000001,0,0,0,0,0,0,8.7243750000000009E-2,0,0.42356250000000001,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated 11.5 (55.4)",36.299999999999997,1.0134374999999998,0,0,0.2084375,0,0,0,0,0,0,9.28984375E-2,0,0.45101562499999998,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated 12.4 (66.1)",35.5,1.0927499999999999,0,0,0.22474999999999998,0,0,0,0,0,0,0.10016875,0,0.48631249999999998,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated 12.8 (66.2)",37.6,1.1279999999999999,0,0,0.23199999999999998,0,0,0,0,0,0,0.10340000000000001,0,0.502,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated 13.5 (66.4)",41.8,1.1896874999999998,0,0,0.24468749999999997,0,0,0,0,0,0,0.1090546875,0,0.52945312499999997,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated 16.4 (88.1)",46.6,1.4452499999999995,0,0,0.29724999999999996,0,0,0,0,0,0,0.13248124999999999,0,0.64318749999999991,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated 16.8 (88.2)",48.7,1.4804999999999997,0,0,0.30449999999999999,0,0,0,0,0,0,0.13571250000000001,0,0.65887499999999999,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated 17.5 (88.4)",52.9,1.5421874999999996,0,0,0.31718749999999996,0,0,0,0,0,0,0.14136718749999999,0,0.68632812499999996,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated offline coated 6.4 (33.1)",21.2,0.56399999999999995,0,0,0.11600000000000001,0,0,0,0,0,0,5.1700000000000003E-2,0,0.251,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated offline coated 6.8 (33.2)",23.4,0.59924999999999984,0,0,0.12324999999999998,0,0,0,0,0,0,5.4931250000000001E-2,0,0.26668749999999997,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated offline coated  8.4 (44.1)",27,0.74024999999999985,0,0,0.15225,0,0,0,0,0,0,6.7856250000000007E-2,0,0.32943749999999999,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated offline coated 8.8 (44.2)",29.3,0.77549999999999986,0,0,0.1595,0,0,0,0,0,0,7.1087500000000012E-2,0,0.34512500000000002,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated offline coated 10.4 (55.1)",32.9,0.91649999999999987,0,0,0.1885,0,0,0,0,0,0,8.4012500000000004E-2,0,0.40787499999999999,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated offline coated 10.8 (55.2)",35.1,0.95174999999999987,0,0,0.19575000000000001,0,0,0,0,0,0,8.7243750000000009E-2,0,0.42356250000000001,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated offline coated 11.5 (55.4)",39.5,1.0134374999999998,0,0,0.2084375,0,0,0,0,0,0,9.28984375E-2,0,0.45101562499999998,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated offline coated 12.4 (66.1)",38.700000000000003,1.0927499999999999,0,0,0.22474999999999998,0,0,0,0,0,0,0.10016875,0,0.48631249999999998,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated offline coated 12.8 (66.2)",40.9,1.1279999999999999,0,0,0.23199999999999998,0,0,0,0,0,0,0.10340000000000001,0,0.502,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated offline coated 13.5 (66.4)",45.4,1.1896874999999998,0,0,0.24468749999999997,0,0,0,0,0,0,0.1090546875,0,0.52945312499999997,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated offline coated 16.4 (88.1)",50.4,1.4452499999999995,0,0,0.29724999999999996,0,0,0,0,0,0,0.13248124999999999,0,0.64318749999999991,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated offline coated 16.8 (88.2)",52.6,1.4804999999999997,0,0,0.30449999999999999,0,0,0,0,0,0,0.13571250000000001,0,0.65887499999999999,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated offline coated 17.5 (88.4)",57,1.5421874999999996,0,0,0.31718749999999996,0,0,0,0,0,0,0.14136718749999999,0,0.68632812499999996,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated toughened 9.5 (44.4)",39.6,1.72,0,0,0.11600000000000001,0,0,0,0,0,0,7.2499999999999995E-2,0,0.376,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated toughened 11.5 (55.4)",47.3,2.0821052631578945,0,0,0.14042105263157895,0,0,0,0,0,0,8.7763157894736835E-2,0,0.45515789473684209,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated toughened 13.5 (66.4)",54.9,2.4442105263157892,0,0,0.1648421052631579,0,0,0,0,0,0,0.10302631578947367,0,0.53431578947368419,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated toughened 17.5 (88.4)",70.3,3.1684210526315786,0,0,0.21368421052631578,0,0,0,0,0,0,0.13355263157894737,0,0.69263157894736849,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated toughened offline coated 9.5 (44.4)",42.6,1.72,0,0,0.11600000000000001,0,0,0,0,0,0,7.2499999999999995E-2,0,0.376,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated toughened offline coated 11.5 (55.4)",50.6,2.0821052631578945,0,0,0.14042105263157895,0,0,0,0,0,0,8.7763157894736835E-2,0,0.45515789473684209,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated toughened offline coated 13.5 (66.4)",58.5,2.4442105263157892,0,0,0.1648421052631579,0,0,0,0,0,0,0.10302631578947367,0,0.53431578947368419,0,"20240940458-FC","2029-12-31"]
[null,null,"AGC","Stratobel Clearvison","Laminated toughened offline coated 17.5 (88.4)",74.400000000000006,3.1684210526315786,0,0,0.21368421052631578,0,0,0,0,0,0,0.13355263157894737,0,0.69263157894736849,0,"20240940458-FC","2029-12-31"]
[]
[null,null,"Euroglass","Eurofloat","Monolithic 2 mm",8.4499999999999993,0,0,0,0,0,0,0,0,0,0,5.0999999999999997E-2,0,5.3999999999999999E-2,0,"EPD-GLS-20250386-IBC1-DE","2030-07-21",null,2]
[null,null,"Euroglass","Eurofloat","Monolithic 3 mm",{"$f":"($F$182/2)*X183","v":12.674999999999999},0,0,0,0,0,0,0,0,0,0,{"$f":"($Q$182/2)*X182","v":5.0999999999999997E-2},0,{"$f":"($S$182/2)*X183","v":8.1000000000000003E-2},0,"EPD-GLS-20250386-IBC1-DE","2030-07-22",null,3]
[null,null,"Euroglass","Eurofloat","Monolithic 4 mm",{"$f":"($F$182/2)*X184","v":16.899999999999999},0,0,0,0,0,0,0,0,0,0,{"$f":"($Q$182/2)*X183","v":7.6499999999999999E-2},0,{"$f":"($S$182/2)*X184","v":0.108},0,"EPD-GLS-20250386-IBC1-DE","2030-07-23",null,4]
[null,null,"Euroglass","Eurofloat","Monolithic 5 mm",21.125,0,0,0,0,0,0,0,0,0,0,0.10199999999999999,0,0.13500000000000001,0,"EPD-GLS-20250386-IBC1-DE","2030-07-24",null,5]
[null,null,"Euroglass","Eurofloat","Monolithic 6 mm",25.349999999999998,0,0,0,0,0,0,0,0,0,0,0.1275,0,0.16200000000000001,0,"EPD-GLS-20250386-IBC1-DE","2030-07-25",null,6]
[null,null,"Euroglass","Eurofloat","Monolithic 8 mm",33.799999999999997,0,0,0,0,0,0,0,0,0,0,0.153,0,0.216,0,"EPD-GLS-20250386-IBC1-DE","2030-07-26",null,8]
[null,null,"Euroglass","Eurofloat","Monolithic 10 mm",42.25,0,0,0,0,0,0,0,0,0,0,0.20399999999999999,0,0.27,0,"EPD-GLS-20250386-IBC1-DE","2030-07-27",null,10]
[null,null,"Euroglass","Eurofloat","Monolithic 12 mm",50.699999999999996,0,0,0,0,0,0,0,0,0,0,0.255,0,0.32400000000000001,0,"EPD-GLS-20250386-IBC1-DE","2030-07-28",null,12]
[null,null,"Euroglass","Eurofloat","Monolithic 15 mm",63.374999999999993,0,0,0,0,0,0,0,0,0,0,0.30599999999999999,0,0.40499999999999997,0,"EPD-GLS-20250386-IBC1-DE","2030-07-29",null,15]
[null,null,"Euroglass","Eurolamex","Laminated 6.4 (33.1)",16.7,0,0,0,0,0,0,0,0,0,0,7.9399999999999998E-2,0,9.2700000000000005E-2,0,"EPD-GLS-20230183-IBB3-EN","2029-02-04",null,6.4]
[null,null,"Euroglass","Eurolamex","Laminated 6.8 (33.2)",{"$f":"($F$191/$X$191)*X192","v":17.743749999999995},0,0,0,0,0,0,0,0,0,0,{"$f":"($Q$191/$X$191)*X192","v":8.4362499999999993E-2},0,{"$f":"($S$191/$X$191)*X192","v":9.8493750000000005E-2},0,"EPD-GLS-20230183-IBB3-EN","2029-02-04",null,6.8]
[null,null,"Euroglass","Eurolamex","Laminated 8.4 (44.1)",{"$f":"($F$191/$X$191)*X193","v":21.918749999999996},0,0,0,0,0,0,0,0,0,0,{"$f":"($Q$191/$X$191)*X193","v":0.1042125},0,{"$f":"($S$191/$X$191)*X193","v":0.12166875000000001},0,"EPD-GLS-20230183-IBB3-EN","2029-02-04",null,8.4]
[null,null,"Euroglass","Eurolamex","Laminated 8.8 (44.2)",22.962499999999999,0,0,0,0,0,0,0,0,0,0,0.10917499999999999,0,0.12746250000000001,0,"EPD-GLS-20230183-IBB3-EN","2029-02-04",null,8.8000000000000007]
[null,null,"Euroglass","Eurolamex","Laminated 10.4 (55.1)",27.137499999999996,0,0,0,0,0,0,0,0,0,0,0.129025,0,0.15063750000000001,0,"EPD-GLS-20230183-IBB3-EN","2029-02-04",null,10.4]
[null,null,"Euroglass","Eurolamex","Laminated 10.8 (55.2)",28.181249999999999,0,0,0,0,0,0,0,0,0,0,0.13398750000000001,0,0.15643125000000002,0,"EPD-GLS-20230183-IBB3-EN","2029-02-04",null,10.8]
[null,null,"Euroglass","Eurolamex","Laminated 11.5 (55.4)",30.007812499999996,0,0,0,0,0,0,0,0,0,0,0.14267187499999998,0,0.16657031250000001,0,"EPD-GLS-20230183-IBB3-EN","2029-02-04",null,11.5]
[null,null,"Euroglass","Eurolamex","Laminated 12.4 (66.1)",32.356249999999996,0,0,0,0,0,0,0,0,0,0,0.15383749999999999,0,0.17960625000000002,0,"EPD-GLS-20230183-IBB3-EN","2029-02-04",null,12.4]
[null,null,"Euroglass","Eurolamex","Laminated 12.8 (66.2)",33.4,0,0,0,0,0,0,0,0,0,0,0.1588,0,0.18540000000000001,0,"EPD-GLS-20230183-IBB3-EN","2029-02-04",null,12.8]
[null,null,"Euroglass","Eurolamex","Laminated 13.5 (66.4)",35.226562499999993,0,0,0,0,0,0,0,0,0,0,0.16748437499999999,0,0.1955390625,0,"EPD-GLS-20230183-IBB3-EN","2029-02-04",null,13.5]
[null,null,"Euroglass","Eurolamex","Laminated 16.4 (88.1)",42.793749999999989,0,0,0,0,0,0,0,0,0,0,0.20346249999999996,0,0.23754375,0,"EPD-GLS-20230183-IBB3-EN","2029-02-04",null,16.399999999999999]
[null,null,"Euroglass","Eurolamex","Laminated 16.8 (88.2)",43.837499999999991,0,0,0,0,0,0,0,0,0,0,0.208425,0,0.24333750000000001,0,"EPD-GLS-20230183-IBB3-EN","2029-02-04",null,16.8]
[null,null,"Euroglass","Eurolamex","Laminated 17.5 (88.4)",45.664062499999993,0,0,0,0,0,0,0,0,0,0,0.21710937499999999,0,0.2534765625,0,"EPD-GLS-20230183-IBB3-EN","2029-02-04",null,17.5]
[]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic 2 mm",3.19,0.34449999999999997,0,0,0.67500000000000004,0,0,0,0,0,0,4.7449999999999999E-2,0,0.2165,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic 3 mm",4.7850000000000001,0.51674999999999993,0,0,1.0125000000000002,0,0,0,0,0,0,7.1175000000000002E-2,0,0.32474999999999998,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic 4 mm",6.38,0.68899999999999995,0,0,1.35,0,0,0,0,0,0,9.4899999999999998E-2,0,0.433,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic 5 mm",7.9749999999999996,0.86124999999999996,0,0,1.6875,0,0,0,0,0,0,0.11862499999999999,0,0.54125000000000001,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic 6 mm",9.57,1.0334999999999999,0,0,2.0250000000000004,0,0,0,0,0,0,0.14235,0,0.64949999999999997,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic 8 mm",12.76,1.3779999999999999,0,0,2.7,0,0,0,0,0,0,0.1898,0,0.86599999999999999,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic 10 mm",15.95,1.7224999999999999,0,0,3.375,0,0,0,0,0,0,0.23724999999999999,0,1.0825,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic 12 mm",19.14,2.0669999999999997,0,0,4.0500000000000007,0,0,0,0,0,0,0.28470000000000001,0,1.2989999999999999,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic 15 mm",23.925000000000001,2.5837499999999998,0,0,5.0625,0,0,0,0,0,0,0.355875,0,1.62375,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic coated 2 mm",3.625,0.34449999999999997,0,0,0.67500000000000004,0,0,0,0,0,0,4.7449999999999999E-2,0,0.2165,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic coated 3 mm",5.4375,0.51674999999999993,0,0,1.0125000000000002,0,0,0,0,0,0,7.1175000000000002E-2,0,0.32474999999999998,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic coated 4 mm",7.25,0.68899999999999995,0,0,1.35,0,0,0,0,0,0,9.4899999999999998E-2,0,0.433,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic coated 5 mm",9.0625,0.86124999999999996,0,0,1.6875,0,0,0,0,0,0,0.11862499999999999,0,0.54125000000000001,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic coated 6 mm",10.875,1.0334999999999999,0,0,2.0250000000000004,0,0,0,0,0,0,0.14235,0,0.64949999999999997,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic coated 8 mm",14.5,1.3779999999999999,0,0,2.7,0,0,0,0,0,0,0.1898,0,0.86599999999999999,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic coated 10 mm",18.125,1.7224999999999999,0,0,3.375,0,0,0,0,0,0,0.23724999999999999,0,1.0825,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic coated 12 mm",21.75,2.0669999999999997,0,0,4.0500000000000007,0,0,0,0,0,0,0.28470000000000001,0,1.2989999999999999,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Monolithic coated 15 mm",27.1875,2.5837499999999998,0,0,5.0625,0,0,0,0,0,0,0.355875,0,1.62375,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Laminated 6.4 (33.1)",7.4690000000000003,1.0725,0,0,2.1074999999999999,0,0,0,0,0,0,0.14774999999999999,0,0.67575000000000007,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Laminated 6.8 (33.2)",9.2690000000000001,1.0725,0,0,2.1074999999999999,0,0,0,0,0,0,0.14774999999999999,0,0.67575000000000007,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Laminated 8.4 (44.1)",9.1039999999999992,1.43,0,0,2.81,0,0,0,0,0,0,0.19700000000000001,0,0.90100000000000002,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Laminated 8.8 (44.2)",10.904,1.43,0,0,2.81,0,0,0,0,0,0,0.19700000000000001,0,0.90100000000000002,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Laminated 10.4 (55.1)",10.739000000000001,1.7874999999999999,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,1.12625,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Laminated 10.8 (55.2)",12.539,1.7874999999999999,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,1.12625,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Laminated 11.5 (55.4)",16.138999999999999,1.7874999999999999,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,1.12625,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Laminated 12.4 (66.1)",12.374000000000001,2.145,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.3515000000000001,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Laminated 12.8 (66.2)",14.173999999999999,2.145,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.3515000000000001,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Laminated 13.5 (66.4)",17.774000000000001,2.145,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.3515000000000001,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Laminated 16.4 (88.1)",15.644,2.86,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.802,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Laminated 16.8 (88.2)",17.443999999999999,2.86,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.802,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 6 Low Carbon","Laminated 17.5 (88.4)",21.044,2.86,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.802,0,"4791438322.105.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic 2 mm",4.29,0.34449999999999997,0,0,0.67500000000000004,0,0,0,0,0,0,4.7449999999999999E-2,0,0.2165,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic 3 mm",6.4350000000000005,0.51674999999999993,0,0,1.0125000000000002,0,0,0,0,0,0,7.1175000000000002E-2,0,0.32474999999999998,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic 4 mm",8.58,0.68899999999999995,0,0,1.35,0,0,0,0,0,0,9.4899999999999998E-2,0,0.433,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic 5 mm",10.725,0.86124999999999996,0,0,1.6875,0,0,0,0,0,0,0.11862499999999999,0,0.54125000000000001,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic 6 mm",12.870000000000001,1.0334999999999999,0,0,2.0250000000000004,0,0,0,0,0,0,0.14235,0,0.64949999999999997,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic 8 mm",17.16,1.3779999999999999,0,0,2.7,0,0,0,0,0,0,0.1898,0,0.86599999999999999,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic 10 mm",21.45,1.7224999999999999,0,0,3.375,0,0,0,0,0,0,0.23724999999999999,0,1.0825,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic 12 mm",25.740000000000002,2.0669999999999997,0,0,4.0500000000000007,0,0,0,0,0,0,0.28470000000000001,0,1.2989999999999999,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic 15 mm",32.174999999999997,2.5837499999999998,0,0,5.0625,0,0,0,0,0,0,0.355875,0,1.62375,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic coated 2 mm",5,0.34449999999999997,0,0,0.67500000000000004,0,0,0,0,0,0,4.7449999999999999E-2,0,0.2165,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic coated 3 mm",7.5,0.51674999999999993,0,0,1.0125000000000002,0,0,0,0,0,0,7.1175000000000002E-2,0,0.32474999999999998,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic coated 4 mm",10,0.68899999999999995,0,0,1.35,0,0,0,0,0,0,9.4899999999999998E-2,0,0.433,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic coated 5 mm",12.5,0.86124999999999996,0,0,1.6875,0,0,0,0,0,0,0.11862499999999999,0,0.54125000000000001,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic coated 6 mm",15,1.0334999999999999,0,0,2.0250000000000004,0,0,0,0,0,0,0.14235,0,0.64949999999999997,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic coated 8 mm",20,1.3779999999999999,0,0,2.7,0,0,0,0,0,0,0.1898,0,0.86599999999999999,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic coated 10 mm",25,1.7224999999999999,0,0,3.375,0,0,0,0,0,0,0.23724999999999999,0,1.0825,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic coated 12 mm",30,2.0669999999999997,0,0,4.0500000000000007,0,0,0,0,0,0,0.28470000000000001,0,1.2989999999999999,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Monolithic coated 15 mm",37.5,2.5837499999999998,0,0,5.0625,0,0,0,0,0,0,0.355875,0,1.62375,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Laminated 6.4 (33.1)",16.754999999999999,1.0725,0,0,2.1074999999999999,0,0,0,0,0,0,0.14774999999999999,0,0.67575000000000007,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Laminated 6.8 (33.2)",18.555,1.0725,0,0,2.1074999999999999,0,0,0,0,0,0,0.14774999999999999,0,0.67575000000000007,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Laminated 8.4 (44.1)",21.15,1.43,0,0,2.81,0,0,0,0,0,0,0.19700000000000001,0,0.90100000000000002,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Laminated 8.8 (44.2)",22.95,1.43,0,0,2.81,0,0,0,0,0,0,0.19700000000000001,0,0.90100000000000002,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Laminated 10.4 (55.1)",25.544999999999998,1.7874999999999999,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,1.12625,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Laminated 10.8 (55.2)",27.344999999999999,1.7874999999999999,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,1.12625,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Laminated 11.5 (55.4)",30.944999999999997,1.7874999999999999,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,1.12625,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Laminated 12.4 (66.1)",29.939999999999998,2.145,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.3515000000000001,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Laminated 12.8 (66.2)",31.74,2.145,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.3515000000000001,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Laminated 13.5 (66.4)",35.340000000000003,2.145,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.3515000000000001,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Laminated 16.4 (88.1)",38.729999999999997,2.86,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.802,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Laminated 16.8 (88.2)",40.53,2.86,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.802,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","NEXA 9 Low Carbon","Laminated 17.5 (88.4)",44.13,2.86,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.802,0,"4791438322.106.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic 2 mm",4.82,0.34449999999999997,0,0,0.67500000000000004,0,0,0,0,0,0,4.7449999999999999E-2,0,0.2165,0,"4791438322.102.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic 3 mm",7.23,0.51674999999999993,0,0,1.0125000000000002,0,0,0,0,0,0,7.1175000000000002E-2,0,0.32474999999999998,0,"4791438322.102.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic 4 mm",9.64,0.68899999999999995,0,0,1.35,0,0,0,0,0,0,9.4899999999999998E-2,0,0.433,0,"4791438322.102.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic 5 mm",12.05,0.86124999999999996,0,0,1.6875,0,0,0,0,0,0,0.11862499999999999,0,0.54125000000000001,0,"4791438322.102.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic 6 mm",14.46,1.0334999999999999,0,0,2.0250000000000004,0,0,0,0,0,0,0.14235,0,0.64949999999999997,0,"4791438322.102.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic 8 mm",19.28,1.3779999999999999,0,0,2.7,0,0,0,0,0,0,0.1898,0,0.86599999999999999,0,"4791438322.102.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic 10 mm",24.1,1.7224999999999999,0,0,3.375,0,0,0,0,0,0,0.23724999999999999,0,1.0825,0,"4791438322.102.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic 12 mm",28.92,2.0669999999999997,0,0,4.0500000000000007,0,0,0,0,0,0,0.28470000000000001,0,1.2989999999999999,0,"4791438322.102.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic 15 mm",36.150000000000006,2.5837499999999998,0,0,5.0625,0,0,0,0,0,0,0.355875,0,1.62375,0,"4791438322.102.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic coated 2 mm",5.5349999999999993,0.34449999999999997,0,0,0.67500000000000004,0,0,0,0,0,0,4.7449999999999999E-2,0,0.2165,0,"4791438322.101.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic coated 3 mm",8.3024999999999984,0.51674999999999993,0,0,1.0125000000000002,0,0,0,0,0,0,7.1175000000000002E-2,0,0.32474999999999998,0,"4791438322.101.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic coated 4 mm",11.069999999999999,0.68899999999999995,0,0,1.35,0,0,0,0,0,0,9.4899999999999998E-2,0,0.433,0,"4791438322.101.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic coated 5 mm",13.837499999999999,0.86124999999999996,0,0,1.6875,0,0,0,0,0,0,0.11862499999999999,0,0.54125000000000001,0,"4791438322.101.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic coated 6 mm",16.604999999999997,1.0334999999999999,0,0,2.0250000000000004,0,0,0,0,0,0,0.14235,0,0.64949999999999997,0,"4791438322.101.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic coated 8 mm",22.139999999999997,1.3779999999999999,0,0,2.7,0,0,0,0,0,0,0.1898,0,0.86599999999999999,0,"4791438322.101.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic coated 10 mm",27.674999999999997,1.7224999999999999,0,0,3.375,0,0,0,0,0,0,0.23724999999999999,0,1.0825,0,"4791438322.101.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic coated 12 mm",33.209999999999994,2.0669999999999997,0,0,4.0500000000000007,0,0,0,0,0,0,0.28470000000000001,0,1.2989999999999999,0,"4791438322.101.1","2029-08-29"]
[null,null,"Guardian Glass","Extraclear","Monolithic coated 15 mm",41.512499999999996,2.5837499999999998,0,0,5.0625,0,0,0,0,0,0,0.355875,0,1.62375,0,"4791438322.101.1","2029-08-29"]
[null,null,"Guardian Glass","Ultraclear","Monolithic 2 mm",6.2,0.34449999999999997,0,0,0.67500000000000004,0,0,0,0,0,0,4.7449999999999999E-2,0,0.2165,0,"4791438322.103.1","2029-08-29"]
[null,null,"Guardian Glass","Ultraclear","Monolithic 3 mm",9.3000000000000007,0.51674999999999993,0,0,1.0125000000000002,0,0,0,0,0,0,7.1175000000000002E-2,0,0.32474999999999998,0,"4791438322.103.1","2029-08-29"]
[null,null,"Guardian Glass","Ultraclear","Monolithic 4 mm",12.4,0.68899999999999995,0,0,1.35,0,0,0,0,0,0,9.4899999999999998E-2,0,0.433,0,"4791438322.103.1","2029-08-29"]
[null,null,"Guardian Glass","Ultraclear","Monolithic 5 mm",15.5,0.86124999999999996,0,0,1.6875,0,0,0,0,0,0,0.11862499999999999,0,0.54125000000000001,0,"4791438322.103.1","2029-08-29"]
[null,null,"Guardian Glass","Ultraclear","Monolithic 6 mm",18.600000000000001,1.0334999999999999,0,0,2.0250000000000004,0,0,0,0,0,0,0.14235,0,0.64949999999999997,0,"4791438322.103.1","2029-08-29"]
[null,null,"Guardian Glass","Ultraclear","Monolithic 8 mm",24.8,1.3779999999999999,0,0,2.7,0,0,0,0,0,0,0.1898,0,0.86599999999999999,0,"4791438322.103.1","2029-08-29"]
[null,null,"Guardian Glass","Ultraclear","Monolithic 10 mm",31,1.7224999999999999,0,0,3.375,0,0,0,0,0,0,0.23724999999999999,0,1.0825,0,"4791438322.103.1","2029-08-29"]
[null,null,"Guardian Glass","Ultraclear","Monolithic 12 mm",37.200000000000003,2.0669999999999997,0,0,4.0500000000000007,0,0,0,0,0,0,0.28470000000000001,0,1.2989999999999999,0,"4791438322.103.1","2029-08-29"]
[null,null,"Guardian Glass","Ultraclear","Monolithic 15 mm",46.5,2.5837499999999998,0,0,5.0625,0,0,0,0,0,0,0.355875,0,1.62375,0,"4791438322.103.1","2029-08-29"]
[null,null,"Guardian Glass","Laminated","Laminated 6.4 (33.1)",17.678000000000001,1.0725,0,0,2.1074999999999999,0,0,0,0,0,0,0.14774999999999999,0,0.67575000000000007,0,"4791438322.104.1","2029-08-29"]
[null,null,"Guardian Glass","Laminated","Laminated 6.8 (33.2)",19.478000000000002,1.0725,0,0,2.81,0,0,0,0,0,0,0.19700000000000001,0,0.67575000000000007,0,"4791438322.104.1","2029-08-29"]
[null,null,"Guardian Glass","Laminated","Laminated 8.4 (44.1)",22.728000000000002,1.43,0,0,2.81,0,0,0,0,0,0,0.19700000000000001,0,0.90100000000000002,0,"4791438322.104.1","2029-08-29"]
[null,null,"Guardian Glass","Laminated","Laminated 8.8 (44.2)",24.528000000000002,1.43,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,0.90100000000000002,0,"4791438322.104.1","2029-08-29"]
[null,null,"Guardian Glass","Laminated","Laminated 10.4 (55.1)",27.778000000000002,1.7874999999999999,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,1.12625,0,"4791438322.104.1","2029-08-29"]
[null,null,"Guardian Glass","Laminated","Laminated 10.8 (55.2)",29.578000000000003,1.7874999999999999,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,1.12625,0,"4791438322.104.1","2029-08-29"]
[null,null,"Guardian Glass","Laminated","Laminated 11.5 (55.4)",33.178000000000004,1.7874999999999999,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.12625,0,"4791438322.104.1","2029-08-29"]
[null,null,"Guardian Glass","Laminated","Laminated 12.4 (66.1)",32.827999999999996,2.145,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.3515000000000001,0,"4791438322.104.1","2029-08-29"]
[null,null,"Guardian Glass","Laminated","Laminated 12.8 (66.2)",34.628,2.145,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.3515000000000001,0,"4791438322.104.1","2029-08-29"]
[null,null,"Guardian Glass","Laminated","Laminated 13.5 (66.4)",38.228000000000002,2.145,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.3515000000000001,0,"4791438322.104.1","2029-08-29"]
[null,null,"Guardian Glass","Laminated","Laminated 16.4 (88.1)",42.927999999999997,2.86,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.802,0,"4791438322.104.1","2029-08-29"]
[null,null,"Guardian Glass","Laminated","Laminated 16.8 (88.2)",44.728000000000002,2.86,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.802,0,"4791438322.104.1","2029-08-29"]
[null,null,"Guardian Glass","Laminated","Laminated 17.5 (88.4)",48.328000000000003,2.86,0,0,0,0,0,0,0,0,0,0,0,1.802,0,"4791438322.104.1","2029-08-29"]
[]
[null,null,"Pilkington NSG","Mirai","Monolithic 4 mm",5.4,1.0880000000000001,2.4E-2,0,2.2400000000000002,0,0,0,0,0,0,0.5,0,0.55600000000000005,0,"S-P-11498 V2","2029-01-23"]
[null,null,"Pilkington NSG","Mirai","Monolithic 6 mm",8.1,1.6319999999999999,3.5999999999999997E-2,0,3.36,0,0,0,0,0,0,0.75,0,0.83399999999999996,0,"S-P-11498 V2","2029-01-23"]
[null,null,"Pilkington NSG","Mirai","Monolithic 8 mm",10.8,2.1760000000000002,4.8000000000000001E-2,0,4.4800000000000004,0,0,0,0,0,0,1,0,1.1120000000000001,0,"S-P-11498 V2","2029-01-23"]
[null,null,"Pilkington NSG","Mirai","Monolithic offline coated 4 mm ",5.9266666670000001,0.20533299999999999,3.5999999999999997E-2,0,0.100666667,0,0,0,0,0,0,0.152,0,0.16975000000000001,0,"IES-0024742","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Monolithic offline coated 6 mm",8.89,0.308,5.3999999999999999E-2,0,0.151,0,0,0,0,0,0,0.22800000000000001,0,0.29599999999999999,0,"IES-0024742","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Monolithic offline coated 8 mm",11.85333333,0.410667,7.1999999999999995E-2,0,0.201333333,0,0,0,0,0,0,0.30399999999999999,0,0.39466666700000003,0,"IES-0024742","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Monolithic toughened 4 mm",8.8000000000000007,0.20533299999999999,3.5999999999999997E-2,0,0.100666667,0,0,0,0,0,0,0.152,0,0.18665999999999999,0,"IES-0024744","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Monolithic toughened 6 mm",13.2,0.308,5.3999999999999999E-2,0,0.151,0,0,0,0,0,0,0.22800000000000001,0,0.28000000000000003,0,"IES-0024744","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Monolithic toughened 8 mm",17.600000000000001,0.410667,7.1999999999999995E-2,0,0.201333333,0,0,0,0,0,0,0.30399999999999999,0,0.37333333299999999,0,"IES-0024744","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Monolithic toughened offline coated 4 mm ",7.4666666670000001,0.20533299999999999,3.5999999999999997E-2,0,0.100666667,0,0,0,0,0,0,0.152,0,0.19066666700000001,0,"IES-0024743","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Monolithic toughened offline coated 6 mm",11.2,0.308,5.3999999999999999E-2,0,0.151,0,0,0,0,0,0,0.22800000000000001,0,0.28599999999999998,0,"IES-0024743","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Monolithic offline coated 8 mm",14.93333333,0.410667,7.1999999999999995E-2,0,0.201333333,0,0,0,0,0,0,0.30399999999999999,0,0.381333333,0,"IES-0024743","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Laminated 8.8 (44.2)",19.9375,0.4345,3.7124999999999998E-2,0,3.7124999999999998E-2,0,0,0,0,0,0,0.3238125,0,0.49156250000000001,0,"IES-0024746","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Laminated 10.8 (55.2)",24.46875,0.53325,4.5562999999999999E-2,0,4.5562499999999999E-2,0,0,0,0,0,0,0.39740625000000002,0,0.60328124999999999,0,"IES-0024746","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Laminated 11.5 (55.4)",26.0546875,0.56781300000000001,4.8515999999999997E-2,0,4.8515625E-2,0,0,0,0,0,0,0.42316406299999998,0,0.642382813,0,"IES-0024746","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Laminated 12.8 (66.2)",29,0.63200000000000001,5.3999999999999999E-2,0,5.3999999999999999E-2,0,0,0,0,0,0,0.47099999999999997,0,0.71499999999999997,0,"IES-0024746","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Laminated 13.5 (66.4)",30.5859375,0.66656300000000002,5.6952999999999997E-2,0,5.6953125E-2,0,0,0,0,0,0,0.49675781299999999,0,0.75410156299999997,0,"IES-0024746","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Laminated offline coated 8.8 (44.2)",20.556249999999999,0.4345,3.7124999999999998E-2,0,3.7124999999999998E-2,0,0,0,0,0,0,0.3238125,0,0.495,0,"IES-0024745","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Laminated offline coated 10.8 (55.2)",25.228124999999999,0.53325,4.5562999999999999E-2,0,4.5562499999999999E-2,0,0,0,0,0,0,0.39740625000000002,0,0.60750000000000004,0,"IES-0024745","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Laminated offline coated 11.5 (55.4)",26.86328125,0.56781300000000001,4.8515999999999997E-2,0,4.8515625E-2,0,0,0,0,0,0,0.42316406299999998,0,0.64687499999999998,0,"IES-0024745","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Laminated offline coated 12.8 (66.2)",29.9,0.63200000000000001,5.3999999999999999E-2,0,5.3999999999999999E-2,0,0,0,0,0,0,0.47099999999999997,0,0.72,0,"IES-0024745","2031-01-16"]
[null,null,"Pilkington NSG","Mirai","Laminated offline coated 13.5 (66.4)",31.53515625,0.66656300000000002,5.6952999999999997E-2,0,5.6953125E-2,0,0,0,0,0,0,0.49675781299999999,0,0.75937500000000002,0,"IES-0024745","2031-01-16"]
[null,null,"Pilkington NSG","Optifloat","Monolithic 2 mm",{"$f":"2.75*2","v":5.5},{"$f":"0.0454*2","v":9.0800000000000006E-2},{"$f":"0.0545*2","v":0.109},0,{"$f":"0.0787*2","v":0.15740000000000001},0,0,0,0,0,0,{"$f":"0.0208*2","v":4.1599999999999998E-2},0,{"$f":"0.0235*2","v":4.7E-2},0,"S-P-08816","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic 3 mm",{"$f":"2.75*3","v":8.25},{"$f":"0.0454*3","v":0.13620000000000002},{"$f":"0.0545*3","v":0.16350000000000001},0,{"$f":"0.0787*3","v":0.23610000000000003},0,0,0,0,0,0,{"$f":"0.0208*3","v":6.2399999999999997E-2},0,{"$f":"0.0235*3","v":7.0500000000000007E-2},0,"S-P-08816","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic 4 mm",{"$f":"2.75*4","v":11},{"$f":"0.0454*4","v":0.18160000000000001},{"$f":"0.0545*4","v":0.218},0,{"$f":"0.0787*4","v":0.31480000000000002},0,0,0,0,0,0,{"$f":"0.0208*4","v":8.3199999999999996E-2},0,{"$f":"0.0235*4","v":9.4E-2},0,"S-P-08816","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic 5 mm",{"$f":"2.75*5","v":13.75},{"$f":"0.0454*5","v":0.22700000000000001},{"$f":"0.0545*5","v":0.27250000000000002},0,{"$f":"0.0787*5","v":0.39350000000000002},0,0,0,0,0,0,{"$f":"0.0208*5","v":0.104},0,{"$f":"0.0235*5","v":0.11749999999999999},0,"S-P-08816","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic 6 mm",{"$f":"2.75*6","v":16.5},{"$f":"0.0454*6","v":0.27240000000000003},{"$f":"0.0545*6","v":0.32700000000000001},0,{"$f":"0.0787*6","v":0.47220000000000006},0,0,0,0,0,0,{"$f":"0.0208*6","v":0.12479999999999999},0,{"$f":"0.0235*6","v":0.14100000000000001},0,"S-P-08816","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic 8 mm",{"$f":"2.75*8","v":22},{"$f":"0.0454*8","v":0.36320000000000002},{"$f":"0.0545*8","v":0.436},0,{"$f":"0.0787*8","v":0.62960000000000005},0,0,0,0,0,0,{"$f":"0.0208*8","v":0.16639999999999999},0,{"$f":"0.0235*8","v":0.188},0,"S-P-08816","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic 10 mm",{"$f":"2.75*10","v":27.5},{"$f":"0.0454*10","v":0.45400000000000001},{"$f":"0.0545*10","v":0.54500000000000004},0,{"$f":"0.0787*10","v":0.78700000000000003},0,0,0,0,0,0,{"$f":"0.0208*10","v":0.20799999999999999},0,{"$f":"0.0235*10","v":0.23499999999999999},0,"S-P-08816","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic 12 mm",{"$f":"2.75*12","v":33},{"$f":"0.0454*12","v":0.54480000000000006},{"$f":"0.0545*12","v":0.65400000000000003},0,{"$f":"0.0787*12","v":0.94440000000000013},0,0,0,0,0,0,{"$f":"0.0208*12","v":0.24959999999999999},0,{"$f":"0.0235*12","v":0.28200000000000003},0,"S-P-08816","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic 15 mm",{"$f":"2.75*15","v":41.25},{"$f":"0.0454*15","v":0.68100000000000005},{"$f":"0.0545*15","v":0.8175},0,{"$f":"0.0787*15","v":1.1805000000000001},0,0,0,0,0,0,{"$f":"0.0208*15","v":0.312},0,{"$f":"0.0235*15","v":0.35249999999999998},0,"S-P-08816","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic offline coated 3 mm",{"$f":"2.79*3","v":8.370000000000001},{"$f":"0.0454*3","v":0.13620000000000002},{"$f":"0.0545*3","v":0.16350000000000001},0,{"$f":"0.0787*3","v":0.23610000000000003},0,0,0,0,0,0,{"$f":"0.0208*3","v":6.2399999999999997E-2},0,{"$f":"0.0235*3","v":7.0500000000000007E-2},0,"S-P-08819","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic offline coated 4 mm",{"$f":"2.79*4","v":11.16},{"$f":"0.0454*4","v":0.18160000000000001},{"$f":"0.0545*4","v":0.218},0,{"$f":"0.0787*4","v":0.31480000000000002},0,0,0,0,0,0,{"$f":"0.0208*4","v":8.3199999999999996E-2},0,{"$f":"0.0235*4","v":9.4E-2},0,"S-P-08819","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic offline coated 5 mm",{"$f":"2.79*5","v":13.95},{"$f":"0.0454*5","v":0.22700000000000001},{"$f":"0.0545*5","v":0.27250000000000002},0,{"$f":"0.0787*5","v":0.39350000000000002},0,0,0,0,0,0,{"$f":"0.0208*5","v":0.104},0,{"$f":"0.0235*5","v":0.11749999999999999},0,"S-P-08819","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic offline coated 6 mm",{"$f":"2.79*6","v":16.740000000000002},{"$f":"0.0454*6","v":0.27240000000000003},{"$f":"0.0545*6","v":0.32700000000000001},0,{"$f":"0.0787*6","v":0.47220000000000006},0,0,0,0,0,0,{"$f":"0.0208*6","v":0.12479999999999999},0,{"$f":"0.0235*6","v":0.14100000000000001},0,"S-P-08819","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic offline coated 8 mm",{"$f":"2.79*8","v":22.32},{"$f":"0.0454*8","v":0.36320000000000002},{"$f":"0.0545*8","v":0.436},0,{"$f":"0.0787*8","v":0.62960000000000005},0,0,0,0,0,0,{"$f":"0.0208*8","v":0.16639999999999999},0,{"$f":"0.0235*8","v":0.188},0,"S-P-08819","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic offline coated 10 mm",{"$f":"2.79*10","v":27.9},{"$f":"0.0454*10","v":0.45400000000000001},{"$f":"0.0545*10","v":0.54500000000000004},0,{"$f":"0.0787*10","v":0.78700000000000003},0,0,0,0,0,0,{"$f":"0.0208*10","v":0.20799999999999999},0,{"$f":"0.0235*10","v":0.23499999999999999},0,"S-P-08819","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic offline coated 12 mm",{"$f":"2.79*12","v":33.480000000000004},{"$f":"0.0454*12","v":0.54480000000000006},{"$f":"0.0545*12","v":0.65400000000000003},0,{"$f":"0.0787*12","v":0.94440000000000013},0,0,0,0,0,0,{"$f":"0.0208*12","v":0.24959999999999999},0,{"$f":"0.0235*12","v":0.28200000000000003},0,"S-P-08819","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic online coated 3 mm",{"$f":"4.27*3","v":12.809999999999999},{"$f":"0.0454*3","v":0.13620000000000002},{"$f":"0.0545*3","v":0.16350000000000001},0,{"$f":"0.0787*3","v":0.23610000000000003},0,0,0,0,0,0,{"$f":"0.0208*3","v":6.2399999999999997E-2},0,{"$f":"0.0235*3","v":7.0500000000000007E-2},0,"S-P-08821","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic online coated 4 mm",{"$f":"4.27*4","v":17.079999999999998},{"$f":"0.0454*4","v":0.18160000000000001},{"$f":"0.0545*4","v":0.218},0,{"$f":"0.0787*4","v":0.31480000000000002},0,0,0,0,0,0,{"$f":"0.0208*4","v":8.3199999999999996E-2},0,{"$f":"0.0235*4","v":9.4E-2},0,"S-P-08821","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic online coated 5 mm",{"$f":"4.27*5","v":21.349999999999998},{"$f":"0.0454*5","v":0.22700000000000001},{"$f":"0.0545*5","v":0.27250000000000002},0,{"$f":"0.0787*5","v":0.39350000000000002},0,0,0,0,0,0,{"$f":"0.0208*5","v":0.104},0,{"$f":"0.0235*5","v":0.11749999999999999},0,"S-P-08821","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic online coated 6 mm",{"$f":"4.27*6","v":25.619999999999997},{"$f":"0.0454*6","v":0.27240000000000003},{"$f":"0.0545*6","v":0.32700000000000001},0,{"$f":"0.0787*6","v":0.47220000000000006},0,0,0,0,0,0,{"$f":"0.0208*6","v":0.12479999999999999},0,{"$f":"0.0235*6","v":0.14100000000000001},0,"S-P-08821","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic online coated 8 mm",{"$f":"4.27*8","v":34.159999999999997},{"$f":"0.0454*8","v":0.36320000000000002},{"$f":"0.0545*8","v":0.436},0,{"$f":"0.0787*8","v":0.62960000000000005},0,0,0,0,0,0,{"$f":"0.0208*8","v":0.16639999999999999},0,{"$f":"0.0235*8","v":0.188},0,"S-P-08821","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic online coated 10 mm",{"$f":"4.27*10","v":42.699999999999996},{"$f":"0.0454*10","v":0.45400000000000001},{"$f":"0.0545*10","v":0.54500000000000004},0,{"$f":"0.0787*10","v":0.78700000000000003},0,0,0,0,0,0,{"$f":"0.0208*10","v":0.20799999999999999},0,{"$f":"0.0235*10","v":0.23499999999999999},0,"S-P-08821","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened 4 mm",{"$f":"4.4*4","v":17.600000000000001},{"$f":"0.0454*4","v":0.18160000000000001},{"$f":"0.0545*4","v":0.218},0,{"$f":"0.0787*4","v":0.31480000000000002},0,0,0,0,0,0,{"$f":"0.0208*4","v":8.3199999999999996E-2},0,{"$f":"0.0349*4","v":0.1396},0,"S-P-08822","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened 5 mm",{"$f":"4.4*5","v":22},{"$f":"0.0454*5","v":0.22700000000000001},{"$f":"0.0545*5","v":0.27250000000000002},0,{"$f":"0.0787*5","v":0.39350000000000002},0,0,0,0,0,0,{"$f":"0.0208*5","v":0.104},0,{"$f":"0.0349*5","v":0.17449999999999999},0,"S-P-08822","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened 6 mm",{"$f":"4.4*6","v":26.400000000000002},{"$f":"0.0454*6","v":0.27240000000000003},{"$f":"0.0545*6","v":0.32700000000000001},0,{"$f":"0.0787*6","v":0.47220000000000006},0,0,0,0,0,0,{"$f":"0.0208*6","v":0.12479999999999999},0,{"$f":"0.0349*6","v":0.2094},0,"S-P-08822","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened 8 mm",{"$f":"4.4*8","v":35.200000000000003},{"$f":"0.0454*8","v":0.36320000000000002},{"$f":"0.0545*8","v":0.436},0,{"$f":"0.0787*8","v":0.62960000000000005},0,0,0,0,0,0,{"$f":"0.0208*8","v":0.16639999999999999},0,{"$f":"0.0349*8","v":0.2792},0,"S-P-08822","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened 10 mm",{"$f":"4.4*10","v":44},{"$f":"0.0454*10","v":0.45400000000000001},{"$f":"0.0545*10","v":0.54500000000000004},0,{"$f":"0.0787*10","v":0.78700000000000003},0,0,0,0,0,0,{"$f":"0.0208*10","v":0.20799999999999999},0,{"$f":"0.0349*10","v":0.34899999999999998},0,"S-P-08822","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened 12 mm",{"$f":"4.4*12","v":52.800000000000004},{"$f":"0.0454*12","v":0.54480000000000006},{"$f":"0.0545*12","v":0.65400000000000003},0,{"$f":"0.0787*12","v":0.94440000000000013},0,0,0,0,0,0,{"$f":"0.0208*12","v":0.24959999999999999},0,{"$f":"0.0349*12","v":0.41880000000000001},0,"S-P-08822","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened 15 mm",{"$f":"4.4*15","v":66},{"$f":"0.0454*15","v":0.68100000000000005},{"$f":"0.0545*15","v":0.8175},0,{"$f":"0.0787*15","v":1.1805000000000001},0,0,0,0,0,0,{"$f":"0.0208*15","v":0.312},0,{"$f":"0.0349*15","v":0.52349999999999997},0,"S-P-08822","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened offline coated 4 mm",{"$f":"4.28*4","v":17.12},{"$f":"0.0454*4","v":0.18160000000000001},{"$f":"0.0545*4","v":0.218},0,{"$f":"0.0787*4","v":0.31480000000000002},0,0,0,0,0,0,{"$f":"0.0208*4","v":8.3199999999999996E-2},0,{"$f":"0.00248*4","v":9.92E-3},0,"S-P-08824","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened offline coated 5 mm",{"$f":"4.28*5","v":21.400000000000002},{"$f":"0.0454*5","v":0.22700000000000001},{"$f":"0.0545*5","v":0.27250000000000002},0,{"$f":"0.0787*5","v":0.39350000000000002},0,0,0,0,0,0,{"$f":"0.0208*5","v":0.104},0,{"$f":"0.00248*5","v":1.24E-2},0,"S-P-08824","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened offline coated 6 mm",{"$f":"4.28*6","v":25.68},{"$f":"0.0454*6","v":0.27240000000000003},{"$f":"0.0545*6","v":0.32700000000000001},0,{"$f":"0.0787*6","v":0.47220000000000006},0,0,0,0,0,0,{"$f":"0.0208*6","v":0.12479999999999999},0,{"$f":"0.00248*6","v":1.4880000000000001E-2},0,"S-P-08824","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened offline coated 8 mm",{"$f":"4.28*8","v":34.24},{"$f":"0.0454*8","v":0.36320000000000002},{"$f":"0.0545*8","v":0.436},0,{"$f":"0.0787*8","v":0.62960000000000005},0,0,0,0,0,0,{"$f":"0.0208*8","v":0.16639999999999999},0,{"$f":"0.00248*8","v":1.984E-2},0,"S-P-08824","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened offline coated 10 mm",{"$f":"4.28*10","v":42.800000000000004},{"$f":"0.0454*10","v":0.45400000000000001},{"$f":"0.0545*10","v":0.54500000000000004},0,{"$f":"0.0787*10","v":0.78700000000000003},0,0,0,0,0,0,{"$f":"0.0208*10","v":0.20799999999999999},0,{"$f":"0.00248*10","v":2.4799999999999999E-2},0,"S-P-08824","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened offline coated 12 mm",{"$f":"4.28*12","v":51.36},{"$f":"0.0454*12","v":0.54480000000000006},{"$f":"0.0545*12","v":0.65400000000000003},0,{"$f":"0.0787*12","v":0.94440000000000013},0,0,0,0,0,0,{"$f":"0.0208*12","v":0.24959999999999999},0,{"$f":"0.00248*12","v":2.9760000000000002E-2},0,"S-P-08824","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened online coated 4 mm",{"$f":"5.67*4","v":22.68},{"$f":"0.0454*4","v":0.18160000000000001},{"$f":"0.0545*4","v":0.218},0,{"$f":"0.0787*4","v":0.31480000000000002},0,0,0,0,0,0,{"$f":"0.0208*4","v":8.3199999999999996E-2},0,{"$f":"0.00152*4","v":6.0800000000000003E-3},0,"S-P-08823","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened online coated 5 mm",{"$f":"5.67*5","v":28.35},{"$f":"0.0454*5","v":0.22700000000000001},{"$f":"0.0545*5","v":0.27250000000000002},0,{"$f":"0.0787*5","v":0.39350000000000002},0,0,0,0,0,0,{"$f":"0.0208*5","v":0.104},0,{"$f":"0.00152*5","v":7.6000000000000009E-3},0,"S-P-08823","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened online coated 6 mm",{"$f":"5.67*6","v":34.019999999999996},{"$f":"0.0454*6","v":0.27240000000000003},{"$f":"0.0545*6","v":0.32700000000000001},0,{"$f":"0.0787*6","v":0.47220000000000006},0,0,0,0,0,0,{"$f":"0.0208*6","v":0.12479999999999999},0,{"$f":"0.00152*6","v":9.1199999999999996E-3},0,"S-P-08823","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened online coated 8 mm",{"$f":"5.67*8","v":45.36},{"$f":"0.0454*8","v":0.36320000000000002},{"$f":"0.0545*8","v":0.436},0,{"$f":"0.0787*8","v":0.62960000000000005},0,0,0,0,0,0,{"$f":"0.0208*8","v":0.16639999999999999},0,{"$f":"0.00152*8","v":1.2160000000000001E-2},0,"S-P-08823","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened online coated 10 mm",{"$f":"5.67*10","v":56.7},{"$f":"0.0454*10","v":0.45400000000000001},{"$f":"0.0545*10","v":0.54500000000000004},0,{"$f":"0.0787*10","v":0.78700000000000003},0,0,0,0,0,0,{"$f":"0.0208*10","v":0.20799999999999999},0,{"$f":"0.00152*10","v":1.5200000000000002E-2},0,"S-P-08823","2028-04-30"]
[null,null,"Pilkington NSG","Optifloat","Monolithic toughened online coated 12 mm",{"$f":"5.67*12","v":68.039999999999992},{"$f":"0.0454*12","v":0.54480000000000006},{"$f":"0.0545*12","v":0.65400000000000003},0,{"$f":"0.0787*12","v":0.94440000000000013},0,0,0,0,0,0,{"$f":"0.0208*12","v":0.24959999999999999},0,{"$f":"0.00152*12","v":1.8239999999999999E-2},0,"S-P-08823","2028-04-30"]
[null,null,"Pilkington NSG","Optilam","Laminated 8.8 (44.2)",{"$f":"3.67*8.8","v":32.295999999999999},{"$f":"0.0436*8.8","v":0.38368000000000002},{"$f":"0.0545*8.8","v":0.47960000000000003},0,{"$f":"0.0787*8.8","v":0.69256000000000006},0,0,0,0,0,0,{"$f":"0.02*8.8","v":0.17600000000000002},0,{"$f":"0.055*8.8","v":0.48400000000000004},0,"S-P-08828","2028-04-30"]
[null,null,"Pilkington NSG","Optilam","Laminated 10.8 (55.2)",{"$f":"3.67*10.8","v":39.636000000000003},{"$f":"0.0436*10.8","v":0.47088000000000002},{"$f":"0.0545*10.8","v":0.58860000000000001},0,{"$f":"0.0787*10.8","v":0.84996000000000016},0,0,0,0,0,0,{"$f":"0.02*10.8","v":0.21600000000000003},0,{"$f":"0.055*10.8","v":0.59400000000000008},0,"S-P-08828","2028-04-30"]
[null,null,"Pilkington NSG","Optilam","Laminated 11.5 (55.4)",{"$f":"3.67*11.5","v":42.204999999999998},{"$f":"0.0436*11.5","v":0.50139999999999996},{"$f":"0.0545*11.5","v":0.62675000000000003},0,{"$f":"0.0787*11.5","v":0.90505000000000002},0,0,0,0,0,0,{"$f":"0.02*11.5","v":0.23},0,{"$f":"0.055*11.5","v":0.63249999999999995},0,"S-P-08828","2028-04-30"]
[null,null,"Pilkington NSG","Optilam","Laminated 12.8 (66.2)",{"$f":"3.67*12.8","v":46.975999999999999},{"$f":"0.0436*12.8","v":0.55808000000000002},{"$f":"0.0545*12.8","v":0.6976},0,{"$f":"0.0787*12.8","v":1.00736},0,0,0,0,0,0,{"$f":"0.02*12.8","v":0.25600000000000001},0,{"$f":"0.055*12.8","v":0.70400000000000007},0,"S-P-08828","2028-04-30"]
[null,null,"Pilkington NSG","Optilam","Laminated 13.5 (66.4)",{"$f":"3.67*13.5","v":49.545000000000002},{"$f":"0.0436*13.5","v":0.58860000000000001},{"$f":"0.0545*13.5","v":0.73575000000000002},0,{"$f":"0.0787*13.5","v":1.0624500000000001},0,0,0,0,0,0,{"$f":"0.02*13.5","v":0.27},0,{"$f":"0.055*13.5","v":0.74250000000000005},0,"S-P-08828","2028-04-30"]
[null,null,"Pilkington NSG","Optilam","Laminated offline coated 8.8 (44.2)",{"$f":"3.6*8.8","v":31.680000000000003},{"$f":"0.0436*8.8","v":0.38368000000000002},{"$f":"0.0545*8.8","v":0.47960000000000003},0,{"$f":"0.0787*8.8","v":0.69256000000000006},0,0,0,0,0,0,{"$f":"0.02*8.8","v":0.17600000000000002},0,{"$f":"0.038*8.8","v":0.33440000000000003},0,"S-P-08827","2028-04-30"]
[null,null,"Pilkington NSG","Optilam","Laminated offline coated 10.8 (55.2)",{"$f":"3.6*10.8","v":38.880000000000003},{"$f":"0.0436*10.8","v":0.47088000000000002},{"$f":"0.0545*10.8","v":0.58860000000000001},0,{"$f":"0.0787*10.8","v":0.84996000000000016},0,0,0,0,0,0,{"$f":"0.02*10.8","v":0.21600000000000003},0,{"$f":"0.038*10.8","v":0.41040000000000004},0,"S-P-08827","2028-04-30"]
[null,null,"Pilkington NSG","Optilam","Laminated offline coated 11.5 (55.4)",{"$f":"3.6*11.5","v":41.4},{"$f":"0.0436*11.5","v":0.50139999999999996},{"$f":"0.0545*11.5","v":0.62675000000000003},0,{"$f":"0.0787*11.5","v":0.90505000000000002},0,0,0,0,0,0,{"$f":"0.02*11.5","v":0.23},0,{"$f":"0.038*11.5","v":0.437},0,"S-P-08827","2028-04-30"]
[null,null,"Pilkington NSG","Optilam","Laminated offline coated 12.8 (66.2)",{"$f":"3.6*12.8","v":46.080000000000005},{"$f":"0.0436*12.8","v":0.55808000000000002},{"$f":"0.0545*12.8","v":0.6976},0,{"$f":"0.0787*12.8","v":1.00736},0,0,0,0,0,0,{"$f":"0.02*12.8","v":0.25600000000000001},0,{"$f":"0.038*12.8","v":0.4864},0,"S-P-08827","2028-04-30"]
[null,null,"Pilkington NSG","Optilam","Laminated offline coated 13.5 (66.4)",{"$f":"3.6*13.5","v":48.6},{"$f":"0.0436*13.5","v":0.58860000000000001},{"$f":"0.0545*13.5","v":0.73575000000000002},0,{"$f":"0.0787*13.5","v":1.0624500000000001},0,0,0,0,0,0,{"$f":"0.02*13.5","v":0.27},0,{"$f":"0.038*13.5","v":0.51300000000000001},0,"S-P-08827","2028-04-30"]
[null,null,"Pilkington NSG","Optilam","Laminated online coated 8.8 (44.2)",{"$f":"4.05*8.8","v":35.64},{"$f":"0.0436*8.8","v":0.38368000000000002},{"$f":"0.0545*8.8","v":0.47960000000000003},0,{"$f":"0.0787*8.8","v":0.69256000000000006},0,0,0,0,0,0,{"$f":"0.02*8.8","v":0.17600000000000002},0,{"$f":"0.035*8.8","v":0.30800000000000005},0,"S-P-08828","2028-04-30"]
[null,null,"Pilkington NSG","Optilam","Laminated online coated 10.8 (55.2)",{"$f":"4.05*10.8","v":43.74},{"$f":"0.0436*10.8","v":0.47088000000000002},{"$f":"0.0545*10.8","v":0.58860000000000001},0,{"$f":"0.0787*10.8","v":0.84996000000000016},0,0,0,0,0,0,{"$f":"0.02*10.8","v":0.21600000000000003},0,{"$f":"0.035*10.8","v":0.37800000000000006},0,"S-P-08828","2028-04-30"]
[null,null,"Pilkington NSG","Optilam","Laminated online coated 11.5 (55.4)",{"$f":"4.05*11.5","v":46.574999999999996},{"$f":"0.0436*11.5","v":0.50139999999999996},{"$f":"0.0545*11.5","v":0.62675000000000003},0,{"$f":"0.0787*11.5","v":0.90505000000000002},0,0,0,0,0,0,{"$f":"0.02*11.5","v":0.23},0,{"$f":"0.035*11.5","v":0.40250000000000002},0,"S-P-08828","2028-04-30"]
[null,null,"Pilkington NSG","Optilam","Laminated online coated 12.8 (66.2)",{"$f":"4.05*12.8","v":51.84},{"$f":"0.0436*12.8","v":0.55808000000000002},{"$f":"0.0545*12.8","v":0.6976},0,{"$f":"0.0787*12.8","v":1.00736},0,0,0,0,0,0,{"$f":"0.02*12.8","v":0.25600000000000001},0,{"$f":"0.035*12.8","v":0.44800000000000006},0,"S-P-08828","2028-04-30"]
[null,null,"Pilkington NSG","Optilam","Laminated online coated 13.5 (66.4)",{"$f":"4.05*13.5","v":54.674999999999997},{"$f":"0.0436*13.5","v":0.58860000000000001},{"$f":"0.0545*13.5","v":0.73575000000000002},0,{"$f":"0.0787*13.5","v":1.0624500000000001},0,0,0,0,0,0,{"$f":"0.02*13.5","v":0.27},0,{"$f":"0.035*13.5","v":0.47250000000000003},0,"S-P-08828","2028-04-30"]
[null,null,"Pilkington NSG","Optilam","Laminated toughened 8.8 (44.2)",36.299999999999997,0.36,{"$f":"0.00365","v":3.65E-3},0,0.121,0,0,0,0,0,0,0.17199999999999999,0,0.25900000000000001,0,"-IES-0017093","2029-12-10"]
[null,null,"Pilkington NSG","Optilam","Laminated 10.8 (55.2)",44.55,0.44180000000000003,4.4999999999999997E-3,0,0.14849999999999999,0,0,0,0,0,0,0.21099999999999999,0,0.31780000000000003,0,"-IES-0017093","2029-12-10"]
[null,null,"Pilkington NSG","Optilam","Laminated 11.5 (55.4)",47.4375,{"$f":"0.47","v":0.47},4.8300000000000001E-3,0,0.158,0,0,0,0,0,0,0.22470000000000001,0,0.33839999999999998,0,"-IES-0017093","2029-12-10"]
[null,null,"Pilkington NSG","Optilam","Laminated 12.8 (66.2)",52.8,{"$f":"0.5236","v":0.52359999999999995},5.3800000000000002E-3,0,0.17599999999999999,0,0,0,0,0,0,0.25009999999999999,0,0.37669999999999998,0,"-IES-0017093","2029-12-10"]
[null,null,"Pilkington NSG","Optilam","Laminated 13.5 (66.4)",55.6875,{"$f":"0.5523","v":0.55230000000000001},5.6699999999999997E-3,0,0.18559999999999999,0,0,0,0,0,0,0.26385999999999998,0,0.39729999999999999,0,"-IES-0017093","2029-12-10"]
[null,null,"Pilkington NSG","Optilam","Laminated 17.5 (88.4)",72.1875,{"$f":"0.7159","v":0.71589999999999998},7.3499999999999998E-3,0,0.24060000000000001,0,0,0,0,0,0,0.34200000000000003,0,0.51500000000000001,0,"-IES-0017093","2029-12-10"]
[null,null,"Pilkington NSG","Optilam","Laminated 21.5 (1010.4)",88.6875,{"$f":"0.8795","v":0.87949999999999995},9.0399999999999994E-3,0,0.29559999999999997,0,0,0,0,0,0,0.42020000000000002,0,0.63270000000000004,0,"-IES-0017093","2029-12-10"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic 2 mm (Low Iron)",{"$f":"2.92*2","v":5.84},{"$f":"0.0454*2","v":9.0800000000000006E-2},{"$f":"0.0545*2","v":0.109},0,{"$f":"0.0787*2","v":0.15740000000000001},0,0,0,0,0,0,{"$f":"0.0208*2","v":4.1599999999999998E-2},0,{"$f":"0.0235*2","v":4.7E-2},0,"S-P-08818","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic 3 mm (Low Iron)",{"$f":"2.92*3","v":8.76},{"$f":"0.0454*3","v":0.13620000000000002},{"$f":"0.0545*3","v":0.16350000000000001},0,{"$f":"0.0787*3","v":0.23610000000000003},0,0,0,0,0,0,{"$f":"0.0208*3","v":6.2399999999999997E-2},0,{"$f":"0.0235*3","v":7.0500000000000007E-2},0,"S-P-08818","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic 4 mm (Low Iron)",{"$f":"2.92*4","v":11.68},{"$f":"0.0454*4","v":0.18160000000000001},{"$f":"0.0545*4","v":0.218},0,{"$f":"0.0787*4","v":0.31480000000000002},0,0,0,0,0,0,{"$f":"0.0208*4","v":8.3199999999999996E-2},0,{"$f":"0.0235*4","v":9.4E-2},0,"S-P-08818","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic 5 mm (Low Iron)",{"$f":"2.92*5","v":14.6},{"$f":"0.0454*5","v":0.22700000000000001},{"$f":"0.0545*5","v":0.27250000000000002},0,{"$f":"0.0787*5","v":0.39350000000000002},0,0,0,0,0,0,{"$f":"0.0208*5","v":0.104},0,{"$f":"0.0235*5","v":0.11749999999999999},0,"S-P-08818","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic 6 mm (Low Iron)",{"$f":"2.92*6","v":17.52},{"$f":"0.0454*6","v":0.27240000000000003},{"$f":"0.0545*6","v":0.32700000000000001},0,{"$f":"0.0787*6","v":0.47220000000000006},0,0,0,0,0,0,{"$f":"0.0208*6","v":0.12479999999999999},0,{"$f":"0.0235*6","v":0.14100000000000001},0,"S-P-08818","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic 8 mm (Low Iron)",{"$f":"2.92*8","v":23.36},{"$f":"0.0454*8","v":0.36320000000000002},{"$f":"0.0545*8","v":0.436},0,{"$f":"0.0787*8","v":0.62960000000000005},0,0,0,0,0,0,{"$f":"0.0208*8","v":0.16639999999999999},0,{"$f":"0.0235*8","v":0.188},0,"S-P-08818","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic 10 mm (Low Iron)",{"$f":"2.92*10","v":29.2},{"$f":"0.0454*10","v":0.45400000000000001},{"$f":"0.0545*10","v":0.54500000000000004},0,{"$f":"0.0787*10","v":0.78700000000000003},0,0,0,0,0,0,{"$f":"0.0208*10","v":0.20799999999999999},0,{"$f":"0.0235*10","v":0.23499999999999999},0,"S-P-08818","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic 12 mm (Low Iron)",{"$f":"2.92*12","v":35.04},{"$f":"0.0454*12","v":0.54480000000000006},{"$f":"0.0545*12","v":0.65400000000000003},0,{"$f":"0.0787*12","v":0.94440000000000013},0,0,0,0,0,0,{"$f":"0.0208*12","v":0.24959999999999999},0,{"$f":"0.0235*12","v":0.28200000000000003},0,"S-P-08818","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic 15 mm (Low Iron)",{"$f":"2.92*15","v":43.8},{"$f":"0.0454*15","v":0.68100000000000005},{"$f":"0.0545*15","v":0.8175},0,{"$f":"0.0787*15","v":1.1805000000000001},0,0,0,0,0,0,{"$f":"0.0208*15","v":0.312},0,{"$f":"0.0235*15","v":0.35249999999999998},0,"S-P-08818","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic offline coated 3 mm (Low Iron)",{"$f":"3.3*3","v":9.8999999999999986},{"$f":"0.0454*3","v":0.13620000000000002},{"$f":"0.0545*3","v":0.16350000000000001},0,{"$f":"0.0787*3","v":0.23610000000000003},0,0,0,0,0,0,{"$f":"0.0208*3","v":6.2399999999999997E-2},0,{"$f":"0.0235*3","v":7.0500000000000007E-2},0,"S-P-08820","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic offline coated 4 mm (Low Iron)",{"$f":"3.3*4","v":13.2},{"$f":"0.0454*4","v":0.18160000000000001},{"$f":"0.0545*4","v":0.218},0,{"$f":"0.0787*4","v":0.31480000000000002},0,0,0,0,0,0,{"$f":"0.0208*4","v":8.3199999999999996E-2},0,{"$f":"0.0235*4","v":9.4E-2},0,"S-P-08820","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic offline coated 5 mm (Low Iron)",{"$f":"3.3*5","v":16.5},{"$f":"0.0454*5","v":0.22700000000000001},{"$f":"0.0545*5","v":0.27250000000000002},0,{"$f":"0.0787*5","v":0.39350000000000002},0,0,0,0,0,0,{"$f":"0.0208*5","v":0.104},0,{"$f":"0.0235*5","v":0.11749999999999999},0,"S-P-08820","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic offline coated 6 mm (Low Iron)",{"$f":"3.3*6","v":19.799999999999997},{"$f":"0.0454*6","v":0.27240000000000003},{"$f":"0.0545*6","v":0.32700000000000001},0,{"$f":"0.0787*6","v":0.47220000000000006},0,0,0,0,0,0,{"$f":"0.0208*6","v":0.12479999999999999},0,{"$f":"0.0235*6","v":0.14100000000000001},0,"S-P-08820","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic offline coated 8 mm (Low Iron)",{"$f":"3.3*8","v":26.4},{"$f":"0.0454*8","v":0.36320000000000002},{"$f":"0.0545*8","v":0.436},0,{"$f":"0.0787*8","v":0.62960000000000005},0,0,0,0,0,0,{"$f":"0.0208*8","v":0.16639999999999999},0,{"$f":"0.0235*8","v":0.188},0,"S-P-08820","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic offline coated 10 mm (Low Iron)",{"$f":"3.3*10","v":33},{"$f":"0.0454*10","v":0.45400000000000001},{"$f":"0.0545*10","v":0.54500000000000004},0,{"$f":"0.0787*10","v":0.78700000000000003},0,0,0,0,0,0,{"$f":"0.0208*10","v":0.20799999999999999},0,{"$f":"0.0235*10","v":0.23499999999999999},0,"S-P-08820","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic offline coated 12 mm (Low Iron)",{"$f":"3.3*12","v":39.599999999999994},{"$f":"0.0454*12","v":0.54480000000000006},{"$f":"0.0545*12","v":0.65400000000000003},0,{"$f":"0.0787*12","v":0.94440000000000013},0,0,0,0,0,0,{"$f":"0.0208*12","v":0.24959999999999999},0,{"$f":"0.0235*12","v":0.28200000000000003},0,"S-P-08820","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic toughened 4 mm (Low Iron)",{"$f":"4.4*4","v":17.600000000000001},{"$f":"0.0454*4","v":0.18160000000000001},{"$f":"0.0545*4","v":0.218},0,{"$f":"0.0787*4","v":0.31480000000000002},0,0,0,0,0,0,{"$f":"0.0208*4","v":8.3199999999999996E-2},0,{"$f":"0.0349*4","v":0.1396},0,"S-P-08822","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic toughened 5 mm (Low Iron)",{"$f":"4.4*5","v":22},{"$f":"0.0454*5","v":0.22700000000000001},{"$f":"0.0545*5","v":0.27250000000000002},0,{"$f":"0.0787*5","v":0.39350000000000002},0,0,0,0,0,0,{"$f":"0.0208*5","v":0.104},0,{"$f":"0.0349*5","v":0.17449999999999999},0,"S-P-08822","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic toughened 6 mm (Low Iron)",{"$f":"4.4*6","v":26.400000000000002},{"$f":"0.0454*6","v":0.27240000000000003},{"$f":"0.0545*6","v":0.32700000000000001},0,{"$f":"0.0787*6","v":0.47220000000000006},0,0,0,0,0,0,{"$f":"0.0208*6","v":0.12479999999999999},0,{"$f":"0.0349*6","v":0.2094},0,"S-P-08822","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic toughened 8 mm (Low Iron)",{"$f":"4.4*8","v":35.200000000000003},{"$f":"0.0454*8","v":0.36320000000000002},{"$f":"0.0545*8","v":0.436},0,{"$f":"0.0787*8","v":0.62960000000000005},0,0,0,0,0,0,{"$f":"0.0208*8","v":0.16639999999999999},0,{"$f":"0.0349*8","v":0.2792},0,"S-P-08822","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic toughened 10 mm (Low Iron)",{"$f":"4.4*10","v":44},{"$f":"0.0454*10","v":0.45400000000000001},{"$f":"0.0545*10","v":0.54500000000000004},0,{"$f":"0.0787*10","v":0.78700000000000003},0,0,0,0,0,0,{"$f":"0.0208*10","v":0.20799999999999999},0,{"$f":"0.0349*10","v":0.34899999999999998},0,"S-P-08822","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic toughened 12 mm (Low Iron)",{"$f":"4.4*12","v":52.800000000000004},{"$f":"0.0454*12","v":0.54480000000000006},{"$f":"0.0545*12","v":0.65400000000000003},0,{"$f":"0.0787*12","v":0.94440000000000013},0,0,0,0,0,0,{"$f":"0.0208*12","v":0.24959999999999999},0,{"$f":"0.0349*12","v":0.41880000000000001},0,"S-P-08822","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic toughened 15 mm (Low Iron)",{"$f":"4.4*15","v":66},{"$f":"0.0454*15","v":0.68100000000000005},{"$f":"0.0545*15","v":0.8175},0,{"$f":"0.0787*15","v":1.1805000000000001},0,0,0,0,0,0,{"$f":"0.0208*15","v":0.312},0,{"$f":"0.0349*15","v":0.52349999999999997},0,"S-P-08822","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic toughened offline coated 4 mm (Low Iron)",{"$f":"4.84*4","v":19.36},{"$f":"0.0454*4","v":0.18160000000000001},{"$f":"0.0545*4","v":0.218},0,{"$f":"0.0787*4","v":0.31480000000000002},0,0,0,0,0,0,{"$f":"0.0208*4","v":8.3199999999999996E-2},0,{"$f":"0.00248*4","v":9.92E-3},0,"S-P-08825","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic toughened offline coated 5 mm (Low Iron)",{"$f":"4.84*5","v":24.2},{"$f":"0.0454*5","v":0.22700000000000001},{"$f":"0.0545*5","v":0.27250000000000002},0,{"$f":"0.0787*5","v":0.39350000000000002},0,0,0,0,0,0,{"$f":"0.0208*5","v":0.104},0,{"$f":"0.00248*5","v":1.24E-2},0,"S-P-08825","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic toughened offline coated 6 mm (Low Iron)",{"$f":"4.84*6","v":29.04},{"$f":"0.0454*6","v":0.27240000000000003},{"$f":"0.0545*6","v":0.32700000000000001},0,{"$f":"0.0787*6","v":0.47220000000000006},0,0,0,0,0,0,{"$f":"0.0208*6","v":0.12479999999999999},0,{"$f":"0.00248*6","v":1.4880000000000001E-2},0,"S-P-08825","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic toughened offline coated 8 mm (Low Iron)",{"$f":"4.84*8","v":38.72},{"$f":"0.0454*8","v":0.36320000000000002},{"$f":"0.0545*8","v":0.436},0,{"$f":"0.0787*8","v":0.62960000000000005},0,0,0,0,0,0,{"$f":"0.0208*8","v":0.16639999999999999},0,{"$f":"0.00248*8","v":1.984E-2},0,"S-P-08825","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic toughened offline coated 10 mm (Low Iron)",{"$f":"4.84*10","v":48.4},{"$f":"0.0454*10","v":0.45400000000000001},{"$f":"0.0545*10","v":0.54500000000000004},0,{"$f":"0.0787*10","v":0.78700000000000003},0,0,0,0,0,0,{"$f":"0.0208*10","v":0.20799999999999999},0,{"$f":"0.00248*10","v":2.4799999999999999E-2},0,"S-P-08825","2028-04-30"]
[null,null,"Pilkington NSG","Optiwhite","Monolithic toughened offline coated 12 mm (Low Iron)",{"$f":"4.84*12","v":58.08},{"$f":"0.0454*12","v":0.54480000000000006},{"$f":"0.0545*12","v":0.65400000000000003},0,{"$f":"0.0787*12","v":0.94440000000000013},0,0,0,0,0,0,{"$f":"0.0208*12","v":0.24959999999999999},0,{"$f":"0.00248*12","v":2.9760000000000002E-2},0,"S-P-08825","2028-04-30"]
[null,null,"Pilkington NSG","Patterned","Monolithic 4 mm",{"$f":"4.4*4","v":17.600000000000001},{"$f":"0.0454*4","v":0.18160000000000001},{"$f":"0.0545*4","v":0.218},0,{"$f":"0.0787*4","v":0.31480000000000002},0,0,0,0,0,0,{"$f":"0.0208*4","v":8.3199999999999996E-2},0,{"$f":"0.0235*4","v":9.4E-2},0,"S-P-08817","2028-04-30"]
[null,null,"Pilkington NSG","Patterned","Monolithic 5 mm",{"$f":"4.4*5","v":22},{"$f":"0.0454*5","v":0.22700000000000001},{"$f":"0.0545*5","v":0.27250000000000002},0,{"$f":"0.0787*5","v":0.39350000000000002},0,0,0,0,0,0,{"$f":"0.0208*5","v":0.104},0,{"$f":"0.0235*5","v":0.11749999999999999},0,"S-P-08817","2028-04-30"]
[null,null,"Pilkington NSG","Patterned","Monolithic 6 mm",{"$f":"4.4*6","v":26.400000000000002},{"$f":"0.0454*6","v":0.27240000000000003},{"$f":"0.0545*6","v":0.32700000000000001},0,{"$f":"0.0787*6","v":0.47220000000000006},0,0,0,0,0,0,{"$f":"0.0208*6","v":0.12479999999999999},0,{"$f":"0.0235*6","v":0.14100000000000001},0,"S-P-08817","2028-04-30"]
[null,null,"Pilkington NSG","Patterned","Monolithic 8 mm",{"$f":"4.4*8","v":35.200000000000003},{"$f":"0.0454*8","v":0.36320000000000002},{"$f":"0.0545*8","v":0.436},0,{"$f":"0.0787*8","v":0.62960000000000005},0,0,0,0,0,0,{"$f":"0.0208*8","v":0.16639999999999999},0,{"$f":"0.0235*8","v":0.188},0,"S-P-08817","2028-04-30"]
[null,null,"Pilkington NSG","Patterned","Monolithic 10 mm",{"$f":"4.4*10","v":44},{"$f":"0.0454*10","v":0.45400000000000001},{"$f":"0.0545*10","v":0.54500000000000004},0,{"$f":"0.0787*10","v":0.78700000000000003},0,0,0,0,0,0,{"$f":"0.0208*10","v":0.20799999999999999},0,{"$f":"0.0235*10","v":0.23499999999999999},0,"S-P-08817","2028-04-30"]
[]
[null,null,"Saint Gobain","ORAE Low carbon","Monolithic 2 mm",2.94,0.19600000000000001,0,0,0.184,0,0,0,0,0,0,1.2200000000000001E-2,0,8.4000000000000005E-2,0,"S-P-09498","2028-12-20"]
[null,null,"Saint Gobain","ORAE Low carbon","Monolithic 3 mm",4.41,0.29399999999999998,0,0,0.184,0,0,0,0,0,0,1.83E-2,0,0.122,0,"S-P-09497","2028-12-20"]
[null,null,"Saint Gobain","ORAE Low carbon","Monolithic 4 mm",5.88,0.39200000000000002,0,0,0.184,0,0,0,0,0,0,2.4400000000000002E-2,0,0.16,0,"S-P-08970","2028-04-13"]
[null,null,"Saint Gobain","ORAE Low carbon","Monolithic  5 mm",7.35,0.49,0,0,0.184,0,0,0,0,0,0,3.0499999999999999E-2,0,0.19900000000000001,0,"S-P-09496","2028-12-20"]
[null,null,"Saint Gobain","ORAE Low carbon","Monolithic  6 mm",8.82,0.58799999999999997,0,0,0.184,0,0,0,0,0,0,3.6600000000000001E-2,0,0.23699999999999999,0,"S-P-09495","2028-12-20"]
[null,null,"Saint Gobain","ORAE Low carbon","Monolithic  8 mm",11.8,0.78400000000000003,0,0,0.184,0,0,0,0,0,0,4.8800000000000003E-2,0,0.312,0,"S-P-09502","2028-12-20"]
[null,null,"Saint Gobain","ORAE Low carbon","Monolithic  10 mm",14.7,0.98,0,0,0.184,0,0,0,0,0,0,6.0999999999999999E-2,0,0.38800000000000001,0,"S-P-09494","2028-12-20"]
[null,null,"Saint Gobain","ORAE Low carbon","Monolithic magnetron-coated 4 mm",6.26,0.39200000000000002,0,0,0.184,0,0,0,0,0,0,2.4400000000000002E-2,0,0.16,0,"S-P-09012","2028-04-13"]
[null,null,"Saint Gobain","ORAE Low carbon","Monolithic magnetron-coated 6 mm",9.2100000000000009,0.58799999999999997,0,0,0.184,0,0,0,0,0,0,3.6600000000000001E-2,0,0.24,0,"S-P-09013","2028-04-13"]
[null,null,"Saint Gobain","ORAE Low carbon","Monolithic magnetron-coated 8 mm",12.1,0.78400000000000003,0,0,0.184,0,0,0,0,0,0,4.8800000000000003E-2,0,0.32,0,"S-P-09014","2028-04-13"]
[null,null,"Saint Gobain","ORAE Low carbon","Monolithic magnetron-coated 10 mm",15.1,0.98,0,0,0.184,0,0,0,0,0,0,6.0999999999999999E-2,0,0.4,0,"S-P-09015","2028-04-13"]
[null,null,"Saint Gobain","ORAE Low carbon","Laminated 8.4 mm (44.1) (STADIP)",16.8,0.624,0,0,0.14499999999999999,0,0,0,0,0,0,6.1499999999999999E-2,0,0.32800000000000001,0,"EPD-IES-0024289","2030-06-11"]
[null,null,"Saint Gobain","ORAE Low carbon","Laminated 8.8 mm (44.2) (STADIP)",16.8,6.2399999999999997E-2,0,0,1.4500000000000001E-2,0,0,0,0,0,0,6.1500000000000001E-3,0,3.2800000000000003E-2,0,"EPD-IES-0024289","2030-06-11"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic 2 mm",5.45,0.17100000000000001,0,0,9.5000000000000001E-2,0,0,0,0,0,0,1.2200000000000001E-2,0,7.0000000000000007E-2,0,"S-P-00882","2026-09-29"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic Clear 3 mm",8.17,0.25600000000000001,0,0,9.5000000000000001E-2,0,0,0,0,0,0,1.83E-2,0,0.105,0,"S-P-00882","2026-09-29"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic Clear 4 mm",10.9,0.34200000000000003,0,0,9.5000000000000001E-2,0,0,0,0,0,0,2.4400000000000002E-2,0,0.14000000000000001,0,"S-P-00882","2026-09-29"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic Clear 5 mm",13.6,0.42699999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.0499999999999999E-2,0,0.17499999999999999,0,"S-P-00882","2026-09-29"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic Clear 6 mm",16.3,0.51200000000000001,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.6600000000000001E-2,0,0.21,0,"S-P-00882","2026-09-29"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic Clear 8 mm",21.8,0.68300000000000005,0,0,9.5000000000000001E-2,0,0,0,0,0,0,4.8800000000000003E-2,0,0.28000000000000003,0,"S-P-00882","2026-09-29"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic Clear 10 mm",27.2,0.85399999999999998,0,0,9.5000000000000001E-2,0,0,0,0,0,0,6.0999999999999999E-2,0,0.35,0,"S-P-00882","2026-09-29"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic Clear 12 mm",32.700000000000003,1.02,0,0,9.5000000000000001E-2,0,0,0,0,0,0,7.3200000000000001E-2,0,0.42,0,"S-P-00882","2026-09-29"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic Clear 15 mm",40.9,1.28,0,0,9.5000000000000001E-2,0,0,0,0,0,0,9.1499999999999998E-2,0,0.52500000000000002,0,"S-P-00882","2026-09-29"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic Clear 19 mm",51.8,1.62,0,0,9.5000000000000001E-2,0,0,0,0,0,0,0.11600000000000001,0,0.66500000000000004,0,"S-P-00882","2026-09-29"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic magnetron coated 3mm",9.1999999999999993,0.183,0,0,9.5000000000000001E-2,0,0,0,0,0,0,1.83E-2,0,0.105,0,"S-P-00926","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic magnetron coated 4 mm",11.9,0.24399999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,2.4400000000000002E-2,0,0.14000000000000001,0,"S-P-00926","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic magnetron coated 5 mm",14.7,0.30499999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.0499999999999999E-2,0,0.17499999999999999,0,"S-P-00926","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic magnetron coated 6 mm",17.399999999999999,0.36599999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.6600000000000001E-2,0,0.21,0,"S-P-00926","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic magnetron coated 8 mm",22.8,0.48799999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,4.8800000000000003E-2,0,0.28000000000000003,0,"S-P-00926","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic magnetron coated 10 mm",28.3,0.61,0,0,9.5000000000000001E-2,0,0,0,0,0,0,6.0999999999999999E-2,0,0.35,0,"S-P-00926","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic magnetron coated 12 mm",33.700000000000003,0.73199999999999998,0,0,9.5000000000000001E-2,0,0,0,0,0,0,7.3200000000000001E-2,0,0.42,0,"S-P-00926","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic toughened 2 mm (SECURIT)",9.31,0.122,0,0,9.5000000000000001E-2,0,0,0,0,0,0,1.2200000000000001E-2,0,7.0000000000000007E-2,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic toughened 3 mm (SECURIT)",12.4,0.183,0,0,9.5000000000000001E-2,0,0,0,0,0,0,1.83E-2,0,0.105,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic toughened 4 mm (SECURIT)",15.5,0.24399999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,2.4400000000000002E-2,0,0.14000000000000001,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic toughened  5 mm (SECURIT)",18.600000000000001,0.30499999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.0499999999999999E-2,0,0.17499999999999999,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic toughened 6 mm (SECURIT)",21.7,0.36599999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.6600000000000001E-2,0,0.21,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic toughened 8 mm (SECURIT)",27.9,0.48799999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,4.8800000000000003E-2,0,0.28000000000000003,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic toughened 10 mm (SECURIT)",34.200000000000003,0.61,0,0,9.5000000000000001E-2,0,0,0,0,0,0,6.0999999999999999E-2,0,0.35,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic toughened 12 mm (SECURIT)",40.4,0.73199999999999998,0,0,9.5000000000000001E-2,0,0,0,0,0,0,7.3200000000000001E-2,0,0.42,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic toughened 15 mm (SECURIT)",49.7,0.91500000000000004,0,0,9.5000000000000001E-2,0,0,0,0,0,0,9.1499999999999998E-2,0,0.52500000000000002,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic toughened 19 mm (SECURIT)",62.1,1.1599999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,0.11600000000000001,0,0.66500000000000004,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic mirror 3 mm (MIRALITE PURE)",10.3,"-",0,0,0,0,0,0,0,0,0,0,0,0,0,"S-P-01744","2025-04-27"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic mirror 4 mm (MIRALITE PURE)",13,"-",0,0,0,0,0,0,0,0,0,0,0,0,0,"S-P-01744","2025-04-27"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic mirror 5 mm (MIRALITE PURE)",15.7,"-",0,0,0,0,0,0,0,0,0,0,0,0,0,"S-P-01744","2025-04-27"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic mirror 6 mm (MIRALITE PURE)",18.399999999999999,"-",0,0,0,0,0,0,0,0,0,0,0,0,0,"S-P-01744","2025-04-27"]
[null,null,"Saint Gobain","PLANICLEAR 1","Monolithic mirror 8 mm (MIRALITE PURE)",23.8,"-",0,0,0,0,0,0,0,0,0,0,0,0,0,"S-P-01744","2025-04-27"]
[null,null,"Saint Gobain","DIAMANT","Monolithic 3 mm",8.6199999999999992,0.36599999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,1.83E-2,0,0.105,0,"S-P-00883","2026-09-29"]
[null,null,"Saint Gobain","DIAMANT","Monolithic 4 mm",11.5,0.48799999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,2.4400000000000002E-2,0,0.14000000000000001,0,"S-P-00883","2026-09-29"]
[null,null,"Saint Gobain","DIAMANT","Monolithic 5 mm",14.4,0.61,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.0499999999999999E-2,0,0.17499999999999999,0,"S-P-00883","2026-09-29"]
[null,null,"Saint Gobain","DIAMANT","Monolithic 6 mm",17.2,0.73199999999999998,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.6600000000000001E-2,0,0.21,0,"S-P-00883","2026-09-29"]
[null,null,"Saint Gobain","DIAMANT","Monolithic 8 mm",23,0.97599999999999998,0,0,9.5000000000000001E-2,0,0,0,0,0,0,4.8800000000000003E-2,0,0.28000000000000003,0,"S-P-00883","2026-09-29"]
[null,null,"Saint Gobain","DIAMANT","Monolithic 10 mm",28.7,1.22,0,0,9.5000000000000001E-2,0,0,0,0,0,0,6.0999999999999999E-2,0,0.35,0,"S-P-00883","2026-09-29"]
[null,null,"Saint Gobain","DIAMANT","Monolithic 12 mm",34.5,1.46,0,0,9.5000000000000001E-2,0,0,0,0,0,0,7.3200000000000001E-2,0,0.42,0,"S-P-00883","2026-09-29"]
[null,null,"Saint Gobain","DIAMANT","Monolithic 15 mm",43.1,1.83,0,0,9.5000000000000001E-2,0,0,0,0,0,0,9.1499999999999998E-2,0,0.52500000000000002,0,"S-P-00883","2026-09-29"]
[null,null,"Saint Gobain","DIAMANT","Monolithic 19 mm",54.6,2.3199999999999998,0,0,9.5000000000000001E-2,0,0,0,0,0,0,0.11600000000000001,0,0.66500000000000004,0,"S-P-00883","2026-09-29"]
[null,null,"Saint Gobain","DIAMANT","Monolithic magnetron coated 3 mm",9.84,0.183,0,0,9.5000000000000001E-2,0,0,0,0,0,0,1.83E-2,0,0.105,0,"S-P-00926","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Monolithic magnetron coated 4 mm",12.7,0.24399999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,2.4400000000000002E-2,0,0.14000000000000001,0,"S-P-00926","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Monolithic magnetron  coated 5 mm",15.6,0.30499999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.0499999999999999E-2,0,0.17499999999999999,0,"S-P-00926","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Monolithic magnetron coated 6 mm",18.399999999999999,0.36599999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.6600000000000001E-2,0,0.21,0,"S-P-00926","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Monolithic magnetron coated 8 mm",24.2,0.48799999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,4.8800000000000003E-2,0,0.28000000000000003,0,"S-P-00926","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Monolithic magnetron coated 10 mm",29.9,0.61,0,0,9.5000000000000001E-2,0,0,0,0,0,0,6.0999999999999999E-2,0,0.35,0,"S-P-00926","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Monolithic magnetron coated 12 mm",35.700000000000003,0.73199999999999998,0,0,9.5000000000000001E-2,0,0,0,0,0,0,7.3200000000000001E-2,0,0.42,0,"S-P-00926","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Monolithic toughened 2 mm",9.66,0.122,0,0,9.5000000000000001E-2,0,0,0,0,0,0,1.2200000000000001E-2,0,7.0000000000000007E-2,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Monolithic toughened 3 mm",12.9,0.183,0,0,9.5000000000000001E-2,0,0,0,0,0,0,1.83E-2,0,0.105,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Monolithic toughened 4 mm",16.2,0.24399999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,2.4400000000000002E-2,0,0.14000000000000001,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Monolithic toughened 5 mm",19.5,0.30499999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.0499999999999999E-2,0,0.17499999999999999,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Monolithic toughened 6 mm",22.8,0.36599999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.6600000000000001E-2,0,0.21,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Monolithic toughened 8 mm",29.3,0.48799999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,4.8800000000000003E-2,0,0.28000000000000003,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Monolithic toughened 10 mm",35.799999999999997,0.61,0,0,9.5000000000000001E-2,0,0,0,0,0,0,6.0999999999999999E-2,0,0.35,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Monolithic toughened 12 mm",42.4,0.73199999999999998,0,0,9.5000000000000001E-2,0,0,0,0,0,0,7.3200000000000001E-2,0,0.42,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Monolithic toughened 15 mm",52.2,0.91500000000000004,0,0,9.5000000000000001E-2,0,0,0,0,0,0,9.1499999999999998E-2,0,0.52500000000000002,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Monolithic toughened 19 mm",65.3,1.1599999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,0.11600000000000001,0,0.66500000000000004,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Laminated 10.8 mm (55.2) STADIP (SILENCE) PROTECT",35.5,0.63,0,0,9.5000000000000001E-2,0,0,0,0,0,0,6.3E-2,0,0.36199999999999999,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","DIAMANT","Laminated 12.8 mm (66.2) STADIP (SILENCE) PROTECT ",41.2,0.752,0,0,9.5000000000000001E-2,0,0,0,0,0,0,7.5200000000000003E-2,0,0.432,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","STADIP","Laminated 4.4 mm (22.1) (SILENCE) ",14.7,0.254,0,0,9.5000000000000001E-2,0,0,0,0,0,0,2.5399999999999999E-2,0,0.14599999999999999,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","STADIP","Laminated 6.4 mm (33.1) (SILENCE)",20.2,0.376,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.7600000000000001E-2,0,0.216,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","STADIP","Laminated 8.4 mm (44.1) (SILENCE)",25.6,0.498,0,0,9.5000000000000001E-2,0,0,0,0,0,0,4.9799999999999997E-2,0,0.28599999999999998,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","STADIP","Laminated 6.8 mm (33.2) (SILENCE) PROTECT ",23.1,0.38600000000000001,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.8600000000000002E-2,0,0.222,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","STADIP","Laminated 8.8 mm (44.2) (SILENCE) PROTECT ",28.6,0.50800000000000001,0,0,9.5000000000000001E-2,0,0,0,0,0,0,5.0799999999999998E-2,0,0.29199999999999998,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","STADIP","Laminated 9.2 mm (44.4)  (SILENCE) PROTECT ",34.6,0.52800000000000002,0,0,9.5000000000000001E-2,0,0,0,0,0,0,5.28E-2,0,0.30299999999999999,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","STADIP","Laminated 10.2 mm (44.6) (SILENCE) PROTECT ",40.5,0.54800000000000004,0,0,9.5000000000000001E-2,0,0,0,0,0,0,5.4800000000000001E-2,0,0.314,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","STADIP","Laminated 10.8 mm (55.2) (SILENCE) PROTECT ",34,0.63,0,0,9.5000000000000001E-2,0,0,0,0,0,0,6.3E-2,0,0.36199999999999999,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","STADIP","Laminated 12.8 mm (66.2) (SILENCE) PROTECT ",39.5,0.752,0,0,9.5000000000000001E-2,0,0,0,0,0,0,7.5200000000000003E-2,0,0.432,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","STADIP","Laminated 16.8 mm (88.2) (SILENCE) PROTECT ",50.3,0.996,0,0,9.5000000000000001E-2,0,0,0,0,0,0,9.9599999999999994E-2,0,0.57199999999999995,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","STADIP","Laminated 20.8 mm (1010.2) (SILENCE) PROTECT ",61.2,1.24,0,0,9.5000000000000001E-2,0,0,0,0,0,0,0.124,0,0.71199999999999997,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","STADIP","Laminated 4.8 mm (22.2) XN  (SILENCE) PROTECT ",18.7,0.26400000000000001,0,0,9.5000000000000001E-2,0,0,0,0,0,0,2.64E-2,0,0.151,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","STADIP","Laminated 6.4 mm (33.1) XN (SILENCE) PROTECT ",21.2,0.376,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.7600000000000001E-2,0,0.216,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","STADIP","Laminated 8.8 mm (44.2) XN (SILENCE) PROTECT ",29.6,0.50800000000000001,0,0,9.5000000000000001E-2,0,0,0,0,0,0,5.0799999999999998E-2,0,0.29199999999999998,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","STADIP","Laminated 9.2 mm (44.4) XN (SILENCE) PROTECT ",35.6,0.52800000000000002,0,0,9.5000000000000001E-2,0,0,0,0,0,0,5.28E-2,0,0.30299999999999999,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","STADIP","Laminated 10.2 mm (44.6) XN (SILENCE) PROTECT ",41.6,0.54800000000000004,0,0,9.5000000000000001E-2,0,0,0,0,0,0,5.4800000000000001E-2,0,0.314,0,"S-P-00930","2026-12-14"]
[null,null,"Saint Gobain","PARSOL","Monolithic tinted 3 mm PARSOL",7.17,0.73199999999999998,0,0,9.5000000000000001E-2,0,0,0,0,0,0,1.83E-2,0,0.105,0,"S-P-00884","2026-09-29"]
[null,null,"Saint Gobain","PARSOL","Monolithic tinted 4 mm PARSOL ",9.56,0.97599999999999998,0,0,9.5000000000000001E-2,0,0,0,0,0,0,2.4400000000000002E-2,0,0.14000000000000001,0,"S-P-00884","2026-09-29"]
[null,null,"Saint Gobain","PARSOL","Monolithic tinted 5 mm PARSOL ",11.9,1.22,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.0499999999999999E-2,0,0.17499999999999999,0,"S-P-00884","2026-09-29"]
[null,null,"Saint Gobain","PARSOL","Monolithic tinted 6 mm PARSOL ",14.3,1.46,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.6600000000000001E-2,0,0.21,0,"S-P-00884","2026-09-29"]
[null,null,"Saint Gobain","PARSOL","Monolithic  tinted 8 mm PARSOL ",19.100000000000001,1.95,0,0,9.5000000000000001E-2,0,0,0,0,0,0,4.8800000000000003E-2,0,0.28000000000000003,0,"S-P-00884","2026-09-29"]
[null,null,"Saint Gobain","PARSOL","Monolithic tinted 10 mm PARSOL ",23.9,2.44,0,0,9.5000000000000001E-2,0,0,0,0,0,0,6.0999999999999999E-2,0,0.35,0,"S-P-00884","2026-09-29"]
[null,null,"Saint Gobain","PARSOL","Monolithic toughened tinted 2 mm PARSOL ",8.69,0.122,0,0,9.5000000000000001E-2,0,0,0,0,0,0,1.2200000000000001E-2,0,7.0000000000000007E-2,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","PARSOL","Monolithic toughened tinted 3 mm PARSOL ",11.4,0.183,0,0,9.5000000000000001E-2,0,0,0,0,0,0,1.83E-2,0,0.105,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","PARSOL","Monolithic toughened tinted 4 mm PARSOL ",14.1,0.24399999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,2.4400000000000002E-2,0,0.14000000000000001,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","PARSOL","Monolithic toughened tinted 5 mm PARSOL ",16.899999999999999,0.30499999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.0499999999999999E-2,0,0.17499999999999999,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","PARSOL","Monolithic toughened tinted 6 mm PARSOL ",19.600000000000001,0.36599999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,3.6600000000000001E-2,0,0.21,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","PARSOL","Monolithic toughened tinted 8 mm PARSOL ",25,0.48799999999999999,0,0,9.5000000000000001E-2,0,0,0,0,0,0,4.8800000000000003E-2,0,0.28000000000000003,0,"S-P-00927","2026-12-14"]
[null,null,"Saint Gobain","PARSOL","Monolithic toughened tinted 10 mm PARSOL ",30.5,0.61,0,0,9.5000000000000001E-2,0,0,0,0,0,0,6.0999999999999999E-2,0,0.35,0,"S-P-00927","2026-12-14"]
[]
[null,null,"Fire rated glass","AGC Pyrobel T","EW30-16, thickness 16 mm",69.319999999999993,1.55,-3.3,0,0.02,0,0,0,0,0,0,0.14499999999999999,0,0.54300000000000004,-1.35,"EPD-AGC-20240539-IBH1-EN","2030-06-24"]
[null,null,"Fire rated glass","AGC Pyrobel T ","EW30-20, thickness 20 mm",86.65,1.94,-4.12,0,0.02,0,0,0,0,0,0,0.16300000000000001,0,0.61099999999999999,-1.52,"EPD-AGC-20240539-IBH1-EN","2030-06-24"]
[null,null,"Fire rated glass","AGC Pyrobel T","EI30-18, thickness 18 mm",77.989999999999995,1.74,-3.71,0,0.02,0,0,0,0,0,0,0.18099999999999999,0,0.67800000000000005,-1.69,"EPD-AGC-20240539-IBH1-EN","2030-06-24"]
[null,null,"Fire rated glass","AGC Pyrobel T ","EI30-22 thickness 22 mm",95.32,2.13,-4.53,0,0.02,0,0,0,0,0,0,0.19900000000000001,0,0.747,-1.86,"EPD-AGC-20240539-IBH1-EN","2030-06-24"]
[null,null,"Fire rated glass","AGC Pyrobel T ","EI30-27 thickness 27 mm",116.98,2.61,-5.56,0,0.03,0,0,0,0,0,0,0.245,0,0.91700000000000004,-2.2799999999999998,"EPD-AGC-20240539-IBH1-EN","2030-06-24"]
[null,null,"Fire rated glass","AGC Pyrobel T ","EI60-28 thickness 28 mm",121.31,2.71,-5.77,0,0.03,0,0,0,0,0,0,0.254,0,0.95099999999999996,-2.36,"EPD-AGC-20240539-IBH1-EN","2030-06-24"]
[null,null,"Fire rated glass","AGC Pyrobel T ","EI60-34 thickness 34 mm",147.31,3.29,-7.01,0,0.04,0,0,0,0,0,0,0.308,0,1.1559999999999999,-2.87,"EPD-AGC-20240539-IBH1-EN","2030-06-24"]
[null,null,"Fire rated glass","AGC Pyrobel T ","EI30-37 thickness 37 mm",160.30000000000001,3.58,-7.63,0,0.04,0,0,0,0,0,0,0.33500000000000002,0,1.258,-3.12,"EPD-AGC-20240539-IBH1-EN","2030-06-24"]
[null,null,"Fire rated glass","POLFLAM","POLFLAM - EI, EW, FR, thickness 16 to 20 mm",61,6.6600000000000006E-2,0,0,0,0,0,0,0,0,0,0.61399999999999999,1.33,3.1E-2,0.84,"Date of issue  28/11/2024","2029-11-28"]
[null,null,"Fire rated glass","POLFLAM","POLFLAM - EI, EW, FR, thickness 21 to 55 mm",69.3,6.6000000000000003E-2,0,0,0,0,0,0,0,0,0,0.622,1.35,0.03,-1.1000000000000001,"Date of issue  28/11/2024","2029-11-28"]
[null,null,"Fire rated glass","POLFLAM","POLFLAM - BR, thickness 30 to 50 mm",95.5,6.6600000000000006E-2,0,0,0,0,0,0,0,0,0,1.22,2.65,0.10299999999999999,-1.58,"Date of issue  28/11/2024","2029-11-28"]
[null,null,"Fire rated glass","Vetrotech","Contraflam 30 (5/5) 16mm",67,1.36,0.45800000000000002,0,8.1300000000000001E-3,0,0,0,0,0,0,8.5000000000000006E-2,0,0.52,0,"S-P-09642","2028-06-22"]
[null,null,"Fire rated glass","Vetrotech","Contraflam lite 30 CFL30 (5/5) 13 mm",77,2.0699999999999998,6.05,0,0.155,0,0,0,0,0,0,9.5899999999999999E-2,0,0.45600000000000002,-1.98,"EPD-IES-0024348","2030-06-12"]
[null,null,"Fire rated glass","Vetrotech","Contraflam structure 30 STADIP CFS 30 (6/5/55.2) 28 mm",196,4.12,6.05,0,0.155,0,0,0,0,0,0,0.20100000000000001,0,0.96799999999999997,-1.98,"EPD-IES-0024372","2030-06-15"]
[null,null,"Fire rated glass","Vetrotech","Contraflam structure 60 STADIP CFS 60  (6/5/5/55.2) 36 mm",293,5.7,0.38800000000000001,0,0.155,0,0,0,0,0,0,0.27400000000000002,0,2.6,-3.9,"EPD-IES-0024375","2030-06-15"]
[]
[null,null,"Painted frit glass","Stronglasas","Monolithic toughened 4 mm",11.88,5.1499999999999997E-2,9.9000000000000005E-2,0,0,0,0,0,0,0,0,0,1.26E-2,1.3599999999999999E-2,-3.2,"S-P-10601","2028-09-08",null,4]
[null,null,"Painted frit glass","Stronglasas","Monolithic toughened 5 mm",{"$f":"($F$547/$X$547)*X548","v":14.850000000000001},{"$f":"($G$547/$X$547)*X548","v":6.4375000000000002E-2},{"$f":"($H$547/$X$547)*X548","v":0.12375},0,0,0,0,0,0,0,0,0,1.26E-2,1.3599999999999999E-2,{"$f":"($T$547/$X$547)*X548","v":-4},"S-P-10601","2028-09-08",null,5]
[null,null,"Painted frit glass","Stronglasas","Monolithic toughened 6 mm",{"$f":"($F$547/$X$547)*X549","v":17.82},{"$f":"($G$547/$X$547)*X549","v":7.7249999999999999E-2},{"$f":"($H$547/$X$547)*X549","v":0.14850000000000002},0,0,0,0,0,0,0,0,0,1.26E-2,1.3599999999999999E-2,{"$f":"($T$547/$X$547)*X549","v":-4.8000000000000007},"S-P-10601","2028-09-08",null,6]
[null,null,"Painted frit glass","Stronglasas","Monolithic toughened 8 mm",23.76,0.10299999999999999,0.19800000000000001,0,0,0,0,0,0,0,0,0,1.26E-2,1.3599999999999999E-2,-6.4,"S-P-10601","2028-09-08",null,8]
[null,null,"Painted frit glass","Stronglasas","Monolithic toughened 10 mm",29.700000000000003,0.12875,0.2475,0,0,0,0,0,0,0,0,0,1.26E-2,1.3599999999999999E-2,-8,"S-P-10601","2028-09-08",null,10]
[null,null,"Painted frit glass","Stronglasas","Monolithic toughened 12 mm",35.64,0.1545,0.29700000000000004,0,0,0,0,0,0,0,0,0,1.26E-2,1.3599999999999999E-2,-9.6000000000000014,"S-P-10601","2028-09-08",null,12]
[null,null,"Painted frit glass","Stronglasas","Monolithic toughened 15 mm",44.550000000000004,0.19312499999999999,0.37125000000000002,0,0,0,0,0,0,0,0,0,1.26E-2,1.3599999999999999E-2,-12,"S-P-10601","2028-09-08",null,15]
[]
[null,null,"Structural glass","Ionoplast film Kuraray Sentry glass","Lam toughened Low/mid iron 13.5 mm (66.4)",54.945599999999999,2.59606,0,0,0.45600226999999999,0,0,0,0,0,0,0.10053959999999999,0,0.49386249999999998,0," EPD-KUR-20230073-CBA2-EN","2029-03-11"]
[null,null,"Structural glass","Ionoplast film Kuraray Sentry glass","Lam toughened Low/mid iron  17.5 mm (88.4)",70.145600000000002,3.4560599999999999,0,0,0.60800226999999996,0,0,0,0,0,0,0.13373960000000001,0,0.65786250000000002,0," EPD-KUR-20230073-CBA2-EN","2029-03-11"]
[null,null,"Structural glass","Ionoplast film Kuraray Sentry glass","Lam toughened Low/mid iron 21.5 mm (1010.4)",85.345600000000005,4.3160600000000002,0,0,0.76000226999999998,0,0,0,0,0,0,0.16693960000000002,0,0.82186250000000005,0," EPD-KUR-20230073-CBA2-EN","2029-03-11"]
[null,null,"Structural glass","Ionoplast film Kuraray Sentry glass","Lam toughened Low/mid iron 25.5 mm (1212.4)",100.54559999999999,5.1760600000000005,0,0,0.91200226999999989,0,0,0,0,0,0,0.2001396,0,0.98586249999999997,0," EPD-KUR-20230073-CBA2-EN","2029-03-11"]
[null,null,"Structural glass","Ionoplast film Kuraray Sentry glass","Lam toughened Low/mid iron 31.5 mm (1515.4)",123.3456,6.4660600000000006,0,0,1.1400022699999999,0,0,0,0,0,0,0.24993960000000001,0,1.2318625000000001,0," EPD-KUR-20230073-CBA2-EN","2029-03-11"]
[]
["Secondary Sealant",null,"None","None","None",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"00:00:00"]
["Secondary Sealant",null,"Silicone","Dow corning","DOWSIL 3362 - 3363",5.31,5.2999999999999999E-2,0.67600000000000005,0,0,0,0,0,0,0,2.7900000000000001E-4,1.24E-2,0.94499999999999995,0.94499999999999995,-0.625,"EPD-DBC-20220179-IBF1-EN","2027-08-30"]
["Secondary Sealant",null,"Silicone","SIKA","IG-25 HM",5.31,5.2999999999999999E-2,0.67600000000000005,0,0,0,0,0,0,0,2.7900000000000001E-4,1.24E-2,0.94499999999999995,0.94499999999999995,-0.625,"EPD-DBC-20220179-IBF1-EN","2027-08-30"]
["Secondary Sealant",null,"Silicone","Silicone generic","Silicone-based products, group 2",6.82,5.8700000000000002E-2,0.69099999999999995,0,0,0,0,0,0,0,1.21E-2,0.45500000000000002,0.45500000000000002,0,-0.61799999999999999,"EPD-DBC-20220180-IBF1-EN","2027-08-30"]
["Secondary Sealant",null,"Polysulphide","Fenzi","Thiover",1.42,0,0,0,0,0,0,0,0,0,0,9.6200000000000001E-3,0,1.17E-2,0,"EPD-IES-13059:001","2029-07-25"]
["Secondary Sealant",null,"Polysulphide","Polysulphide generic","Generic Value",6.03,0.111,0.17599999999999999,0,0,0,0,0,0,0,2.7599999999999999E-4,4.8900000000000002E-3,1.24,0,-0.36499999999999999,"EPD-FEI-20250067-IBP1-EN","2030-06-03"]
[]
["Primary Sealant",null,"Fenzi Primary Sealant","Butylver","Butylver",3.5099999999999999E-2,1.1999999999999999E-3,1E-3,0,0,0,0,0,0,0,0,1E-3,1.2E-2,1E-3,0,"EPD-IES-13054:001","2029-07-25"]
["Primary Sealant",null,"Butyle generic","Butyle generic","Butyle generic",0.05,1E-3,1.8E-3,0,0,0,0,0,0,0,0,1E-3,1.47E-2,1E-3,0,"EPD-FEI-20250068-IBP1-EN","2030-06-03"]
["Primary Sealant",null,"None","None","None",0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,0,"00/01/1900"]
[]
[]
["Spacer bar",null,"ALUPRO","Aluminium spacer","Aluminium H65 A155, width 10 mm",1.4325000000000001,0,0,0,0,0,0,0,0,0,0,1.91E-3,0,2.8250000000000001E-2,-4.2000000000000006E-3,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Aluminium spacer","Aluminium H65 A155, width 12 mm",1.7190000000000001,0,0,0,0,0,0,0,0,0,0,2.2920000000000002E-3,0,3.39E-2,-5.0400000000000002E-3,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Aluminium spacer","Aluminium H65 A155, width 14 mm",2.0055000000000001,0,0,0,0,0,0,0,0,0,0,2.6740000000000002E-3,0,3.9549999999999988E-2,-5.8799999999999998E-3,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Aluminium spacer","Aluminium H65 A155, width 16 mm",2.2919999999999998,0,0,0,0,0,0,0,0,0,0,3.0560000000000001E-3,0,4.5199999999999997E-2,-6.7200000000000003E-3,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Aluminium spacer","Aluminium H65 A155, width 18 mm",2.5785,0,0,0,0,0,0,0,0,0,0,3.4380000000000001E-3,0,5.0849999999999999E-2,-7.5600000000000007E-3,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Aluminium spacer","Aluminium H65 A155, width 20 mm",2.8650000000000002,0,0,0,0,0,0,0,0,0,0,3.82E-3,0,5.6499999999999988E-2,-8.4000000000000012E-3,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Aluminium spacer","Aluminium H65 A155, width 22 mm",3.1515,0,0,0,0,0,0,0,0,0,0,4.202E-3,0,6.2149999999999997E-2,-9.2399999999999999E-3,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Aluminium spacer","Aluminium H65 A155, width 24 mm",3.4380000000000002,0,0,0,0,0,0,0,0,0,0,4.5840000000000004E-3,0,6.7799999999999999E-2,-1.008E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Aluminium spacer","Aluminium H65 A155, width 26 mm",3.7244999999999999,0,0,0,0,0,0,0,0,0,0,4.9659999999999999E-3,0,7.3450000000000001E-2,-1.0919999999999999E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Chromatech","Ultra F, width 10 mm",0.54297600000000001,0,0,0,0,0,0,0,0,0,0,3.5875200000000012E-3,0,9.5343999999999998E-2,-4.2662400000000003E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Chromatech","Ultra F, width 12 mm",0.56515199999999999,0,0,0,0,0,0,0,0,0,0,3.7340400000000001E-3,0,9.9237999999999993E-2,-4.4404800000000001E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Chromatech","Ultra F, width 14 mm",0.58732800000000007,0,0,0,0,0,0,0,0,0,0,3.8805599999999999E-3,0,0.103132,-4.6147199999999999E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Chromatech","Ultra F, width 16 mm",0.67200000000000004,0,0,0,0,0,0,0,0,0,0,4.4400000000000004E-3,0,0.11799999999999999,-5.28E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Chromatech","Ultra F, width 18 mm",0.69955199999999995,0,0,0,0,0,0,0,0,0,0,4.62204E-3,0,0.122838,-5.4964799999999987E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Chromatech","Ultra F, width 20 mm",0.75331200000000009,0,0,0,0,0,0,0,0,0,0,4.9772400000000008E-3,0,0.13227800000000001,-5.91888E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Chromatech","Ultra F, width 22 mm",0.81446400000000008,0,0,0,0,0,0,0,0,0,0,5.3812799999999996E-3,0,0.143016,-6.3993599999999998E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Multitech G","Multitech G, width 10 mm",0.49458400000000002,0,0,0,0,0,0,0,0,0,0,2.3158720000000001E-3,0,9.0009599999999981E-2,-6.6569600000000007E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Multitech G","Multitech G, width 12 mm",0.59586399999999995,0,0,0,0,0,0,0,0,0,0,2.790112E-3,0,0.1084416,-8.0201599999999998E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Multitech G","Multitech G, width 14 mm",0.669292,0,0,0,0,0,0,0,0,0,0,3.1339359999999999E-3,0,0.1218048,-9.0084800000000007E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Multitech G","Multitech G, width 16 mm",0.84399999999999997,0,0,0,0,0,0,0,0,0,0,3.9519999999999998E-3,0,0.15359999999999999,-0.11360000000000001,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Multitech G","Multitech G, width 18 mm",0.91573999999999989,0,0,0,0,0,0,0,0,0,0,4.2879199999999998E-3,0,0.166656,-0.123256,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Multitech G","Multitech G, width 20 mm",0.98832399999999998,0,0,0,0,0,0,0,0,0,0,4.6277919999999986E-3,0,0.17986559999999999,-0.13302559999999999,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Multitech G","Multitech G, width 22 mm",1.061752,0,0,0,0,0,0,0,0,0,0,4.9716159999999999E-3,0,0.19322880000000001,-0.1429088,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Multitech G","Multitech G, width 24 mm",1.134336,0,0,0,0,0,0,0,0,0,0,5.3114879999999996E-3,0,0.20643839999999999,-0.15267839999999999,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Multitech G","Multitech G, width 26 mm",1.2643120000000001,0,0,0,0,0,0,0,0,0,0,5.9200959999999997E-3,0,0.23009279999999999,-0.17017280000000001,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Thermix TX Pro","Thermix TX Pro, width 10 mm",0.51771600000000007,0,0,0,0,0,0,0,0,0,0,2.6280000000000001E-3,0,3.6266399999999997E-2,-3.6266399999999997E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Thermix TX Pro","Thermix TX Pro, width 12 mm",0.53978000000000004,0,0,0,0,0,0,0,0,0,0,2.7399999999999998E-3,0,3.7812000000000012E-2,-3.7812000000000012E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Thermix TX Pro","Thermix TX Pro, width 14 mm",0.67216399999999998,0,0,0,0,0,0,0,0,0,0,3.4120000000000001E-3,0,4.7085599999999998E-2,-4.7085599999999998E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Thermix TX Pro","Thermix TX Pro, width 16 mm",0.78800000000000003,0,0,0,0,0,0,0,0,0,0,4.0000000000000001E-3,0,5.5199999999999999E-2,-5.5199999999999999E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Thermix TX Pro","Thermix TX Pro, width 18 mm",0.85182800000000003,0,0,0,0,0,0,0,0,0,0,4.3239999999999997E-3,0,5.9671199999999987E-2,-5.9671199999999987E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Thermix TX Pro","Thermix TX Pro, width 20 mm",0.88807600000000009,0,0,0,0,0,0,0,0,0,0,4.5079999999999999E-3,0,6.2210399999999999E-2,-6.2210399999999999E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Thermix TX Pro","Thermix TX Pro, width 22 mm",0.91565600000000003,0,0,0,0,0,0,0,0,0,0,4.6479999999999994E-3,0,6.4142399999999988E-2,-6.4142399999999988E-2,"S-P-08910","2028-03-23"]
["Spacer bar",null,"ALUPRO","Thermix TX Pro","Thermix TX Pro, width 24 mm",0.95347999999999999,0,0,0,0,0,0,0,0,0,0,4.8399999999999997E-3,0,6.679199999999999E-2,-6.679199999999999E-2,"S-P-08910","2028-03-23"]
[]
["Spacer bar",null,"Swisspacer","Advance","Width 10 mm",0.37519999999999998,0,0,0,0,0,0,0,0,0,0,9.5943999999999999E-4,0,6.7804000000000007E-3,-9.5943999999999999E-4,"EPD-IES-0011836:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Advance","Width 12 mm",0.47039999999999998,0,0,0,0,0,0,0,0,0,0,1.2028799999999999E-3,0,8.5007999999999993E-3,-1.2028799999999999E-3,"EPD-IES-0011836:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Advance","Width 14 mm",0.53760000000000008,0,0,0,0,0,0,0,0,0,0,1.3747200000000001E-3,0,9.7152000000000002E-3,-1.3747200000000001E-3,"EPD-IES-0011836:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Advance","Width 16 mm",0.54320000000000002,0,0,0,0,0,0,0,0,0,0,1.38904E-3,0,9.8163999999999994E-3,-1.38904E-3,"EPD-IES-0011836:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Advance","Width 18 mm",0.63280000000000003,0,0,0,0,0,0,0,0,0,0,1.61816E-3,0,1.1435600000000001E-2,-1.61816E-3,"EPD-IES-0011836:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Advance","Width 20 mm",0.68320000000000003,0,0,0,0,0,0,0,0,0,0,1.7470400000000001E-3,0,1.23464E-2,-1.7470400000000001E-3,"EPD-IES-0011836:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Advance","Width 22 mm",0.73920000000000008,0,0,0,0,0,0,0,0,0,0,1.8902400000000001E-3,0,1.3358399999999999E-2,-1.8902400000000001E-3,"EPD-IES-0011836:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Advance","Width 24 mm",0.84000000000000008,0,0,0,0,0,0,0,0,0,0,2.1480000000000002E-3,0,1.5180000000000001E-2,-2.1480000000000002E-3,"EPD-IES-0011836:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Advance","Width 27 mm",0.88480000000000014,0,0,0,0,0,0,0,0,0,0,2.2625599999999998E-3,0,1.59896E-2,-2.2625599999999998E-3,"EPD-IES-0011836:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Ultimate","Width 10 mm",0.37519999999999998,0,0,0,0,0,0,0,0,0,0,9.5943999999999999E-4,0,6.8608000000000011E-3,-9.326400000000001E-4,"EPD-IES-0011837:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Ultimate","Width 12 mm",0.47039999999999998,0,0,0,0,0,0,0,0,0,0,1.2028799999999999E-3,0,8.6016000000000009E-3,-1.16928E-3,"EPD-IES-0011837:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Ultimate","Width 14 mm",0.53760000000000008,0,0,0,0,0,0,0,0,0,0,1.3747200000000001E-3,0,9.8304000000000013E-3,-1.33632E-3,"EPD-IES-0011837:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Ultimate","Width 16 mm",0.56000000000000005,0,0,0,0,0,0,0,0,0,0,1.4319999999999999E-3,0,1.0240000000000001E-2,-1.392E-3,"EPD-IES-0011837:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Ultimate","Width 18 mm",0.63280000000000003,0,0,0,0,0,0,0,0,0,0,1.61816E-3,0,1.15712E-2,-1.57296E-3,"EPD-IES-0011837:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Ultimate","Width 20 mm",0.68320000000000003,0,0,0,0,0,0,0,0,0,0,1.7470400000000001E-3,0,1.24928E-2,-1.6982399999999999E-3,"EPD-IES-0011837:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Ultimate","Width 22 mm",0.73920000000000008,0,0,0,0,0,0,0,0,0,0,1.8902400000000001E-3,0,1.3516800000000001E-2,-1.8374400000000001E-3,"EPD-IES-0011837:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Ultimate","Width 24 mm",0.84000000000000008,0,0,0,0,0,0,0,0,0,0,2.1480000000000002E-3,0,1.536E-2,-2.088E-3,"EPD-IES-0011837:001","2029-12-15"]
["Spacer bar",null,"Swisspacer","Ultimate","Width 27 mm",0.88480000000000014,0,0,0,0,0,0,0,0,0,0,2.2625599999999998E-3,0,1.6179200000000001E-2,-2.19936E-3,"EPD-IES-0011837:001","2029-12-15"]
[]
["Spacer bar",null,"Technoform","Warm edge SP14","Width 10 mm",0.37519999999999998,5.0384000000000002E-3,8.3347999999999998E-3,0,0,0,0,0,0,0,0,9.5943999999999999E-4,0,6.8608000000000011E-3,-9.326400000000001E-4,"S-P-10425","2028-12-11"]
["Spacer bar",null,"Technoform","Warm edge SP14","Width 12 mm",0.47039999999999998,6.3167999999999992E-3,1.04496E-2,0,0,0,0,0,0,0,0,1.2028799999999999E-3,1,8.6016000000000009E-3,-1.16928E-3,"S-P-10425","2028-12-11"]
["Spacer bar",null,"Technoform","Warm edge SP14","Width 14 mm",0.53760000000000008,7.2191999999999994E-3,1.1942400000000001E-2,0,0,0,0,0,0,0,0,1.3747200000000001E-3,2,9.8304000000000013E-3,-1.33632E-3,"S-P-10425","2028-12-11"]
["Spacer bar",null,"Technoform","Warm edge SP14","Width 16 mm",0.56000000000000005,7.5199999999999998E-3,1.244E-2,0,0,0,0,0,0,0,0,1.4319999999999999E-3,3,1.0240000000000001E-2,-1.392E-3,"S-P-10425","2028-12-11"]
["Spacer bar",null,"Technoform","Warm edge SP14","Width 18 mm",0.63280000000000003,8.4975999999999993E-3,1.4057200000000001E-2,0,0,0,0,0,0,0,0,1.61816E-3,4,1.15712E-2,-1.57296E-3,"S-P-10425","2028-12-11"]
["Spacer bar",null,"Technoform","Warm edge SP14","Width 20 mm",0.68320000000000003,9.1743999999999992E-3,1.5176800000000001E-2,0,0,0,0,0,0,0,0,1.7470400000000001E-3,5,1.24928E-2,-1.6982399999999999E-3,"S-P-10425","2028-12-11"]

{"sheet":"Calculation Guardian","index":5,"n_rows":147,"n_cols":26,"rows_kept":147,"cut":false,"hidden":true,"merged":[[128,0,146,0],[128,19,128,21],[129,19,129,21],[130,19,130,21],[131,19,131,21],[132,19,132,21],[133,19,133,21],[134,19,134,21],[136,19,136,21],[141,19,141,21],[142,19,142,21],[137,19,137,21],[138,19,138,21],[139,19,139,21],[140,19,140,21],[25,0,38,0],[31,19,31,21],[32,19,32,21],[14,19,14,21],[15,19,15,21],[16,19,16,21],[14,0,23,0],[33,19,33,21],[34,19,34,21],[25,19,25,21],[26,19,26,21],[27,19,27,21],[28,19,28,21],[29,19,29,21],[30,19,30,21],[1,2,2,2],[3,0,12,0],[5,19,5,21],[6,19,6,21],[7,19,7,21],[8,19,8,21],[4,19,4,21],[3,19,3,21],[40,0,49,0],[40,19,40,21],[41,19,41,21],[42,19,42,21],[43,19,43,21],[44,19,44,21],[45,19,45,21],[51,0,60,0],[51,19,51,21],[52,19,52,21],[53,19,53,21],[62,0,75,0],[62,19,62,21],[63,19,63,21],[64,19,64,21],[65,19,65,21],[66,19,66,21],[67,19,67,21],[68,19,68,21],[69,19,69,21],[70,19,70,21],[71,19,71,21],[77,0,86,0],[77,19,77,21],[78,19,78,21],[79,19,79,21],[80,19,80,21],[81,19,81,21],[82,19,82,21],[88,0,97,0],[88,19,88,21],[89,19,89,21],[90,19,90,21],[99,0,108,0],[99,19,99,21],[100,19,100,21],[101,19,101,21],[102,19,102,21],[103,19,103,21],[104,19,104,21],[110,0,123,0],[110,19,110,21],[111,19,111,21],[112,19,112,21],[113,19,113,21],[114,19,114,21],[115,19,115,21],[116,19,116,21],[117,19,117,21],[118,19,118,21],[119,19,119,21]]}
[]
[null,null,"Thickness","A1-A3","A4","A5","B1","B2","B3","B4","B5","B6","B7","C1","C2","C3","C4","D",null,null,null,null,null,null,"Coating \nimpact","Laminating\n impact"]
[]
["Nexa 6 monolithic",null,1,{"$f":"W4*W5","v":1.595},{"$f":"W4*W6","v":0.17224999999999999},0,0,{"$f":"W4*W7","v":0.33750000000000002},0,0,0,0,0,0,{"$f":"W4*W8","v":2.3725E-2},0,{"$f":"W4*W9","v":0.10825},0,null,"Glass impact per 1 mm",null,null,0.25]
[null,null,2,{"$f":"$D$4*C5","v":3.19},{"$f":"$E$4*C5","v":0.34449999999999997},0,0,{"$f":"$H$4*C5","v":0.67500000000000004},0,0,0,0,0,0,{"$f":"$O$4*C5","v":4.7449999999999999E-2},0,{"$f":"$Q$4*C5","v":0.2165},0,null,"Scaling factor per 4 mm (A1-A3)",null,null,6.38]
[null,null,3,{"$f":"$D$4*C6","v":4.7850000000000001},{"$f":"$E$4*C6","v":0.51674999999999993},0,0,{"$f":"$H$4*C6","v":1.0125000000000002},0,0,0,0,0,0,{"$f":"$O$4*C6","v":7.1175000000000002E-2},0,{"$f":"$Q$4*C6","v":0.32474999999999998},0,null,"Scaling factor per 4 mm (A4)",null,null,0.68899999999999995]
[null,null,4,6.38,0.68899999999999995,0,0,1.35,0,0,0,0,0,0,9.4899999999999998E-2,0,0.433,0,null,"Scaling factor per 4 mm (B2)",null,null,1.35]
[null,null,5,7.9749999999999996,0.86124999999999996,0,0,1.6875,0,0,0,0,0,0,0.11862499999999999,0,0.54125000000000001,0,null,"Scaling factor per 4 mm (C2)",null,null,9.4899999999999998E-2]
[null,null,6,9.57,1.0334999999999999,0,0,2.0250000000000004,0,0,0,0,0,0,0.14235,0,0.64949999999999997,0,null,"Scaling factor per 4 mm (C4)",null,null,0.433]
[null,null,8,12.76,1.3779999999999999,0,0,2.7,0,0,0,0,0,0,0.1898,0,0.86599999999999999,0]
[null,null,10,15.95,1.7224999999999999,0,0,3.375,0,0,0,0,0,0,0.23724999999999999,0,1.0825,0]
[null,null,12,19.14,2.0669999999999997,0,0,4.0500000000000007,0,0,0,0,0,0,0.28470000000000001,0,1.2989999999999999,0]
[null,null,15,23.925000000000001,2.5837499999999998,0,0,5.0625,0,0,0,0,0,0,0.355875,0,1.62375,0]
[]
["Nexa 6 coated monolithic",null,1,{"$f":"W15*W16","v":1.8125},{"$f":"W18*W15","v":0.17224999999999999},0,0,{"$f":"W15*W19","v":0.33750000000000002},0,0,0,0,0,0,{"$f":"W15*W20","v":2.3725E-2},0,{"$f":"W15*W21","v":0.10825},0,null,"Glass impact per 1 mm",null,null,0.25]
[null,null,2,{"$f":"$D$15*C16","v":3.625},{"$f":"$E$15*C16","v":0.34449999999999997},0,0,{"$f":"$H$15*C16","v":0.67500000000000004},0,0,0,0,0,0,{"$f":"$O$15*C16","v":4.7449999999999999E-2},0,{"$f":"$Q$15*C16","v":0.2165},0,null,"Scaling factor per 4 mm (A1-A3) (flat+coating)",null,null,{"$f":"W17+Y16","v":7.25},null,0.87]
[null,null,3,{"$f":"$D$15*C17","v":5.4375},0.51674999999999993,0,0,{"$f":"$H$15*C17","v":1.0125000000000002},0,0,0,0,0,0,{"$f":"$O$15*C17","v":7.1175000000000002E-2},0,{"$f":"$Q$15*C17","v":0.32474999999999998},0,null,"Scaling factor per 4 mm (A1-A3)",null,null,6.38]
[null,null,4,7.25,0.68899999999999995,0,0,1.35,0,0,0,0,0,0,9.4899999999999998E-2,0,0.433,0,null,"Scaling factor per 4 mm (A4)",null,null,0.68899999999999995]
[null,null,5,9.0625,0.86124999999999996,0,0,1.6875,0,0,0,0,0,0,0.11862499999999999,0,0.54125000000000001,0,null,"Scaling factor per 4 mm (B2)",null,null,1.35]
[null,null,6,10.875,1.0334999999999999,0,0,2.0250000000000004,0,0,0,0,0,0,0.14235,0,0.64949999999999997,0,null,"Scaling factor per 4 mm (C2)",null,null,9.4899999999999998E-2]
[null,null,8,14.5,1.3779999999999999,0,0,2.7,0,0,0,0,0,0,0.1898,0,0.86599999999999999,0,null,"Scaling factor per 4 mm (C4)",null,null,0.433]
[null,null,10,18.125,1.7224999999999999,0,0,3.375,0,0,0,0,0,0,0.23724999999999999,0,1.0825,0]
[null,null,12,21.75,2.0669999999999997,0,0,4.0500000000000007,0,0,0,0,0,0,0.28470000000000001,0,1.2989999999999999,0]
[null,null,15,27.1875,2.5837499999999998,0,0,5.0625,0,0,0,0,0,0,0.355875,0,1.62375,0]
[]
["Nexa 6 laminated",null,1,{"$f":"W27*W28","v":0.8175},{"$f":"W27*W36","v":0.17874999999999999},0,0,{"$f":"W27*W37","v":0.35125000000000001},0,0,0,0,0,0,{"$f":"W27*W38","v":2.4625000000000001E-2},0,{"$f":"W27*W39","v":0.112625},0,null,"Glass impact per 1 mm",null,null,0.25]
[null,"6.4 (33.1)",6,{"$f":"($D$26*C27)+($W$32*W29)+$Z$27","v":7.4690000000000003},{"$f":"$E$26*C27","v":1.0725},0,0,{"$f":"$H$26*C27","v":2.1074999999999999},0,0,0,0,0,0,{"$f":"$O$26*C27","v":0.14774999999999999},0,{"$f":"$Q$26*C27","v":0.67575000000000007},0,null,null,null,null,0.125,null,null,0.76400000000000001]
[null,"6.8 (33.2)",6,{"$f":"($D$26*C28)+($W$32*W30)+$Z$27","v":9.2690000000000001},{"$f":"$E$26*C28","v":1.0725},0,0,{"$f":"$H$26*C28","v":2.1074999999999999},0,0,0,0,0,0,{"$f":"$O$26*C28","v":0.14774999999999999},0,{"$f":"$Q$26*C28","v":0.67575000000000007},0,null,"Scaling factor per 4 mm (A1-A3)",null,null,6.54]
[null,"8.4 (44.1)",8,{"$f":"($D$26*C29)+($W$32*W29)+$Z$27","v":9.1039999999999992},1.43,0,0,2.81,0,0,0,0,0,0,0.19700000000000001,0,0.90100000000000002,0,null,"Scaling factor - Interlayer 0.38 (1)",null,null,1]
[null,"8.8 (44.2)",8,{"$f":"($D$26*C30)+($W$32*W30)+$Z$27","v":10.904},1.43,0,0,2.81,0,0,0,0,0,0,0.19700000000000001,0,0.90100000000000002,0,null,"Scaling factor - Interlayer 0.76 (2)",null,null,2]
[null,"10.4 (55.1)",10,{"$f":"($D$26*C31)+($W$32*W29)+$Z$27","v":10.739000000000001},1.7874999999999999,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,1.12625,0,null,"Scaling factor - Interlayer 1.52 (4)",null,null,4]
[null,"10.8 (55.2)",10,{"$f":"($D$26*C32)+($W$32*W30)+$Z$27","v":12.539},1.7874999999999999,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,1.12625,0,null,"Interlayer factor",null,null,1.8]
[null,"11.5 (55.4)",10,{"$f":"($D$26*C33)+($W$32*W31)+$Z$27","v":16.138999999999999},1.7874999999999999,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,1.12625,0]
[null,"12.4 (66.1)",12,{"$f":"($D$26*C34)+($W$32*W29)+$Z$27","v":12.374000000000001},2.145,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.3515000000000001,0]
[null,"12.8 (66.2)",12,{"$f":"($D$26*C35)+($W$32*W30)+$Z$27","v":14.173999999999999},2.145,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.3515000000000001,0]
[null,"13.5 (66.4)",12,{"$f":"($D$26*C36)+($W$32*W31)+$Z$27","v":17.774000000000001},2.145,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.3515000000000001,0,null,"Scaling factor per 44.2 mm (A4)",null,null,1.43]
[null,"16.4 (88.1)",16,{"$f":"($D$26*C37)+($W$32*W29)+$Z$27","v":15.644},2.86,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.802,0,null,"Scaling factor per 44.2 mm (B2)",null,null,2.81]
[null,"16.8 (88.2)",16,{"$f":"($D$26*C38)+($W$32*W30)+$Z$27","v":17.443999999999999},2.86,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.802,0,null,"Scaling factor per 44.2 mm (C2)",null,null,0.19700000000000001]
[null,"17.5 (88.4)",16,{"$f":"($D$26*C39)+($W$32*W31)+$Z$27","v":21.044},2.86,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.802,0,null,"Scaling factor per 44.2 mm (C4)",null,null,0.90100000000000002]
[]
["Nexa 9 monolithic",null,1,{"$f":"W41*W42","v":2.145},{"$f":"W41*W43","v":0.17224999999999999},0,0,{"$f":"W41*W44","v":0.33750000000000002},0,0,0,0,0,0,{"$f":"W41*W45","v":2.3725E-2},0,{"$f":"W41*W46","v":0.10825},0,null,"Glass impact per 1 mm",null,null,0.25]
[null,null,2,{"$f":"$D$41*C42","v":4.29},{"$f":"$E$41*C42","v":0.34449999999999997},0,0,{"$f":"$H$41*C42","v":0.67500000000000004},0,0,0,0,0,0,{"$f":"$O$41*C42","v":4.7449999999999999E-2},0,{"$f":"$Q$41*C42","v":0.2165},0,null,"Scaling factor per 4 mm (A1-A3)",null,null,8.58]
[null,null,3,{"$f":"$D$41*C43","v":6.4350000000000005},{"$f":"$E$41*C43","v":0.51674999999999993},0,0,{"$f":"$H$41*C43","v":1.0125000000000002},0,0,0,0,0,0,{"$f":"$O$41*C43","v":7.1175000000000002E-2},0,{"$f":"$Q$41*C43","v":0.32474999999999998},0,null,"Scaling factor per 4 mm (A4)",null,null,0.68899999999999995]
[null,null,4,8.58,0.68899999999999995,0,0,1.35,0,0,0,0,0,0,9.4899999999999998E-2,0,0.433,0,null,"Scaling factor per 4 mm (B2)",null,null,1.35]
[null,null,5,10.725,0.86124999999999996,0,0,1.6875,0,0,0,0,0,0,0.11862499999999999,0,0.54125000000000001,0,null,"Scaling factor per 4 mm (C2)",null,null,9.4899999999999998E-2]
[null,null,6,12.870000000000001,1.0334999999999999,0,0,2.0250000000000004,0,0,0,0,0,0,0.14235,0,0.64949999999999997,0,null,"Scaling factor per 4 mm (C4)",null,null,0.433]
[null,null,8,17.16,1.3779999999999999,0,0,2.7,0,0,0,0,0,0,0.1898,0,0.86599999999999999,0]
[null,null,10,21.45,1.7224999999999999,0,0,3.375,0,0,0,0,0,0,0.23724999999999999,0,1.0825,0]
[null,null,12,25.740000000000002,2.0669999999999997,0,0,4.0500000000000007,0,0,0,0,0,0,0.28470000000000001,0,1.2989999999999999,0]
[null,null,15,32.174999999999997,2.5837499999999998,0,0,5.0625,0,0,0,0,0,0,0.355875,0,1.62375,0]
[]
["Nexa 9 coated monolithic",null,1,{"$f":"W52*W53","v":2.5},{"$f":"W55*W52","v":0.17224999999999999},0,0,{"$f":"W52*W56","v":0.33750000000000002},0,0,0,0,0,0,{"$f":"W52*W57","v":2.3725E-2},0,{"$f":"W52*W58","v":0.10825},0,null,"Glass impact per 1 mm",null,null,0.25]
[null,null,2,{"$f":"$D$52*C53","v":5},{"$f":"$E$52*C53","v":0.34449999999999997},0,0,{"$f":"$H$52*C53","v":0.67500000000000004},0,0,0,0,0,0,{"$f":"$O$52*C53","v":4.7449999999999999E-2},0,{"$f":"$Q$52*C53","v":0.2165},0,null,"Scaling factor per 4 mm (A1-A3) (flat+coating)",null,null,{"$f":"W54+Y53","v":10},null,1.01]
[null,null,3,{"$f":"$D$52*C54","v":7.5},{"$f":"$E$52*C54","v":0.51674999999999993},0,0,{"$f":"$H$52*C54","v":1.0125000000000002},0,0,0,0,0,0,{"$f":"$O$52*C54","v":7.1175000000000002E-2},0,{"$f":"$Q$52*C54","v":0.32474999999999998},0,null,"Scaling factor per 4 mm (A1-A3)",null,null,8.99]
[null,null,4,10,0.68899999999999995,0,0,1.35,0,0,0,0,0,0,9.4899999999999998E-2,0,0.433,0,null,"Scaling factor per 4 mm (A4)",null,null,0.68899999999999995]
[null,null,5,12.5,0.86124999999999996,0,0,1.6875,0,0,0,0,0,0,0.11862499999999999,0,0.54125000000000001,0,null,"Scaling factor per 4 mm (B2)",null,null,1.35]
[null,null,6,15,1.0334999999999999,0,0,2.0250000000000004,0,0,0,0,0,0,0.14235,0,0.64949999999999997,0,null,"Scaling factor per 4 mm (C2)",null,null,9.4899999999999998E-2]
[null,null,8,20,1.3779999999999999,0,0,2.7,0,0,0,0,0,0,0.1898,0,0.86599999999999999,0,null,"Scaling factor per 4 mm (C4)",null,null,0.433]
[null,null,10,25,1.7224999999999999,0,0,3.375,0,0,0,0,0,0,0.23724999999999999,0,1.0825,0]
[null,null,12,30,2.0669999999999997,0,0,4.0500000000000007,0,0,0,0,0,0,0.28470000000000001,0,1.2989999999999999,0]
[null,null,15,37.5,2.5837499999999998,0,0,5.0625,0,0,0,0,0,0,0.355875,0,1.62375,0]
[]
["Nexa 9 laminated",null,1,{"$f":"W63*W65","v":2.1974999999999998},{"$f":"W64*W73","v":0.17874999999999999},0,0,{"$f":"W64*W74","v":0.35125000000000001},0,0,0,0,0,0,{"$f":"W64*W75","v":2.4625000000000001E-2},0,{"$f":"W64*W76","v":0.112625},0,null,"Glass impact per 1 mm",null,null,0.25]
[null,"6.4 (33.1)",6,{"$f":"($D$63*C64)+($W$69*W66)+$Z$64","v":16.754999999999999},{"$f":"$E$63*C64","v":1.0725},0,0,{"$f":"$H$63*C64","v":2.1074999999999999},0,0,0,0,0,0,{"$f":"$O$63*C64","v":0.14774999999999999},0,{"$f":"$Q$63*C64","v":0.67575000000000007},0,null,null,null,null,0.125,null,null,1.77]
[null,"6.8 (33.2)",6,{"$f":"($D$63*C65)+($W$69*W67)+$Z$64","v":18.555},{"$f":"$E$63*C65","v":1.0725},0,0,{"$f":"$H$63*C65","v":2.1074999999999999},0,0,0,0,0,0,{"$f":"$O$63*C65","v":0.14774999999999999},0,{"$f":"$Q$63*C65","v":0.67575000000000007},0,null,"Scaling factor per 4 mm (A1-A3)",null,null,8.7899999999999991]
[null,"8.4 (44.1)",8,{"$f":"($D$63*C66)+($W$69*W66)+$Z$64","v":21.15},{"$f":"$E$63*C66","v":1.43},0,0,2.81,0,0,0,0,0,0,0.19700000000000001,0,0.90100000000000002,0,null,"Scaling factor - Interlayer 0.38 (1)",null,null,1]
[null,"8.8 (44.2)",8,{"$f":"($D$63*C67)+($W$69*W67)+$Z$64","v":22.95},1.43,0,0,2.81,0,0,0,0,0,0,0.19700000000000001,0,0.90100000000000002,0,null,"Scaling factor - Interlayer 0.76 (2)",null,null,2]
[null,"10.4 (55.1)",10,{"$f":"($D$63*C68)+($W$69*W66)+$Z$64","v":25.544999999999998},1.7874999999999999,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,1.12625,0,null,"Scaling factor - Interlayer 1.52 (4)",null,null,4]
[null,"10.8 (55.2)",10,{"$f":"($D$63*C69)+($W$69*W67)+$Z$64","v":27.344999999999999},1.7874999999999999,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,1.12625,0,null,"Interlayer factor",null,null,1.8]
[null,"11.5 (55.4)",10,{"$f":"($D$63*C70)+($W$69*W68)+$Z$64","v":30.944999999999997},1.7874999999999999,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,1.12625,0]
[null,"12.4 (66.1)",12,{"$f":"($D$63*C71)+($W$69*W66)+$Z$64","v":29.939999999999998},2.145,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.3515000000000001,0]
[null,"12.8 (66.2)",12,{"$f":"($D$63*C72)+($W$69*W67)+$Z$64","v":31.74},2.145,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.3515000000000001,0]
[null,"13.5 (66.4)",12,35.340000000000003,2.145,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.3515000000000001,0,null,"Scaling factor per 44.2 mm (A4)",null,null,1.43]
[null,"16.4 (88.1)",16,{"$f":"($D$63*C74)+($W$69*W66)+$Z$64","v":38.729999999999997},2.86,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.802,0,null,"Scaling factor per 44.2 mm (B2)",null,null,2.81]
[null,"16.8 (88.2)",16,{"$f":"($D$63*C75)+($W$69*W67)+$Z$64","v":40.53},2.86,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.802,0,null,"Scaling factor per 44.2 mm (C2)",null,null,0.19700000000000001]
[null,"17.5 (88.4)",16,44.13,2.86,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.802,0,null,"Scaling factor per 44.2 mm (C4)",null,null,0.90100000000000002]
[]
["Monolithic Extraclear ",null,1,{"$f":"W78*W79","v":2.41},{"$f":"W78*W80","v":0.17224999999999999},0,0,{"$f":"W78*W81","v":0.33750000000000002},0,0,0,0,0,0,{"$f":"W78*W82","v":2.3725E-2},0,{"$f":"W78*W83","v":0.10825},0,null,"Glass impact per 1 mm",null,null,0.25]
[null,null,2,{"$f":"$D$78*C79","v":4.82},{"$f":"$E$78*C79","v":0.34449999999999997},0,0,{"$f":"$H$78*C79","v":0.67500000000000004},0,0,0,0,0,0,{"$f":"$O$78*C79","v":4.7449999999999999E-2},0,{"$f":"$Q$78*C79","v":0.2165},0,null,"Scaling factor per 4 mm (A1-A3)",null,null,9.64]
[null,null,3,{"$f":"$D$78*C80","v":7.23},{"$f":"$E$78*C80","v":0.51674999999999993},0,0,{"$f":"$H$78*C80","v":1.0125000000000002},0,0,0,0,0,0,{"$f":"$O$78*C80","v":7.1175000000000002E-2},0,{"$f":"$Q$78*C80","v":0.32474999999999998},0,null,"Scaling factor per 4 mm (A4)",null,null,0.68899999999999995]
[null,null,4,9.64,0.68899999999999995,0,0,1.35,0,0,0,0,0,0,9.4899999999999998E-2,0,0.433,0,null,"Scaling factor per 4 mm (B2)",null,null,1.35]
[null,null,5,12.05,0.86124999999999996,0,0,1.6875,0,0,0,0,0,0,0.11862499999999999,0,0.54125000000000001,0,null,"Scaling factor per 4 mm (C2)",null,null,9.4899999999999998E-2]
[null,null,6,14.46,1.0334999999999999,0,0,2.0250000000000004,0,0,0,0,0,0,0.14235,0,0.64949999999999997,0,null,"Scaling factor per 4 mm (C4)",null,null,0.433]
[null,null,8,19.28,1.3779999999999999,0,0,2.7,0,0,0,0,0,0,0.1898,0,0.86599999999999999,0]
[null,null,10,24.1,1.7224999999999999,0,0,3.375,0,0,0,0,0,0,0.23724999999999999,0,1.0825,0]
[null,null,12,28.92,2.0669999999999997,0,0,4.0500000000000007,0,0,0,0,0,0,0.28470000000000001,0,1.2989999999999999,0]
[null,null,15,36.150000000000006,2.5837499999999998,0,0,5.0625,0,0,0,0,0,0,0.355875,0,1.62375,0]
[]
["Monolithic Extraclear coated",null,1,{"$f":"W89*W90","v":2.7674999999999996},{"$f":"W92*W89","v":0.17224999999999999},0,0,{"$f":"W89*W93","v":0.33750000000000002},0,0,0,0,0,0,{"$f":"W89*W94","v":2.3725E-2},0,{"$f":"W89*W95","v":0.10825},0,null,"Glass impact per 1 mm",null,null,0.25]
[null,null,2,{"$f":"$D$89*C90","v":5.5349999999999993},{"$f":"$E$89*C90","v":0.34449999999999997},0,0,{"$f":"$H$89*C90","v":0.67500000000000004},0,0,0,0,0,0,{"$f":"$O$89*C90","v":4.7449999999999999E-2},0,{"$f":"$Q$89*C90","v":0.2165},0,null,"Scaling factor per 4 mm (A1-A3) (flat+coating)",null,null,{"$f":"W91+Y90","v":11.069999999999999},null,0.87]
[null,null,3,{"$f":"$D$89*C91","v":8.3024999999999984},{"$f":"$E$89*C91","v":0.51674999999999993},0,0,{"$f":"$H$89*C91","v":1.0125000000000002},0,0,0,0,0,0,{"$f":"$O$89*C91","v":7.1175000000000002E-2},0,{"$f":"$Q$89*C91","v":0.32474999999999998},0,null,"Scaling factor per 4 mm (A1-A3)",null,null,10.199999999999999]
[null,null,4,11.069999999999999,0.68899999999999995,0,0,1.35,0,0,0,0,0,0,9.4899999999999998E-2,0,0.433,0,null,"Scaling factor per 4 mm (A4)",null,null,0.68899999999999995]
[null,null,5,13.837499999999999,0.86124999999999996,0,0,1.6875,0,0,0,0,0,0,0.11862499999999999,0,0.54125000000000001,0,null,"Scaling factor per 4 mm (B2)",null,null,1.35]
[null,null,6,16.604999999999997,1.0334999999999999,0,0,2.0250000000000004,0,0,0,0,0,0,0.14235,0,0.64949999999999997,0,null,"Scaling factor per 4 mm (C2)",null,null,9.4899999999999998E-2]
[null,null,8,22.139999999999997,1.3779999999999999,0,0,2.7,0,0,0,0,0,0,0.1898,0,0.86599999999999999,0,null,"Scaling factor per 4 mm (C4)",null,null,0.433]
[null,null,10,27.674999999999997,1.7224999999999999,0,0,3.375,0,0,0,0,0,0,0.23724999999999999,0,1.0825,0]
[null,null,12,33.209999999999994,2.0669999999999997,0,0,4.0500000000000007,0,0,0,0,0,0,0.28470000000000001,0,1.2989999999999999,0]
[null,null,15,41.512499999999996,2.5837499999999998,0,0,5.0625,0,0,0,0,0,0,0.355875,0,1.62375,0]
[]
["Monolithic Ultraclear ",null,1,{"$f":"W100*W101","v":3.1},{"$f":"W100*W102","v":0.17224999999999999},0,0,{"$f":"W100*W103","v":0.33750000000000002},0,0,0,0,0,0,{"$f":"W100*W104","v":2.3725E-2},0,{"$f":"W100*W105","v":0.10825},0,null,"Glass impact per 1 mm",null,null,0.25]
[null,null,2,{"$f":"$D$100*C101","v":6.2},{"$f":"$E$100*C101","v":0.34449999999999997},0,0,{"$f":"$H$100*C101","v":0.67500000000000004},0,0,0,0,0,0,{"$f":"$O$100*C101","v":4.7449999999999999E-2},0,{"$f":"$Q$100*C101","v":0.2165},0,null,"Scaling factor per 4 mm (A1-A3)",null,null,12.4]
[null,null,3,{"$f":"$D$100*C102","v":9.3000000000000007},{"$f":"$E$100*C102","v":0.51674999999999993},0,0,{"$f":"$H$100*C102","v":1.0125000000000002},0,0,0,0,0,0,{"$f":"$O$100*C102","v":7.1175000000000002E-2},0,{"$f":"$Q$100*C102","v":0.32474999999999998},0,null,"Scaling factor per 4 mm (A4)",null,null,0.68899999999999995]
[null,null,4,12.4,0.68899999999999995,0,0,1.35,0,0,0,0,0,0,9.4899999999999998E-2,0,0.433,0,null,"Scaling factor per 4 mm (B2)",null,null,1.35]
[null,null,5,15.5,0.86124999999999996,0,0,1.6875,0,0,0,0,0,0,0.11862499999999999,0,0.54125000000000001,0,null,"Scaling factor per 4 mm (C2)",null,null,9.4899999999999998E-2]
[null,null,6,18.600000000000001,1.0334999999999999,0,0,2.0250000000000004,0,0,0,0,0,0,0.14235,0,0.64949999999999997,0,null,"Scaling factor per 4 mm (C4)",null,null,0.433]
[null,null,8,24.8,1.3779999999999999,0,0,2.7,0,0,0,0,0,0,0.1898,0,0.86599999999999999,0]
[null,null,10,31,1.7224999999999999,0,0,3.375,0,0,0,0,0,0,0.23724999999999999,0,1.0825,0]
[null,null,12,37.200000000000003,2.0669999999999997,0,0,4.0500000000000007,0,0,0,0,0,0,0.28470000000000001,0,1.2989999999999999,0]
[null,null,15,46.5,2.5837499999999998,0,0,5.0625,0,0,0,0,0,0,0.355875,0,1.62375,0]
[]
["Laminated",null,1,{"$f":"W111*W113","v":2.5249999999999999},{"$f":"W112*W121","v":0.17874999999999999},0,0,{"$f":"W112*W122","v":0.35125000000000001},0,0,0,0,0,0,{"$f":"W112*W123","v":2.4625000000000001E-2},0,{"$f":"W112*W124","v":0.112625},0,null,"Glass impact per 1 mm",null,null,0.25]
[null,"6.4 (33.1)",6,{"$f":"($D$111*C112)+($W$117*W114)+$Z$112","v":17.678000000000001},{"$f":"$E$111*C112","v":1.0725},0,0,{"$f":"$H$63*C113","v":2.1074999999999999},0,0,0,0,0,0,{"$f":"$O$63*C113","v":0.14774999999999999},0,{"$f":"$Q$111*C112","v":0.67575000000000007},0,null,null,null,null,0.125,null,null,0.72799999999999998]
[null,"6.8 (33.2)",6,{"$f":"($D$111*C113)+($W$117*W115)+$Z$112","v":19.478000000000002},{"$f":"$E$111*C113","v":1.0725},0,0,{"$f":"$H$63*C114","v":2.81},0,0,0,0,0,0,{"$f":"$O$63*C114","v":0.19700000000000001},0,{"$f":"$Q$111*C113","v":0.67575000000000007},0,null,"Scaling factor per 4 mm (A1-A3)",null,null,10.1]
[null,"8.4 (44.1)",8,{"$f":"($D$111*C114)+($W$117*W114)+$Z$112","v":22.728000000000002},1.43,0,0,2.81,0,0,0,0,0,0,0.19700000000000001,0,0.90100000000000002,0,null,"Scaling factor - Interlayer 0.38 (1)",null,null,1]
[null,"8.8 (44.2)",8,{"$f":"($D$111*C115)+($W$117*W115)+$Z$112","v":24.528000000000002},1.43,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,0.90100000000000002,0,null,"Scaling factor - Interlayer 0.76 (2)",null,null,2]
[null,"10.4 (55.1)",10,{"$f":"($D$111*C116)+($W$117*W114)+$Z$112","v":27.778000000000002},1.7874999999999999,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,1.12625,0,null,"Scaling factor - Interlayer 1.52 (4)",null,null,4]
[null,"10.8 (55.2)",10,{"$f":"($D$111*C117)+($W$117*W115)+$Z$112","v":29.578000000000003},1.7874999999999999,0,0,3.5125000000000002,0,0,0,0,0,0,0.24625000000000002,0,1.12625,0,null,"Interlayer factor",null,null,1.8]
[null,"11.5 (55.4)",10,{"$f":"($D$111*C118)+($W$117*W116)+$Z$112","v":33.178000000000004},1.7874999999999999,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.12625,0]
[null,"12.4 (66.1)",12,{"$f":"($D$111*C119)+($W$117*W114)+$Z$112","v":32.827999999999996},2.145,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.3515000000000001,0]
[null,"12.8 (66.2)",12,{"$f":"($D$111*C120)+($W$117*W115)+$Z$112","v":34.628},2.145,0,0,4.2149999999999999,0,0,0,0,0,0,0.29549999999999998,0,1.3515000000000001,0]
[null,"13.5 (66.4)",12,{"$f":"($D$111*C121)+($W$117*W116)+$Z$112","v":38.228000000000002},2.145,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.3515000000000001,0,null,"Scaling factor per 44.2 mm (A4)",null,null,1.43]
[null,"16.4 (88.1)",16,{"$f":"($D$111*C122)+($W$117*W114)+$Z$112","v":42.927999999999997},2.86,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.802,0,null,"Scaling factor per 44.2 mm (B2)",null,null,2.81]
[null,"16.8 (88.2)",16,{"$f":"($D$111*C123)+($W$117*W115)+$Z$112","v":44.728000000000002},2.86,0,0,5.62,0,0,0,0,0,0,0.39400000000000002,0,1.802,0,null,"Scaling factor per 44.2 mm (C2)",null,null,0.19700000000000001]
[null,"17.5 (88.4)",16,{"$f":"($D$111*C124)+($W$117*W116)+$Z$112","v":48.328000000000003},2.86,0,0,0,0,0,0,0,0,0,0,0,1.802,0,null,"Scaling factor per 44.2 mm (C4)",null,null,0.90100000000000002]
[]
[]
[]
[]
["Sentry glass",null,1,3.8,0.215,0,0,3.7999999999999999E-2,0,0,0,0,0,0,8.3000000000000001E-3,0,4.1000000000000002E-2,0]
[null,"13.5 (66.4)",12,{"$f":"($D$129*C130)+($W$143*$W$137)","v":54.945599999999999},{"$f":"($E$129*C130)+($W$144*$W$138)","v":2.59606},0,0,{"$f":"($H$129*C130)+($W$145*$W$139)","v":0.45600226999999999},0,0,0,0,0,0,{"$f":"($O$129*C130)+($W$146*$W$140)","v":0.10053959999999999},0,{"$f":"($Q$129*C130)+($W$147*$W$141)","v":0.49386249999999998},0]
[null,"17.5 (88.4)",16,{"$f":"($D$129*C131)+($W$143*$W$137)","v":70.145600000000002},{"$f":"($E$129*C131)+($W$144*$W$138)","v":3.4560599999999999},0,0,{"$f":"($H$129*C131)+($W$145*$W$139)","v":0.60800226999999996},0,0,0,0,0,0,{"$f":"($O$129*C131)+($W$146*$W$140)","v":0.13373960000000001},0,{"$f":"($Q$129*C131)+($W$147*$W$141)","v":0.65786250000000002},0]
[null,"21.5 (1010.4)",20,{"$f":"($D$129*C132)+($W$143*$W$137)","v":85.345600000000005},4.3160600000000002,0,0,0.76000226999999998,0,0,0,0,0,0,0.16693960000000002,0,0.82186250000000005,0]
[null,"25.5 (1212.4)",24,{"$f":"($D$129*C133)+($W$143*$W$137)","v":100.54559999999999},5.1760600000000005,0,0,0.91200226999999989,0,0,0,0,0,0,0.2001396,0,0.98586249999999997,0]
[null,"31.5 (1515.4)",30,{"$f":"($D$129*C134)+($W$143*$W$137)","v":123.3456},6.4660600000000006,0,0,1.1400022699999999,0,0,0,0,0,0,0.24993960000000001,0,1.2318625000000001,0]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Laminating process (A1-A3)",null,null,1.77]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Laminating process (A4)",null,null,7.2999999999999995E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Laminating process (C2)",null,null,1E-3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Laminating process (C4)",null,null,1.7999999999999999E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Laminating process (D)",null,null,2.5000000000000001E-2]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Interlayer factor 1.52 (A1-A3)",null,null,5.28]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Interlayer factor 1.52 (A4)",null,null,0.22]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Interlayer factor 1.52 (C2)",null,null,2.2699999999999999E-3]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Interlayer factor 1.52 (C4)",null,null,5.2200000000000003E-2]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Interlayer factor 1.52 (D)",null,null,7.4499999999999997E-2]

{"sheet":"Calculation Pilkington","index":6,"n_rows":122,"n_cols":21,"rows_kept":122,"cut":false,"hidden":true,"merged":[[20,0,24,0],[3,0,5,0],[6,0,8,0],[9,0,11,0],[12,0,14,0],[15,0,19,0]]}
[]
[null,null,"Thickness","A1-A3","A4","A5","B1","B2","B3","B4","B5","B6","B7","C1","C2","C3","C4","D"]
[]
["Mirai monolithic",null,4,{"$f":"1.35*C4","v":5.4},{"$f":"0.272*C4","v":1.0880000000000001},{"$f":"0.006*C4","v":2.4E-2},0,{"$f":"0.56*C4","v":2.2400000000000002},0,0,0,0,0,0,{"$f":"0.125*C4","v":0.5},0,{"$f":"0.139*C4","v":0.55600000000000005},0]
[null,null,6,{"$f":"1.35*C5","v":8.1000000000000014},{"$f":"0.272*C5","v":1.6320000000000001},{"$f":"0.006*C5","v":3.6000000000000004E-2},0,{"$f":"0.56*C5","v":3.3600000000000003},0,0,0,0,0,0,{"$f":"0.125*C5","v":0.75},0,{"$f":"0.139*C5","v":0.83400000000000007},0]
[null,null,8,10.8,2.1760000000000002,4.8000000000000001E-2,0,4.4800000000000004,0,0,0,0,0,0,1,0,1.1120000000000001,0]
["Monolithic offline coated ",null,4,{"$f":"D8/C8*C7","v":5.9266666666666667},{"$f":"E8/C8*C7","v":0.20533333333333334},{"$f":"F8/C8*C7","v":3.5999999999999997E-2},0,{"$f":"H8/C8*C7","v":0.10066666666666667},0,0,0,0,0,0,{"$f":"O8/C8*C7","v":0.152},0,0.16975000000000001,0]
[null,null,6,8.89,0.308,5.3999999999999999E-2,0,0.151,0,0,0,0,0,0,0.22800000000000001,0,0.29599999999999999,0]
[null,null,8,{"$f":"D8/C8*C9","v":11.853333333333333},{"$f":"E8/C8*C9","v":0.41066666666666668},{"$f":"F8/C8*C9","v":7.1999999999999995E-2},0,{"$f":"H8/C8*C9","v":0.20133333333333334},0,0,0,0,0,0,{"$f":"O8/C8*C9","v":0.30399999999999999},0,{"$f":"Q8/C8*C9","v":0.39466666666666667},0]
["Monolithic toughened",null,4,{"$f":"D11/C11*C10","v":8.7999999999999989},{"$f":"E11/C11*C10","v":0.20533333333333334},{"$f":"F11/C11*C10","v":3.5999999999999997E-2},0,{"$f":"H11/C11*C10","v":0.10066666666666667},0,0,0,0,0,0,{"$f":"O11/C11*C10","v":0.152},0,0.18665999999999999,0]
[null,null,6,13.2,0.308,5.3999999999999999E-2,0,0.151,0,0,0,0,0,0,0.22800000000000001,0,0.28000000000000003,0]
[null,null,8,{"$f":"D11/C11*C12","v":17.599999999999998},{"$f":"E11/C11*C12","v":0.41066666666666668},{"$f":"F11/C11*C12","v":7.1999999999999995E-2},0,{"$f":"H11/C11*C12","v":0.20133333333333334},0,0,0,0,0,0,{"$f":"O11/C11*C12","v":0.30399999999999999},0,{"$f":"Q11/C11*C12","v":0.37333333333333335},0]
["Monolithic toughened offline coated",null,4,{"$f":"D14/C14*C13","v":7.4666666666666659},{"$f":"E14/C14*C13","v":0.20533333333333334},{"$f":"F14/C14*C13","v":3.5999999999999997E-2},0,{"$f":"H14/C14*C13","v":0.10066666666666667},0,0,0,0,0,0,{"$f":"O14/C14*C13","v":0.152},0,{"$f":"Q14/C14*C13","v":0.19066666666666665},0]
[null,null,6,11.2,0.308,5.3999999999999999E-2,0,0.151,0,0,0,0,0,0,0.22800000000000001,0,0.28599999999999998,0]
[null,null,8,{"$f":"D14/C14*C15","v":14.933333333333332},{"$f":"E14/C14*C15","v":0.41066666666666668},{"$f":"F14/C14*C15","v":7.1999999999999995E-2},0,{"$f":"H14/C14*C15","v":0.20133333333333334},0,0,0,0,0,0,{"$f":"O14/C14*C15","v":0.30399999999999999},0,{"$f":"Q14/C14*C15","v":0.3813333333333333},0]
["Laminated 8.8",null,8.8000000000000007,{"$f":"D19/C19*C16","v":19.9375},{"$f":"E19/C19*C16","v":0.4345},{"$f":"F19/C19*C16","v":3.7124999999999998E-2},0,{"$f":"H19/C19*C16","v":3.7124999999999998E-2},0,0,0,0,0,0,{"$f":"O19/C19*C16","v":0.32381249999999995},0,{"$f":"Q19/C19*C16","v":0.49156250000000001},0]
[null,null,10.8,{"$f":"D19/C19*C17","v":24.46875},{"$f":"E19/C19*C17","v":0.53325},{"$f":"F19/C19*C17","v":4.5562499999999999E-2},0,{"$f":"H19/C19*C17","v":4.5562499999999999E-2},0,0,0,0,0,0,{"$f":"O19/C19*C17","v":0.39740624999999996},0,{"$f":"Q19/C19*C17","v":0.60328124999999999},0]
[null,null,11.5,{"$f":"D19/C19*C18","v":26.0546875},{"$f":"E19/C19*C18","v":0.56781249999999994},{"$f":"F19/C19*C18","v":4.8515624999999993E-2},0,{"$f":"H19/C19*C18","v":4.8515624999999993E-2},0,0,0,0,0,0,{"$f":"O19/C19*C18","v":0.42316406249999994},0,{"$f":"Q19/C19*C18","v":0.64238281249999996},0]
[null,null,12.8,29,0.63200000000000001,5.3999999999999999E-2,0,5.3999999999999999E-2,0,0,0,0,0,0,0.47099999999999997,0,{"$f":"0.715","v":0.71499999999999997},0]
[null,null,13.5,{"$f":"D19/C19*C20","v":30.5859375},{"$f":"E19/C19*C20","v":0.66656249999999995},{"$f":"F19/C19*C20","v":5.6953124999999993E-2},0,{"$f":"H19/C19*C20","v":5.6953124999999993E-2},0,0,0,0,0,0,{"$f":"O19/C19*C20","v":0.4967578124999999},0,{"$f":"Q19/C19*C20","v":0.75410156249999993},0]
["Laminated offline coated",null,8.8000000000000007,{"$f":"D24/C24*C21","v":20.556249999999999},{"$f":"E24/C24*C21","v":0.4345},{"$f":"F24/C24*C21","v":3.7124999999999998E-2},0,{"$f":"H24/C24*C21","v":3.7124999999999998E-2},0,0,0,0,0,0,{"$f":"O24/C24*C21","v":0.32381249999999995},0,{"$f":"Q24/C24*C21","v":0.495},0]
[null,null,10.8,{"$f":"D24/C24*C22","v":25.228124999999999},{"$f":"E24/C24*C22","v":0.53325},{"$f":"F24/C24*C22","v":4.5562499999999999E-2},0,{"$f":"H24/C24*C22","v":4.5562499999999999E-2},0,0,0,0,0,0,{"$f":"O24/C24*C22","v":0.39740624999999996},0,{"$f":"Q24/C24*C22","v":0.60749999999999993},0]
[null,null,11.5,{"$f":"D24/C24*C23","v":26.863281249999996},{"$f":"E24/C24*C23","v":0.56781249999999994},{"$f":"F24/C24*C23","v":4.8515624999999993E-2},0,{"$f":"H24/C24*C23","v":4.8515624999999993E-2},0,0,0,0,0,0,{"$f":"O24/C24*C23","v":0.42316406249999994},0,{"$f":"Q24/C24*C23","v":0.64687499999999998},0]
[null,null,12.8,29.9,0.63200000000000001,5.3999999999999999E-2,0,5.3999999999999999E-2,0,0,0,0,0,0,0.47099999999999997,0,0.72,0]
[null,null,13.5,{"$f":"D24/C24*C25","v":31.535156249999993},{"$f":"E24/C24*C25","v":0.66656249999999995},{"$f":"F24/C24*C25","v":5.6953124999999993E-2},0,{"$f":"H24/C24*C25","v":5.6953124999999993E-2},0,0,0,0,0,0,{"$f":"O24/C24*C25","v":0.4967578124999999},0,{"$f":"Q24/C24*C25","v":0.75937499999999991},0]
["Monolithic 2 mm",null,2]
["Monolithic 3 mm",null,3]
["Monolithic 4 mm",null,4]
["Monolithic 5 mm",null,5]
["Monolithic 6 mm",null,6]
["Monolithic 8 mm",null,8]
["Monolithic 10 mm",null,10]
["Monolithic 12 mm",null,12]
["Monolithic 15 mm",null,15]
["Monolithic offline coated 3 mm",null,3]
["Monolithic offline coated 4 mm",null,4,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,2.75]
["Monolithic offline coated 5 mm",null,5]
["Monolithic offline coated 6 mm",null,6]
["Monolithic offline coated 8 mm",null,8]
["Monolithic offline coated 10 mm",null,10]
["Monolithic offline coated 12 mm",null,12]
["Monolithic online coated 3 mm",null,3]
["Monolithic online coated 4 mm",null,4]
["Monolithic online coated 5 mm",null,5]
["Monolithic online coated 6 mm",null,6]
["Monolithic online coated 8 mm",null,8]
["Monolithic online coated 10 mm",null,10]
["Monolithic toughened 4 mm",null,4]
["Monolithic toughened 5 mm",null,5]
["Monolithic toughened 6 mm",null,6]
["Monolithic toughened 8 mm",null,8]
["Monolithic toughened 10 mm",null,10]
["Monolithic toughened 12 mm",null,12]
["Monolithic toughened 15 mm",null,15]
["Monolithic toughened offline coated 4 mm",null,4]
["Monolithic toughened offline coated 5 mm",null,5]
["Monolithic toughened offline coated 6 mm",null,6]
["Monolithic toughened offline coated 8 mm",null,8]
["Monolithic toughened offline coated 10 mm",null,10]
["Monolithic toughened offline coated 12 mm",null,12]
["Monolithic toughened online coated 4 mm",null,4]
["Monolithic toughened online coated 5 mm",null,5]
["Monolithic toughened online coated 6 mm",null,6]
["Monolithic toughened online coated 8 mm",null,8]
["Monolithic toughened online coated 10 mm",null,10]
["Monolithic toughened online coated 12 mm",null,12]
["Laminated 8.8 (44.2)",null,8.8000000000000007]
["Laminated 10.8 (55.2)",null,10.8]
["Laminated 11.5 (55.4)",null,11.5]
["Laminated 12.8 (66.2)",null,12.8]
["Laminated 13.5 (66.4)",null,13.5]
["Laminated offline coated 8.8 (44.2)",null,8.8000000000000007]
["Laminated offline coated 10.8 (55.2)",null,10.8]
["Laminated offline coated 11.5 (55.4)",null,11.5]
["Laminated offline coated 12.8 (66.2)",null,12.8]
["Laminated offline coated 13.5 (66.4)",null,13.5]
["Laminated online coated 8.8 (44.2)",null,8.8000000000000007]
["Laminated online coated 10.8 (55.2)",null,10.8]
["Laminated online coated 11.5 (55.4)",null,11.5]
["Laminated online coated 12.8 (66.2)",null,12.8]
["Laminated online coated 13.5 (66.4)",null,13.5]
["Laminated toughened 8.8 (44.2)",null,8.8000000000000007]
["Laminated 10.8 (55.2)",null,10.8]
["Laminated 11.5 (55.4)",null,11.5]
["Laminated 12.8 (66.2)",null,12.8]
["Laminated 13.5 (66.4)",null,13.5]
["Laminated 17.5 (88.4)",null,17.5]
["Laminated 21.5 (1010.4)",null,21.5]
["Monolithic 2 mm (Low Iron)",null,2]
["Monolithic 3 mm (Low Iron)",null,3]
["Monolithic 4 mm (Low Iron)",null,4]
["Monolithic 5 mm (Low Iron)",null,5]
["Monolithic 6 mm (Low Iron)",null,6]
["Monolithic 8 mm (Low Iron)",null,8]
["Monolithic 10 mm (Low Iron)",null,10]
["Monolithic 12 mm (Low Iron)",null,12]
["Monolithic 15 mm (Low Iron)",null,15]
["Monolithic offline coated 3 mm (Low Iron)",null,3]
["Monolithic offline coated 4 mm (Low Iron)",null,4]
["Monolithic offline coated 5 mm (Low Iron)",null,5]
["Monolithic offline coated 6 mm (Low Iron)",null,6]
["Monolithic offline coated 8 mm (Low Iron)",null,8]
["Monolithic offline coated 10 mm (Low Iron)",null,10]
["Monolithic offline coated 12 mm (Low Iron)",null,12]
["Monolithic toughened 4 mm (Low Iron)",null,4]
["Monolithic toughened 5 mm (Low Iron)",null,5]
["Monolithic toughened 6 mm (Low Iron)",null,6]
["Monolithic toughened 8 mm (Low Iron)",null,8]
["Monolithic toughened 10 mm (Low Iron)",null,10]
["Monolithic toughened 12 mm (Low Iron)",null,12]
["Monolithic toughened 15 mm (Low Iron)",null,15]
["Monolithic toughened offline coated 4 mm (Low Iron)",null,4]
["Monolithic toughened offline coated 5 mm (Low Iron)",null,5]
["Monolithic toughened offline coated 6 mm (Low Iron)",null,6]
["Monolithic toughened offline coated 8 mm (Low Iron)",null,8]
["Monolithic toughened offline coated 10 mm (Low Iron)",null,10]
["Monolithic toughened offline coated 12 mm (Low Iron)",null,12]
["Monolithic 4 mm",null,4]
["Monolithic 5 mm",null,5]
["Monolithic 6 mm",null,6]
["Monolithic 8 mm",null,8]
["Monolithic 10 mm",null,10]